{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["公共工程碳排放係數資料(113年)"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"公共工程碳排放係數資料(113年)","index":0,"n_rows":1104,"n_cols":19,"rows_kept":1104,"merged":[[0,0,0,9],[0,17,0,18]]}
["公共工程產品碳排放係數資料(113年)"]
[" ","項目","碳排放量(kgCO2)","宣告單位","碳排放係數(kgCO2e/宣告單位)","生命週期範疇","數據來源","查驗單位","公告年分","提報單位","工程編碼","1~5碼","6碼","7碼","8碼","9碼","10碼","環境部意見","提報單位修正結果"]
[1,"機械拆除，無筋混凝土，未含運費","0222010423","m3",13.641,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署","0222010423","02220",1,0,4,2,3]
[2,"清除及掘除","0223100003","m3",1.325,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署","0222010423","02220",1,0,4,2,3]
[3,"臨時擋土樁設施，打拔(不分類)","0225500031","m",0.483,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署","0222010423","02220",1,0,4,2,3]
[4,"臨時擋土樁設施，鋼軌樁，打拔","0225530031","m",0.483,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[5,"臨時擋土樁設施，鋼板樁，L=13m，打拔","0225540D31","m",{"v":14.5,"d":"14.500"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[6,"臨時擋土樁設施，鋼板樁，L=13m，打拔","0225540D3C","片",{"v":5.8,"d":"5.800"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[7,"臨時擋土支撐工法，H型鋼橫擋及支撐，裝拆","02256200B2","m2",39.637,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[8,"土方工作(不分類)","0230000003","m3",{"v":1.6715,"d":"1.672"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[9,"土方工作，挖方","02300C0003","m3",0.981,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[10,"土方工作，填方","02300D0003","m3",1.339,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[11,"土方工作，回填方","02300F0003","m3",0.736,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[12,"土方工作，近運填方","02300G0003","m3",1.201,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[13,"土方工作，遠運填方","02300H0003","m3",4.791,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[14,"土方工作，挖填方","02300E0003","m3",0.981,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[15,"土方工作，遠運利用","02300N0003","m3",3.908,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[16,"構造物開挖，機械挖","0231600703","m3",1.325,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[17,"構造物回填(不分類)","0231700003","m3",{"v":10.2295,"d":"10.230"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[18,"選擇材料回填(不分類)","0231900003","m3",{"v":10.2295,"d":"10.230"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[19,"選擇材料回填，透水材料，砂","0231911003","m3",8.213,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[20,"選擇材料回填，透水材料，礫石","0231912003","m3",10.961,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[21,"選擇材料回填，透水材料，碎石","0231913003","m3",13.241,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[22,"選擇材料回填，透水材料，塊石","0231919003","m3",14.106,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[23,"選擇材料回填，級配粒料，碎石級配","0231921003","m3",7.428,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[24,"選擇材料回填，級配粒料，天然級配","0231922003","m3",7.428,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[25,"棄土，餘方近運利用","0232310003","m3",1.042,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[26,"浚挖(不分類)","0232500003","m3",0.981,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[27,"地工織物，織布，合成纖維","0234221002","m2",2.479,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[28,"蛇籠，橢圓60cm*100cm，甲種","0237320101","m",26.176,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[29,"石籠(不分類)","0237400001","m",{"v":45.92,"d":"45.920"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[30,"土石籠(不分類)","0237400001","m",{"v":64.7675,"d":"64.768"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[31,"土石籠(不分類)","0237400003","m3",{"v":64.7675,"d":"64.768"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[32,"石籠(不分類)","0237400003","m3",{"v":45.92,"d":"45.920"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[33,"土石籠(不分類)","0237400008","組",{"v":64.7675,"d":"64.768"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[34,"石籠(不分類)","0237400008","組",{"v":45.92,"d":"45.920"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[35,"石籠，1m × 1m × 1m","0237430003","m3",19.355,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[36,"土石籠，1m × 1m × 1m","0237430003","m3",26.894,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[37,"石籠，1m × 1m × 1m","0237430008","組",19.355,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[38,"土石籠，1m × 1m × 1m","0237430008","組",26.894,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[39,"石籠，1m × 1m × 2m","0237480001","m",37.065,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[40,"石籠，1m × 1m × 2m","0237480008","組",37.065,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[41,"土石籠，1m × 1m × 2m","0237480008","組",52.143,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[42,"土石籠，1m × 1m × 2m","0237480003","m",52.143,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[43,"石籠，1m × 1m × 3m","0237490001","m",54.775,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[44,"石籠，1m × 1m × 3m","0237490008","組",54.775,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[45,"土石籠，1m × 1m × 3m","0237490008","組",77.392,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[46,"土石籠，1m × 1m × 3m","0237490003","m",77.392,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[47,"石籠，1m × 1m × 4m","02374A0001","m",72.485,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[48,"石籠，1m × 1m × 4m","02374A0008","組",72.485,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[49,"土石籠，1m × 1m × 4m","02374A0008","組",102.641,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[50,"土石籠，1m × 1m × 4m","02374A0003","m",102.641,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[51,"邊坡穩定水平排水管，塑膠管(不分類)","0237700001","m",{"v":11.3104,"d":"11.310"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[52,"邊坡穩定水平排水管，塑膠管，D=50mm(t=4.1mm)","0237700201","m",2.693,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[53,"邊坡穩定水平排水管，塑膠管，D=75mm(t=5.5mm)","0237700501","m",5.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[54,"邊坡穩定水平排水管，塑膠管，D=100mm(t=6.6mm)","0237700701","m",8.182,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[55,"邊坡穩定水平排水管，塑膠管，D=150mm(t=8.9mm)","0237700C01","m",16.082,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[56,"邊坡穩定水平排水管，塑膠管，D=200mm(t=10.3mm)","0237700H01","m",{"v":24.31,"d":"24.310"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[57,"拋石","0238100003","m3",5.352,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[58,"混凝土塊(不分類)","023840000A","塊",{"v":926.6544,"d":"926.654"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[59,"混凝土塊，重2t，含製作及吊放","023844010A","塊",202.712,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[60,"混凝土塊，重5t，含製作及吊放","023847010A","塊",463.452,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[61,"混凝土塊，重10t，含製作及吊放","02384B010A","塊",883.717,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[62,"混凝土塊，重15t，含製作及吊放","02384D010A","塊",1348.259,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[63,"混凝土塊，重20t，製作","02384E020A","塊",1735.132,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[64,"混凝土塊，重20t，吊放","02384E050A","塊",29.378,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[65,"坡面工(不分類)","0238500002","m2",49.415,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[66,"坡面工，混凝土，厚20cm","0238510302","m2",39.708,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[67,"坡面工，混凝土，厚30cm","0238510502","m2",59.122,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[68,"砌排石工(不分類)","0238600002","m2",{"v":18.7972,"d":"18.797"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[69,"砌排石工，鋪塊石，(厚25cm，未含勾縫)","0238621202","m2",0.975,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[70,"砌排石工，乾砌塊石，(厚25cm，未含勾縫)","0238631202","m2",1.221,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[71,"砌排石工，混凝土砌塊石，(厚25cm，未含勾縫)","0238641502","m2",16.427,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[72,"砌排石工，混凝土排塊石，(厚25cm，未含勾縫)","0238651502","m2",22.994,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[73,"砌排石工，混凝土襯排塊石，(厚25cm，未含勾縫)","0238661502","m2",52.369,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[74,"預力混凝土基樁(不分類，B種)","0245700001","m",{"v":79.5805,"d":"79.581"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[75,"預力混凝土基樁，D=300mm，B種","0245712001","m",35.604,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[76,"預力混凝土基樁，D=500mm，B種","0245752001","m",66.232,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[77,"預力混凝土基樁，D=600mm，B種","0245762001","m",85.168,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[78,"預力混凝土基樁，D=800mm，B種","0245782001","m",131.318,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[79,"預力混凝土基樁，D=800mm，B種，L=12m","0245782C0A","支",1626.521,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[80,"鑽掘樁(不分類)","0246500001","m",0.483,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[81,"微型樁(不分類，D=30cm)","0247250008","組",{"v":883.429333333333,"d":"883.429"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[82,"微型樁，D=30cm，L=4.5m","0247253008","組",680.958,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[83,"微型樁，D=30cm，L=6m","0247254008","組",863.182,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[84,"微型樁，D=30cm，L=8m","0247255008","組",1106.148,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[85,"自來水用塑膠管，聚氯乙烯塑膠管(不分類)","0251110001","m",{"v":11.3104,"d":"11.310"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[86,"自來水用塑膠管，聚氯乙烯塑膠管，D=50mm(t=4.1mm)","0251114001","m",2.693,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[87,"自來水用塑膠管，聚氯乙烯塑膠管，D=75mm(t=5.5mm)","0251117001","m",5.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[88,"自來水用塑膠管，聚氯乙烯塑膠管，D=100mm(t=6.6mm)","025111A001","m",8.182,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[89,"自來水用塑膠管，聚氯乙烯塑膠管，D=150mm(t=8.9mm)","025111E001","m",16.082,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[90,"自來水用塑膠管，聚氯乙烯塑膠管，D=200mm(t=10.3mm)","025111H001","m",{"v":24.31,"d":"24.310"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[91,"自來水用塑膠管，高密度聚乙烯管，D=200mm(t=11.9mm)","025115H001","m",{"v":17.28,"d":"17.280"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[92,"污水管管材，鋼筋混凝土管 (不分類)","0253310001","m",{"v":205.49,"d":"205.490"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[93,"污水管管材，鋼筋混凝土管(不分類，L=2.4m) ","025331000A","支",493.176,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[94,"污水管管材，鋼筋混凝土 管，D=600mm","0253319001","m",151.338,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[95,"污水管管材，鋼筋混凝土 管，D=600mm(L=2.4m)","025331900A","支",363.212,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[96,"污水管管材，鋼筋混凝土 管，D=800mm","025331B001","m",205.708,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[97,"污水管管材，鋼筋混凝土 管，D=800mm(L=2.4m)","025331B00A","支",{"v":493.7,"d":"493.700"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[98,"污水管管材，鋼筋混凝土 管，D=1000mm","025331D001","m",259.424,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[99,"污水管管材，鋼筋混凝土 管，D=1000mm(L=2.4m)","025331D00A","支",622.617,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[100,"污水管管材，聚氯乙烯塑膠硬質管，D=200mm(t=10.3mm) ","0253391201","m",{"v":24.31,"d":"24.310"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[101,"排水管溝，塑膠管(不分類) ","0260100001","m",{"v":11.31,"d":"11.310"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[102,"排水管溝，塑膠管，D=100mm(t=6.6mm) ","02601B1001","m",8.182,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[103,"排水管溝，塑膠管，D=150mm(t=8.9mm) ","02601B3001","m",16.082,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[104,"排水管溝，塑膠管，D=200mm(t=10.3mm) ","02601B4001","m",{"v":24.31,"d":"24.310"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[105,"管涵，鋼筋混凝土管 B 型(不分類)","0260220001","m",{"v":205.49,"d":"205.490"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[106,"管涵，鋼筋混凝土管 B 型(不分類，L=2.4m) ","0260220007","個",493.176,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[107,"管涵，鋼筋混凝土管 B 型，D=600mm ","0260229001","m",151.338,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[108,"管涵，鋼筋混凝土管 B 型，D=600mm(L=2.4m) ","0260229007","個",363.212,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[109,"管涵，鋼筋混凝土管 B 型，D=800mm","026022B001","m",205.708,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[110,"管涵，鋼筋混凝土管 B 型，D=800mm(L=2.4m)","026022B007","個",{"v":493.7,"d":"493.700"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[111,"管涵，鋼筋混凝土管 B 型，D=1000mm","026022D001","m",259.424,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[112,"管涵，鋼筋混凝土管B型，D=1000mm(L=2.4m)","026022D007","個",622.617,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[113,"排水管涵，鋼筋混凝土管(不分類)","0261020001","m",{"v":205.49,"d":"205.490"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[114,"排水管涵，鋼筋混凝土管(不分類)","0261020001","m",{"v":205.49,"d":"205.490"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[115,"排水管涵，鋼筋混凝土管(不分類，L=2.4m)","026102D00A","支",{"v":493.176333333333,"d":"493.176"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[116,"排水管涵，鋼筋混凝土管(B型)，D=600mm","026102D001","m",151.338,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[117,"排水管涵，鋼筋混凝土管(B型)，D=600mm(L=2.4m)","026102D00A","支",363.212,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[118,"排水管涵，鋼筋混凝土管(B型)，D=800mm","026102F001","m",205.708,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[119,"排水管涵，鋼筋混凝土管(B型)，D=800mm(L=2.4m)","026102F00A","支",{"v":493.7,"d":"493.700"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[120,"排水管涵，鋼筋混凝土管(B型)，D=1000mm","026102H001","m",259.424,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[121,"排水管涵，鋼筋混凝土管(B型)，D=1000mm(L=2.4m)","026102H00A","支",622.617,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[122,"排水管涵，聚氯乙烯排水管，D=50mm(t=4.1mm)","0261081001","m",2.693,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[123,"排水管涵，聚氯乙烯排水管，D=75mm(t=5.5mm)","0261082001","m",5.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[124,"排水管涵，聚氯乙烯排水管，D=100mm(t=6.6mm)","0261083001","m",8.182,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[125,"排水管涵，聚氯乙烯排水管，D=150mm(t=8.9mm)","0261085001","m",16.082,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[126,"排水管涵，聚氯乙烯排水管，D=200mm(t=10.3mm)","0261086001","m",{"v":24.31,"d":"24.310"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[127,"級配粒料基層，碎石級配，鋪設及滾壓","02722100A3","m3",{"v":5.74,"d":"5.740"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[128,"級配粒料底層，碎石級配，鋪設及滾壓","0272610053","m3",{"v":5.74,"d":"5.740"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[129,"瀝青混凝土鋪面(不分類)","0274200002","m2",13.465,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[130,"瀝青混凝土鋪面，厚5cm","027420D002","m2",{"v":8.13,"d":"8.130"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[131,"瀝青混凝土鋪面，厚8cm","027420G002","m2",16.704,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[132,"瀝青混凝土鋪面，厚10cm","027420J002","m2",21.133,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[133,"多孔隙瀝青混凝土鋪面，厚5cm","027428D002","m2",7.893,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[134,"瀝青透層(不分類)","0274500002","m2",2E-3,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[135,"瀝青黏層(不分類)","0274700002","m2",2E-3,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[136,"舖單元磚(不分類)","0278000002","m2",33.739,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[137,"濕式壓花地坪","0278040002","m2",60.582,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[138,"乾式噴花地坪","0278040002","m2",6.896,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[139,"乾式壓花地坪","0278040002","m2",{"v":6.87,"d":"6.870"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[140,"植栽，客土","02900B0003","m3",{"v":0,"d":"0.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[141,"植樹，喬木(不分類)","0293100000","株",{"v":-250.8375,"d":"-250.838"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[142,"植樹，喬木，相思樹","0293111100","株",{"v":-381,"d":"-381.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[143,"植樹，喬木，樟樹","0293112400","株",{"v":-219,"d":"-219.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[144,"植樹，喬木，光臘樹","0293113100","株",{"v":-168,"d":"-168.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[145,"植樹，喬木，楓香","0293113B00","株",{"v":-222,"d":"-222.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[146,"植樹，灌木(不分類)","0293120000","株",-9.375,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[147,"灌木類植栽(不分類)","0293200000","株",-9.375,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[148,"喬木植栽(不分類)","0293800000","株",{"v":-250.8375,"d":"-250.838"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[149,"喬木植栽，台灣杉","029381B000","株",{"v":-381,"d":"-381.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[150,"喬木植栽，台灣肖楠","029381E000","株",{"v":-285.9,"d":"-285.900"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[151,"喬木植栽，烏心石","0293828000","株",{"v":-178.8,"d":"-178.800"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[152,"喬木植栽，相思樹","029384J000","株",{"v":-381,"d":"-381.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[153,"喬木植栽，楓香","029386J000","株",{"v":-222,"d":"-222.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[154,"喬木植栽，櫸木","0293886000","株",{"v":-171,"d":"-171.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[155,"道路施工及復舊(不分類)","0295200002","m2",8.182,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[156,"瀝青混凝土面層刨除(不分類，厚5cm)","0296100002","m2",2.094,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[157,"瀝青混凝土面層刨除，厚5cm，刨除機2.2m寬","0296140402","m2",2.094,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[158,"瀝青混凝土面層刨除，刨除料運費","0296103003","m3",17.032,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[159,"再生瀝青混凝土，舖築及滾壓(不分類，含料)","0296600003","m3",85.209,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[160,"再生瀝青混凝土，舖築及滾壓(不分類，含料)","0296600005","t",36.259,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[161,"水泥混凝土構造物，場鑄混凝土(20%礦物摻料)(不分類)","0305400003","m3",{"v":361.089285714286,"d":"361.089"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[162,"水泥混凝土構造物，場鑄混凝土(50%礦物摻料)(不分類)","0305400003","m3",{"v":238.985571428571,"d":"238.986"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[163,"水泥混凝土構造物，場鑄混凝土140kgf/cm2(20%礦物摻料)","0305420003","m3",267.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[164,"水泥混凝土構造物，場鑄混凝土140kgf/cm2(50%礦物摻料)","0305420003","m3",{"v":195.05,"d":"195.050"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[165,"水泥混凝土構造物，場鑄混凝土175kgf/cm2(20%礦物摻料)","0305430003","m3",292.505,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[166,"水泥混凝土構造物，場鑄混凝土175kgf/cm2(50%礦物摻料)","0305430003","m3",{"v":204.43,"d":"204.430"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[167,"水泥混凝土構造物，場鑄混凝土210kgf/cm2(20%礦物摻料)","0305440003","m3",321.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[168,"水泥混凝土構造物，場鑄混凝土210kgf/cm2(50%礦物摻料)","0305440003","m3",{"v":209.02,"d":"209.020"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[169,"水泥混凝土構造物，場鑄混凝土245kgf/cm2(20%礦物摻料)","0305450003","m3",352.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[170,"水泥混凝土構造物，場鑄混凝土245kgf/cm2(50%礦物摻料)","0305450003","m3",{"v":231.1,"d":"231.100"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[171,"水泥混凝土構造物，場鑄混凝土280kgf/cm2(20%礦物摻料)","0305460003","m3",366.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[172,"水泥混凝土構造物，場鑄混凝土280kgf/cm2(50%礦物摻料)","0305460003","m3",252.995,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[173,"水泥混凝土構造物，場鑄混凝土350kgf/cm2(20%礦物摻料)","0305480003","m3",433.695,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[174,"水泥混凝土構造物，場鑄混凝土350kgf/cm2(50%礦物摻料)","0305480003","m3",275.865,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[175,"水泥混凝土構造物，場鑄混凝土420kgf/cm2(20%礦物摻料)","03054A0003","m3",494.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[176,"水泥混凝土構造物，場鑄混凝土420kgf/cm2(50%礦物摻料)","03054A0003","m3",304.439,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[177,"混凝土模板及附屬品，支撐施工架，鋼料，4.1≦支撐高度＜6.0m","0310022102","m2",{"v":0,"d":"0.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[178,"場鑄結構混凝土用模板(不分類)","0311000002","m2",{"v":1.2702,"d":"1.270"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[179,"場鑄結構混凝土用模板，普通模板，一般工程用","0311011002","m2",1.202,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[180,"場鑄結構混凝土用模板，普通模板，建築","0311011502","m2",1.202,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[181,"場鑄結構混凝土用模板，清水模板","0311020002","m2",1.204,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[182,"場鑄結構混凝土用模板，免拆模板，木質","0311060002","m2",0.852,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[183,"場鑄結構混凝土用模板，免拆模板，鋼質(t=0.3mm)","0311070002","m2",6.902,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[184,"場鑄結構混凝土用模板，鋼製模板","0311090002","m2",11.109,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[185,"場鑄結構混凝土用模板，造型模板","03110A0002","m2",1.891,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[186,"混凝土附屬品，填縫版、止水帶、伸縮縫","0315000002","m2",{"v":0,"d":"0.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[187,"混凝土附屬品，填縫版、止水帶、伸縮縫","0315000004","式",{"v":0,"d":"0.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[188,"混凝土附屬品，填縫版、止水帶、伸縮縫","0315000008","組",{"v":0,"d":"0.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[189,"混凝土附屬品，填縫版、止水帶、伸縮縫","031500000B","處",{"v":0,"d":"0.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[190,"鋼筋(不分類)","0321000005","t",{"v":893.09,"d":"893.090"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[191,"鋼筋(不分類)","0321000009","kg",{"v":0.89309,"d":"0.893"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[192,"鋼筋，SD280，連工帶料","0321030075","t",{"v":893.62,"d":"893.620"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[193,"鋼筋，SD280，連工帶料","0321030079","kg",{"v":0.89362,"d":"0.894"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[194,"鋼筋，SD280W，連工帶料","0321040075","t",{"v":893.62,"d":"893.620"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[195,"鋼筋，SD280W，連工帶料","0321040079","kg",{"v":0.89362,"d":"0.894"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[196,"鋼筋，SD420，連工帶料","0321050075","t",{"v":892.56,"d":"892.560"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[197,"鋼筋，SD420，連工帶料","0321050079","kg",{"v":0.89256,"d":"0.893"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[198,"鋼筋，SD420W，連工帶料","0321060075","t",{"v":892.56,"d":"892.560"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[199,"鋼筋，SD420W，連工帶料","0321060079","kg",{"v":0.89256,"d":"0.893"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[200,"鋼筋，植筋","032100E00B","孔",{"v":0,"d":"0.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[201,"銲接鋼線網，線徑10mm，方孔10x10cm","0322006142","m2",10.296,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[202,"銲接鋼線網，線徑10mm，方孔15x15cm","0322006162","m2",6.864,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[203,"銲接鋼線網，線徑10mm，方孔20x20cm","0322006182","m2",5.152,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[204,"銲接鋼線網(不分類，線徑10mm)","0322000002","m2","7.437","規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[205,"結構用混凝土(純水泥)(不分類)","0331000003","m3",425.187,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[206,"結構用混凝土(10%礦物摻料)(不分類)","0331000003","m3",{"v":387.628571428571,"d":"387.629"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[207,"結構用混凝土(20%礦物摻料)(不分類)","0331000003","m3",{"v":361.089285714286,"d":"361.089"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[208,"結構用混凝土(30%礦物摻料)(不分類)","0331000003","m3",{"v":300.681142857143,"d":"300.681"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[209,"結構用混凝土(40%礦物摻料)(不分類)","0331000003","m3",{"v":276.189571428571,"d":"276.190"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[210,"結構用混凝土(50%礦物摻料)(不分類)","0331000003","m3",{"v":238.985571428571,"d":"238.986"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[211,"結構用混凝土，預拌，140kgf/cm2","0331023003","m3",304.785,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[212,"結構用混凝土，預拌，140kgf/cm2(10%礦物摻料)","0331023003","m3",282.838,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[213,"結構用混凝土，預拌，140kgf/cm2(30%礦物摻料)","0331023003","m3",228.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[214,"結構用混凝土，預拌，140kgf/cm2(40%礦物摻料)","0331023003","m3",216.997,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[215,"結構用混凝土，預拌，140kgf/cm2(50%礦物摻料)","0331023003","m3",{"v":195.05,"d":"195.050"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[216,"結構用混凝土，預拌，140kgf/cm2(20%礦物摻料)","0331023003","m3",267.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[217,"結構用混凝土，預拌，175kgf/cm2","0331024003","m3",344.288,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[218,"結構用混凝土，預拌，175kgf/cm2(10%礦物摻料)","0331024003","m3",316.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[219,"結構用混凝土，預拌，175kgf/cm2(20%礦物摻料)","0331024003","m3",292.505,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[220,"結構用混凝土，預拌，175kgf/cm2(30%礦物摻料)","0331024003","m3",249.873,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[221,"結構用混凝土，預拌，175kgf/cm2(40%礦物摻料)","0331024003","m3",232.418,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[222,"結構用混凝土，預拌，175kgf/cm2(50%礦物摻料)","0331024003","m3",{"v":204.43,"d":"204.430"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[223,"結構用混凝土，預拌，210kgf/cm2","0331025003","m3",384.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[224,"結構用混凝土，預拌，210kgf/cm2(10%礦物摻料)","0331025003","m3",349.232,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[225,"結構用混凝土，預拌，210kgf/cm2(20%礦物摻料)","0331025003","m3",321.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[226,"結構用混凝土，預拌，210kgf/cm2(40%礦物摻料)","0331025003","m3",244.073,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[227,"結構用混凝土，預拌，210kgf/cm2(50%礦物摻料)","0331025003","m3",{"v":209.02,"d":"209.020"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[228,"結構用混凝土，預拌，210kgf/cm2(30%礦物摻料)","0331025003","m3",267.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[229,"結構用混凝土，預拌，245kgf/cm2","0331026003","m3",419.785,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[230,"結構用混凝土，預拌，245kgf/cm2(10%礦物摻料)","0331026003","m3",382.048,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[231,"結構用混凝土，預拌，245kgf/cm2(20%礦物摻料)","0331026003","m3",352.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[232,"結構用混凝土，預拌，245kgf/cm2(30%礦物摻料)","0331026003","m3",293.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[233,"結構用混凝土，預拌，245kgf/cm2(40%礦物摻料)","0331026003","m3",268.837,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[234,"結構用混凝土，預拌，245kgf/cm2(50%礦物摻料)","0331026003","m3",{"v":231.1,"d":"231.100"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[235,"結構用混凝土，預拌，280kgf/cm2","0331027003","m3",433.785,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[236,"結構用混凝土，預拌，280kgf/cm2(10%礦物摻料)","0331027003","m3",397.627,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[237,"結構用混凝土，預拌，280kgf/cm2(30%礦物摻料)","0331027003","m3",317.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[238,"結構用混凝土，預拌，280kgf/cm2(20%礦物摻料)","0331027003","m3",366.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[239,"結構用混凝土，預拌，280kgf/cm2(40%礦物摻料)","0331027003","m3",289.153,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[240,"結構用混凝土，預拌，280kgf/cm2(50%礦物摻料)","0331027003","m3",252.995,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[241,"結構用混凝土，預拌，350kgf/cm2","0331029003","m3",{"v":511.29,"d":"511.290"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[242,"結構用混凝土，預拌，350kgf/cm2(10%礦物摻料)","0331029003","m3",463.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[243,"結構用混凝土，預拌，350kgf/cm2(50%礦物摻料)","0331029003","m3",275.865,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[244,"結構用混凝土，預拌，350kgf/cm2(20%礦物摻料)","0331029003","m3",433.695,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[245,"結構用混凝土，預拌，350kgf/cm2(30%礦物摻料)","0331029003","m3",{"v":354.47,"d":"354.470"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[246,"結構用混凝土，預拌，350kgf/cm2(40%礦物摻料)","0331029003","m3",{"v":322.84,"d":"322.840"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[247,"結構用混凝土，預拌，420kgf/cm2","033102C003","m3",578.091,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[248,"結構用混凝土，預拌，420kgf/cm2(10%礦物摻料)","033102C003","m3",522.085,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[249,"結構用混凝土，預拌，420kgf/cm2(20%礦物摻料)","033102C003","m3",494.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[250,"結構用混凝土，預拌，420kgf/cm2(30%礦物摻料)","033102C003","m3",394.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[251,"結構用混凝土，預拌，420kgf/cm2(40%礦物摻料)","033102C003","m3",359.009,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[252,"結構用混凝土，預拌，420kgf/cm2(50%礦物摻料)","033102C003","m3",304.439,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[253,"控制性低強度回填材料(CLSm)","0337700013","m3",94.495,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[254,"預鑄混凝土，異形塊(不分類)","034000000A","塊",{"v":926.6544,"d":"926.654"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[255,"預鑄混凝土，異形塊，5t","03400C100A","塊",463.452,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[256,"預鑄混凝土，異形塊，10t","03400C200A","塊",883.717,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[257,"預鑄混凝土，異形塊，15t","03400C300A","塊",1348.259,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[258,"預鑄混凝土，異形塊，20t","03400C400A","塊",1735.132,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[259,"港灣用預鑄混凝土塊(不分類)","034390000A","塊",{"v":926.6544,"d":"926.654"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[260,"港灣用預鑄混凝土塊，重10t","03439B000A","塊",883.717,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[261,"港灣用預鑄混凝土塊，重20t","03439E000A","塊",1735.132,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[262,"港灣用預鑄混凝土塊，重2t","034394000A","塊",202.712,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[263,"港灣用預鑄混凝土塊，重5t","034397000A","塊",463.452,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[264,"港灣用預鑄混凝土塊，重15t","03439D000A","塊",1348.259,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[265,"水泥砂漿(不分類)","0406100003","m3",{"v":671.33,"d":"671.330"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[266,"水泥砂漿，1:1","0406110003","m3",{"v":952,"d":"952.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[267,"水泥砂漿，1:2","0406120003","m3",{"v":625,"d":"625.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[268,"水泥砂漿，1:3","0406130003","m3",{"v":437,"d":"437.000"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[269,"金屬材料(不分類，鋼)","0506000009","kg",{"v":2.42,"d":"2.420"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[270,"金屬製品，不銹鋼踏步(D=19mm實心)","05500f0001","m",3.895,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[271,"金屬製品，不銹鋼踏步(D=19mm實心)","05500f0007","個",{"v":3.35,"d":"3.350"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[272,"金屬製品，不銹鋼踏步(D=19mm實心)","05500f0R08","組",{"v":3.35,"d":"3.350"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[273,"金屬製品，不銹鋼踏步(D=19mm實心)","05500f000A","支",{"v":3.35,"d":"3.350"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[274,"金屬製品，不銹鋼踏步","05500f0R09","kg",{"v":1.75,"d":"1.750"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[275,"金屬製品，不鏽鋼踏步(不分類)","05500f0009","kg",{"v":1.75,"d":"1.750"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[276,"不銹鋼欄杆(D=50mm，t=3.5mm)","05523310H1","m",36.508,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[277,"金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座(不分類)","0553000008","組",{"v":255.7945,"d":"255.795"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[278,"金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=60cm(52.6kg)","05530BD008","組",157.274,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[279,"金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=70cm(70.1kg)","05530BE008","組",209.599,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[280,"金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=80cm(99.5kg)","05530BF008","組",297.505,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[281,"金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=90cm(120kg)","05530BG008","組",{"v":358.8,"d":"358.800"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[282,"不銹鋼水尺","057330D008","組",113.982,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[283,"材料，玻璃(不分類)","0881000009","kg",1.435,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[284,"材料，玻璃，普通平板玻璃","0881010009","kg",{"v":1.12,"d":"1.120"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[285,"材料，玻璃，強化玻璃","0881030009","kg",{"v":1.75,"d":"1.750"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[286,"水泥砂漿粉刷，1：3水泥砂漿，牆面，打底","0922030322","m2",{"v":8.74,"d":"8.740"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[287,"材料，再生纖維水泥板(不分類)","m0924000009","kg",{"v":1.12,"d":"1.120"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[288,"材料，再生纖維水泥板，纖維水泥板","m0924020009","kg",{"v":1.12,"d":"1.120"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[289,"材料，再生纖維水泥板，矽酸鈣板","m0924030009","kg",{"v":1.12,"d":"1.120"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[290,"材料，石膏板，石膏板","0925010009","kg",{"v":0.51,"d":"0.510"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[291,"洗石子","0978000002","m2",8.089,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[292,"抿石子","0978200002","m2",8.089,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[293,"材料，水泥漆，水性水泥漆","0991210009","kg",1.33,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[294,"聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)(不分類)",1510720001,"m",{"v":11.3104,"d":"11.310"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[295,"聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=50mm(t=4.1mm)","1510727001","m",2.693,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[296,"聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=75mm(t=5.5mm)","1510729001","m",5.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[297,"聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=100mm(t=6.6mm)","151072B001","m",8.182,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[298,"聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=150mm(t=8.9mm)","151072D001","m",16.082,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[299,"聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=200mm(t=10.3mm)","151072E001","m",{"v":24.31,"d":"24.310"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[300,"污水管路系統，聚氯乙烯管(B管厚管)，橘色管(不分類)","m151516100001","m",{"v":11.3104,"d":"11.310"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[301,"污水管路系統，聚氯乙烯管(B管厚管)，橘色管，D=50mm(t=4.1mm)","m151516170001","m",2.693,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[302,"污水管路系統，聚氯乙烯管(B管厚管)，橘色管，D=75mm(t=5.5mm)","m151516190001","m",5.285,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[303,"污水管路系統，聚氯乙烯管(B管厚管)，橘色管，D=100mm(t=6.6mm)","m1515161B0001","m",8.182,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[304,"污水管路系統，聚氯乙烯管(B管厚管)，橘色管，D=150mm(t=8.9mm)","m1515161D0001","m",16.082,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[305,"污水管路系統，聚氯乙烯管(B管厚管)，橘色管，D=200mm(t=10.3mm)","m1515161E0001","m",{"v":24.31,"d":"24.310"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"經濟部水利署"]
[306,"機械拆除，無鋼筋混凝土結構物，未含運送","0222010423","m3",10.387,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[307,"機械拆除，無筋混凝土，未含運費","0222010423","m3",13.641,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"農業部農村水保署"]
[308,"清除及掘除","0223100003","m3",1.009,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[309,"臨時擋土樁設施，打拔(不分類)","0225500031","m",0.483,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"農業部農村水保署"]
[310,"臨時擋土樁設施，鋼軌樁，打拔","0225530031","m",0.483,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"農業部農村水保署"]
[311,"臨時擋土樁設施，鋼板樁，L=13m，打拔","0225540D31","m",{"v":14.5,"d":"14.500"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"農業部農村水保署"]
[312,"臨時擋土樁設施，鋼板樁，L=13m，打拔","0225540D3C","片",{"v":5.8,"d":"5.800"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"農業部農村水保署"]
[313,"臨時擋土樁設施，鋼板樁，含施作","0225500001","m",11.045,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[314,"臨時擋土樁設施，鋼板樁(不分類)","022550000D","支",4.418,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[315,"臨時擋土樁設施，鋼軌樁 42kg/m，含施作","022552004D","支",{"v":5.26,"d":"5.260"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[316,"臨時擋土樁設施，鋼軌樁及鋼板，含引孔、打拔","0225520064","m",13.067,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[317,"臨時擋土樁設施，鋼軌樁 37kg/m，L=5m、間距=60cm(單邊水平長度，含擋土支撐系統)","0225525611","m",{"v":4.64,"d":"4.640"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[318,"臨時擋土樁設施，鋼軌樁 37kg/m，L=6m，含引孔、打拔","022552603D","支",{"v":27.84,"d":"27.840"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[319,"臨時擋土樁設施，鋼軌樁 50kg/m，L=4m，含引孔、打拔","022553313D","支",{"v":21.6,"d":"21.600"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[320,"臨時擋土樁設施，鋼軌樁 50kg/m，L=6m、間距=60cm(單\n邊水平長度，含擋土支撐系統) ","0225538621","m",{"v":32.4,"d":"32.400"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[321,"臨時擋土樁設施，鋼板樁，L=13m，打拔","0225540D3D","支",{"v":5.8,"d":"5.800"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"農業部農村水保署"]
[322,"臨時擋土支撐工法，H 型鋼橫擋及支撐，裝拆","02256200B2","m2",39.637,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[323,"臨時擋土支撐工法，木橫擋及支撐、H 型鋼橫擋及支撐，未含在臨時擋土樁內","0225610002","m2",39.637,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[324,"臨時擋土樁設施(≧49kg/m，L=6m)，含引孔、打拔 ","02256500C1","m",{"v":32.4,"d":"32.400"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[325,"土方工作(不分類)","0230000003","m3",1.553,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[326,"土方工作(不分類)","0230000003","m3",{"v":1.6715,"d":"1.672"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[327,"土方工作，挖方","02300C0003","m3",{"v":2.51,"d":"2.510"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[328,"土方工作，填方","02300D0003","m3",1.339,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"農業部農村水保署"]
[329,"土方工作，回填方","02300F0003","m3",0.736,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"農業部農村水保署"]
[330,"土方工作，近運填方","02300G0003","m3",1.201,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"農業部農村水保署"]
[331,"土方工作，遠運填方","02300H0003","m3",4.791,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"農業部農村水保署"]
[332,"土方工作，遠運利用","0230010003","m3",3.064,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[333,"土方工作，填方和回填方","02300DF0003","m3",{"v":2.78,"d":"2.780"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[334,"構造物開挖，機械挖掘","0231600703","m3",1.325,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"農業部農村水保署"]
[335,"構造物開挖，軟弱地質，機械挖","0231610703","m3",{"v":2.78,"d":"2.780"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[336,"構造物開挖，砂土礫石，機械挖","0231620003","m3",{"v":2.51,"d":"2.510"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[337,"構造物開挖，卵石(挖普通土含 30%以上砂礫)，機械挖","0231630703","m3",{"v":2.51,"d":"2.510"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[338,"構造物開挖，軟岩，機械挖","0231640703","m3",{"v":2.78,"d":"2.780"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[339,"構造物開挖，硬岩，機械挖","0231650003","m3",{"v":5.88,"d":"5.880"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[340,"構造物回填(不分類)","0231700003","m3",8.591,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[341,"構造物回填，原材料回填，機械","0231710003","m3",8.591,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[342,"構造物回填，回填及夯實(實際)","0231740003","m3",8.591,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[343,"工區內土方調整","0231730003","m3",{"v":1.42,"d":"1.420"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[344,"工區內土方整理，機械","02317K0103","m3",{"v":0.75,"d":"0.750"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[345,"選擇材料回填(不分類)","0231900003","m3",{"v":10.23,"d":"10.230"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"農業部農村水保署"]
[346,"選擇性回填材料，透水材料，砂","0231911003","m3",6.996,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[347,"選擇性回填材料，透水材料，礫石","0231912003","m3",9.088,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[348,"選擇性回填材料，透水材料，碎石","0231913003","m3",10.994,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[349,"選擇性回填材料，透水材料，塊石","0231919003","m3",11.672,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[350,"選擇性回填材料，級配粒料，碎石級配","0231921003","m3",6.398,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[351,"選擇性回填材料，級配粒料，天然級配","0231922003","m3",6.398,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[352,"選擇性回填材料，級配粒料","0231920003","m3",{"v":63.98,"d":"63.980"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[353,"棄土，餘方近運利用","0232310003","m3",1.042,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[354,"餘土處理(現場攤平)","0232300003","m3",0.713,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[355,"棄土區費用(含水土保持)，0≦運距＜5km，近運利用","02323AX003","m3",{"v":1.43,"d":"1.430"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[356,"廢方處理","02323C00031","m3",{"v":25.69,"d":"25.690"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[357,"浚挖(不分類)","0232500003","m3",0.981,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[358,"地工織物，透水性織布、不織布、合成纖維","0234220002","m2",{"v":3,"d":"3.000"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[359,"蛇籠，橢圓 60cm*100cm，甲種(機編蛇籠網材另計)","0237320101","m",26.176,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[360,"蛇籠，橢圓 40cm*67cm(機編蛇籠網材另計)","0237320001","m",8.824,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[361,"石籠(不分類)","0237400001","m",{"v":45.92,"d":"45.920"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[362,"土石籠(不分類)","0237400001","m",64.768,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[363,"石籠(不分類)","0237400003","m3",{"v":45.92,"d":"45.920"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[364,"土石籠(不分類)","0237400003","m3",64.768,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[365,"石籠(不分類)","0237400008","組",{"v":45.92,"d":"45.920"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[366,"土石籠(不分類)","0237400008","組",64.768,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[367,"土石籠，1m × 1m × 1m","0237430003","m",26.894,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[368,"石籠，1m × 1m × 2m","0237480001","m",37.065,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[369,"土石籠，1m × 1m × 2m","0237480003","m",52.143,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[370,"石籠，1m × 1m × 3m","0237490001","m",54.775,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[371,"土石籠，1m × 1m × 3m","0237490003","m",77.392,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[372,"石籠，1m × 1m × 4m","02374A0001","m",72.485,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[373,"土石籠，1m × 1m × 4m","02374A0003","m",102.641,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[374,"石籠，鍍鋅鋼線箱形石籠網材","0237400002","m2",{"v":1.3,"d":"1.300"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[375,"石籠，石塊現採","0237400013","m3",{"v":10.75,"d":"10.750"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[376,"石籠，1m × 1m × 1m","0237430001","m",19.355,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[377,"石籠，1m × 1m × 0.5m","0237430002","m",7.768,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[378,"石籠，箱型石籠內填卵(塊)石，石塊外購","0237460023","m3",{"v":11.67,"d":"11.670"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[379,"邊坡穩定水平排水管，塑膠管(不分類)","0237700001","m",{"v":11.31,"d":"11.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[380,"邊坡穩定水平排水管，塑膠管，D=50mm(t=4.1mm)","0237700201","m",2.693,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[381,"邊坡穩定水平排水管，塑膠管，D=75mm(t=5.5mm)","0237700501","m",5.285,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[382,"邊坡穩定水平排水管，塑膠管，D=100mm(t=6.6mm)","0237700701","m",8.182,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[383,"邊坡穩定水平排水管，塑膠管，D=150mm(t=8.9mm)","0237700C01","m",16.082,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[384,"邊坡穩定水平排水管，塑膠管，D=200mm(t=10.3mm)","0237700H01","m",{"v":24.31,"d":"24.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[385,"∮3 吋管徑 PVC 洩水管(厚≧5.0mm)及安裝","023770303","m",{"v":6.84,"d":"6.840"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[386,"拋石","0238100003","m3",5.022,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[387,"拋石，塊石(長徑：15~40cm)","02381B0002","m2",{"v":8.08,"d":"8.080"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[388,"拋石，大塊石(長徑：41~80cm)","02381B0002","m2",{"v":11.33,"d":"11.330"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[389,"拋石，巨石(長徑：80cm 以上)","02381E0002","m2",{"v":14.29,"d":"14.290"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[390,"拋石，卵石(長徑：15cm 以下)","02381A0002","m2",{"v":5.31,"d":"5.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[391,"混凝土塊(不分類)","023840000A","塊",996.719,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[392,"混凝土塊，重 2t，含製作及吊放","023844010A","塊",202.712,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[393,"混凝土塊，重 5t，含製作及吊放","023847010A","塊",463.452,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[394,"混凝土塊，重 10t，含製作及吊放","02384B010A","塊",883.717,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[395,"混凝土塊，重 15t，含製作及吊放","02384D010A","塊",1348.259,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[396,"混凝土塊，重 20t，製作","02384E020A","塊",1735.132,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[397,"混凝土塊，重 20t，吊放","02384E050A","塊",29.378,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[398,"坡面工(不分類)","0238500002","m2",33.032,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[399,"坡面工，混凝土，厚 20cm","0238510302","m2",{"v":26.56,"d":"26.560"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[400,"坡面工，混凝土，厚 30cm","0238510502","m2",39.504,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[401,"砌排石工(不分類)","0238600002","m2",12.898,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[402,"砌排石工，舖石，塊石(15≦∮≦40cm、厚 25cm、未含溝縫)","0238621202","m2",0.975,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[403,"砌排石工，乾砌石，塊石(15≦∮≦40cm，厚 25cm，未含溝縫)","0238631202","m2",1.221,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[404,"砌排石工，漿砌石，(塊石，厚 25cm，未含勾縫)","0238641502","m2",{"v":11.27,"d":"11.270"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[405,"砌排石工，混凝土排石，(塊石，厚 25cm，未含勾縫)","0238651502","m2",15.646,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[406,"砌排石工，混凝土襯排石，(塊石，厚 25cm，未含勾縫)","0238661502","m2",35.376,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[407,"砌排石工，乾砌石，卵石(15cm 以下)","0238610102","m2",{"v":0.36,"d":"0.360"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[408,"砌排石工，乾砌石，大塊石(41≦∮≦80cm)","0238614102","m2",{"v":8.86,"d":"8.860"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[409,"砌排石工，混凝土砌石，大塊石(41≦∮≦80cm)，1:3 水泥 砂漿表面勾縫","0238634102","m2",{"v":43.58,"d":"43.580"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[410,"砌排石工，乾砌石，巨石(80cm≦∮≦120cm)","0238616102","m2",{"v":12.3,"d":"12.300"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[411,"砌排石工，乾砌石，角石(約 25cm)","023861A002","m2",{"v":0.6,"d":"0.600"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[412,"砌排石工，乾砌石，再生粒料混凝土塊(20*30*45~50cm)","023861B002","m2",{"v":170.08,"d":"170.080"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[413,"砌排石工，舖石，卵石(15cm 以下)","0238620102","m2",{"v":0.36,"d":"0.360"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[414,"砌排石工，舖石，大塊石(41≦∮≦80cm)","0238623002","m2",{"v":7.38,"d":"7.380"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[415,"砌排石工，混凝土砌石，卵石(15cm 以下)，1:3 水泥砂漿表面勾縫","0238630102","m2",{"v":25,"d":"25.000"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[416,"砌排石工，混凝土砌石，塊石，30*30*45cm 親水平台外緣 (石材另計)，1:3 水泥砂漿表面勾縫","0238632101","m",{"v":22.55,"d":"22.550"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[417,"砌排石工，混凝土砌石，塊石(15≦∮≦40cm)，1:3 水泥砂 漿表面勾縫","0238632102","m2",{"v":25.3,"d":"25.300"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[418,"砌排石工，混凝土砌石，巨石，1:3 水泥砂漿表面勾縫","0238636102","m2",{"v":24.89,"d":"24.890"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[419,"砌排石工，混凝土砌石，角石(約 25cm)，1:3 水泥砂漿表面 勾縫","023863A102","m2",{"v":14.31,"d":"14.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[420,"砌排石工，混凝土砌石，再生粒料混 凝土塊 (20*30*45~50cm)，1:3 水泥砂漿表面勾縫","023863B102","m2",{"v":189.77,"d":"189.770"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[421,"邊坡穩定，∮12 吋管徑 HDPE 螺旋式排水管(有孔)，安裝 及埋設(連工帶料)","0239100202","m",{"v":50.76,"d":"50.760"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[422,"預力混凝土基樁(不分類，B 種)","0245700001","m",79.581,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[423,"預力混凝土基樁，D=300mm，B 種","0245712001","m",35.604,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[424,"預力混凝土基樁，D=500mm，B 種","0245752001","m",66.232,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[425,"預力混凝土基樁，D=600mm，B 種","0245762001","m",85.168,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[426,"預力混凝土基樁，D=800mm，B 種","0245782001","m",131.318,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[427,"預力混凝土基樁，D=800mm，B 種，L=12m","0245782C0A","支",1626.521,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[428,"預力混凝土基樁(不分類)","024570000A","支",1626.521,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[429,"鋼軌樁，打樁施作(樁材另計)","0246200011","m",{"v":15.33,"d":"15.330"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[430,"鑽掘樁(不分類)","0246500001","m",0.483,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[431,"微型樁(不分類，D=30cm)","0247250008","組",883.429,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[432,"微型樁，D=30cm，L=4.5m","0247253008","組",680.958,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[433,"微型樁，D=30cm，L=6m","0247254008","組",863.182,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[434,"微型樁，D=30cm，L=8m","0247255008","組",1106.148,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[435,"自來水用塑膠管，聚氯乙烯塑膠管(不分類)","0251110001","m",{"v":11.3104,"d":"11.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[436,"自來水用塑膠管，聚氯乙烯塑膠管，D=50mm(t=4.1mm)","0251114001","m",2.693,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[437,"自來水用塑膠管，聚氯乙烯塑膠管，D=75mm(t=5.5mm)","0251117001","m",5.285,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[438,"自來水用塑膠管，聚氯乙烯塑膠管，D=100mm(t=6.6mm)","025111A001","m",8.182,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[439,"自來水用塑膠管，聚氯乙烯塑膠管，D=150mm(t=8.9mm)","025111E001","m",16.082,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[440,"自來水用塑膠管，聚氯乙烯塑膠管，D=200mm(t=10.3mm)","025111H001","m",{"v":24.31,"d":"24.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[441,"自來水用塑膠管，高密度聚乙烯管，D=200mm(t=11.9mm)","025115H001","m",{"v":17.28,"d":"17.280"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[442,"污水管管材，鋼筋混凝土管 (不分類)","0253310001","m",{"v":205.49,"d":"205.490"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[443,"污水管管材，鋼筋混凝土管(不分類，L=2.4m) ","025331000A","支",493.176,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[444,"污水管管材，鋼筋混凝土 管，D=600mm","0253319001","m",151.338,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[445,"污水管管材，鋼筋混凝土 管，D=600mm(L=2.4m)","025331900A","支",363.212,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[446,"污水管管材，鋼筋混凝土 管，D=800mm","025331B001","m",205.708,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[447,"污水管管材，鋼筋混凝土 管，D=800mm(L=2.4m)","025331B00A","支",{"v":493.7,"d":"493.700"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[448,"污水管管材，鋼筋混凝土 管，D=1000mm","025331D001","m",259.424,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[449,"污水管管材，鋼筋混凝土 管，D=1000mm(L=2.4m)","025331D00A","支",622.617,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[450,"污水管管材，聚氯乙烯塑膠硬質管，D=200mm(t=10.3mm) ","0253391201","m",{"v":24.31,"d":"24.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[451,"排水管溝，塑膠管(不分類) ","0260100001","m",{"v":11.31,"d":"11.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[452,"排水管溝，塑膠管，D=100mm(t=6.6mm) ","02601B1001","m",8.182,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[453,"排水管溝，塑膠管，D=150mm(t=8.9mm) ","02601B3001","m",16.082,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[454,"排水管溝，塑膠管，D=200mm(t=10.3mm) ","02601B4001","m",{"v":24.31,"d":"24.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[455,"ψ3\"PVC 管(CNS，t≧5.1mm)安裝","02601A0001","m",{"v":6.75,"d":"6.750"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[456,"排水管溝，塑膠管 B 管，D=200mm","02601B4001","m",9.789,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[457,"管涵，鋼筋混凝土管 B 型(不分類)","0260220001","m",{"v":205.49,"d":"205.490"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[458,"管涵，鋼筋混凝土管 B 型(不分類，L=2.4m) ","0260220007","個",493.176,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[459,"管涵，鋼筋混凝土管 B 型，D=600mm ","0260229001","m",151.338,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[460,"管涵，鋼筋混凝土管 B 型，D=600mm(L=2.4m) ","0260229007","個",363.212,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[461,"管涵，鋼筋混凝土管 B 型，D=800mm","026022B001","m",205.708,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[462,"管涵，鋼筋混凝土管 B 型，D=800mm(L=2.4m)","026022B007","個",{"v":493.7,"d":"493.700"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[463,"管涵，鋼筋混凝土管 B 型，D=1000mm","026022D001","m",259.424,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[464,"管涵，鋼筋混凝土管B型，D=1000mm(L=2.4m)","026022D007","個",622.617,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[465,"排水管涵，鋼筋混凝土管(不分類，L=2.4m)","026102D00A","支",{"v":493.176333333333,"d":"493.176"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[466,"排水管涵，鋼筋混凝土管(B型)，D=600mm","026102D001","m",151.338,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[467,"排水管涵，鋼筋混凝土管(B型)，D=600mm(L=2.4m)","026102D00A","支",363.212,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[468,"排水管涵，鋼筋混凝土管(B型)，D=800mm","026102F001","m",205.708,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[469,"排水管涵，鋼筋混凝土管(B型)，D=800mm(L=2.4m)","026102F00A","支",{"v":493.7,"d":"493.700"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[470,"排水管涵，鋼筋混凝土管(B型)，D=1000mm","026102H001","m",259.424,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[471,"排水管涵，鋼筋混凝土管(B型)，D=1000mm(L=2.4m)","026102H00A","支",622.617,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[472,"排水管涵，聚氯乙烯排水管，D=50mm(t=4.1mm)","0261081001","m",2.693,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[473,"排水管涵，聚氯乙烯排水管，D=75mm(t=5.5mm)","0261082001","m",5.285,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[474,"排水管涵，聚氯乙烯排水管，D=100mm(t=6.6mm)","0261083001","m",8.182,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[475,"排水管涵，聚氯乙烯排水管，D=150mm(t=8.9mm)","0261085001","m",16.082,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[476,"排水管涵，聚氯乙烯排水管，D=200mm(t=10.3mm)","0261086001","m",{"v":24.31,"d":"24.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[477,"鋼筋混凝土管(A 型)，D=600mm，連工帶料","026101D101","m",{"v":163.63,"d":"163.630"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[478,"塑膠管","0261080001","m",9.789,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[479,"級配粒料基層，總厚 5cm","0272201002","m2",{"v":3.76,"d":"3.760"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[480,"級配粒料基層，總厚 10cm","0272202002","m2",{"v":7.52,"d":"7.520"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[481,"級配粒料基層，總厚 15cm","0272203002","m2",{"v":11.28,"d":"11.280"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[482,"級配粒料基層，總厚 20cm","0272204002","m2",{"v":15.04,"d":"15.040"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[483,"級配粒料「基層」，鋪設及滾壓，壓實厚 20cm，再生級配 粒料","0272254002","m2",{"v":15.04,"d":"15.040"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[484,"級配粒料底層(不分類)","0272600003","m3",5.113,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[485,"級配粒料底層，總厚 10cm，鋪設及滾壓","0272601052","m2",{"v":7.52,"d":"7.520"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[486,"級配粒料底層，總厚 15cm，鋪設及滾壓","0272602052","m2",{"v":11.28,"d":"11.280"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[487,"級配粒料底層，總厚 20cm，鋪設及滾壓","0272603052","m2",{"v":15.04,"d":"15.040"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[488,"級配粒料「底層」，鋪設及滾壓，壓實厚 5cm","027260H052","m2",{"v":3.76,"d":"3.760"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[489,"碎石級配粒料(含運費及滾壓)","0272610000","m3",{"v":32.67,"d":"32.670"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[490,"瀝青混凝土鋪面(不分類)","0274200002","m2",16.207,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[491,"瀝青混凝土鋪面，厚5cm","027420D002","m2",11.699,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[492,"瀝青混凝土鋪面，厚8cm","027420G002","m2",18.406,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[493,"瀝青混凝土鋪面，厚10cm","027420J002","m2",23.204,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[494,"多孔隙瀝青混凝土鋪面，厚5cm","027428D002","m2",11.518,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[495,"瀝青透層(不分類)","0274500002","m2",2E-3,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[496,"瀝青黏層(不分類)","0274700002","m2",2E-3,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[497,"舖單元磚(不分類)","0278000002","m2",33.739,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[498,"濕式壓花地坪","0278040002","m2",60.582,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[499,"乾式噴花地坪","0278040002","m2",6.896,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[500,"乾式壓花地坪","0278040002","m2",{"v":6.87,"d":"6.870"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[501,"反光導標及安裝","0289200007","個",{"v":0.07,"d":"0.070"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[502,"道路施工及復舊(不分類)","0295200002","m2",16.207,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[503,"道路施工及復舊(不分類)","0295200001","m",16.207,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[504,"瀝青混凝土面層刨除(不分類，厚5cm)","0296100002","m2",2.094,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[505,"瀝青混凝土面層刨除","0296100002","m2",7.484,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[506,"瀝青混凝土面層刨除，厚5cm，刨除機2.2m寬","0296140402","m2",2.094,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[507,"瀝青混凝土面層刨除，刨除料運費","0296103003","m3",17.032,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[508,"再生瀝青混凝土，舖築及滾壓(不分類，含料)","0296600003","m3",85.209,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[509,"再生瀝青混凝土，舖築及滾壓(不分類，含料)","0296600005","t",36.259,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[510,"再生瀝青混凝土(不分類)","0296600005","t",17.767,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[511,"再生瀝青混凝土，(密級配，40%回收料)，舖築及滾壓","02966200B3","m3",84.384,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[512,"場鑄結構混凝土用模板(不分類)","0311000002","m2",1.543,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[513,"場鑄結構混凝土用模板，普通模板，一般工程用","0311011002","m2",{"v":0.29,"d":"0.290"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[514,"場鑄結構混凝土用模板，普通模板，建築","0311011502","m2",{"v":0.29,"d":"0.290"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[515,"場鑄結構混凝土用模板，清水模板","0311020002","m2",{"v":1.01,"d":"1.010"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[516,"場鑄結構混凝土用模板，免拆模板，木質","0311060002","m2",0.852,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[517,"場鑄結構混凝土用模板，免拆模板，鋼質","0311070002","m2",86.052,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[518,"場鑄結構混凝土用模板，鋼製模板","0311090002","m2",8.897,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[519,"場鑄結構混凝土用模板，造型模板","03110A0002","m2",3.253,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[520,"場鑄結構混凝土用模板，小搬運","0311002102","m2",{"v":17.12,"d":"17.120"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[521,"場鑄結構混凝土用模板，結構模板","0311002202","m2",{"v":0.29,"d":"0.290"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[522,"場鑄結構混凝土用模板，普通模板，軀体","0311012102","m2",{"v":0.29,"d":"0.290"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[523,"場鑄結構混凝土用模板，基礎模板","0311012201","m2",{"v":0.29,"d":"0.290"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[524,"場鑄結構混凝土用模板，普通模板， 基礎","0311012202","m2",{"v":0.29,"d":"0.290"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[525,"場鑄結構混凝土用模板，清水模板，軀体","0311022102","m2",{"v":1.01,"d":"1.010"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[526,"場鑄結構混凝土用模板，鋼模板","0311032100","m2",{"v":8.28,"d":"8.280"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[527,"場鑄結構混凝土用模板，景觀造型模板","03110C0002","m2",{"v":2.48,"d":"2.480"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[528,"鋼筋(不分類)","0321000005","t",{"v":983.72,"d":"983.720"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[529,"鋼筋(不分類)","0321000009","kg",0.984,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[530,"鋼筋，SD280，連工帶料","0321030075","t",{"v":983.72,"d":"983.720"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[531,"鋼筋，SD280，連工帶料","0321030079","kg",0.984,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[532,"鋼筋，SD280W，連工帶料","0321040075","t",{"v":983.72,"d":"983.720"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[533,"鋼筋，SD280W，連工帶料","0321040079","kg",0.984,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[534,"鋼筋，SD420W，連工帶料","0321050075","t",{"v":983.72,"d":"983.720"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[535,"鋼筋，SD420W，連工帶料","0321050079","kg",0.984,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[536,"鋼筋","03210000A5","t",{"v":983.72,"d":"983.720"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[537,"鋼筋加工及組立(鋼筋另計)","0321030003","t",{"v":9.31,"d":"9.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[538,"鋼筋加工及組立(含鋼筋)","0321030004","t",{"v":993.03,"d":"993.030"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[539,"鋼筋，SD280","0321030005","t",{"v":835,"d":"835.000"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[540,"鋼筋，SD280，小搬運","0321030015","t",{"v":17.12,"d":"17.120"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[541,"鋼筋，竹節鋼筋","0321031002","t",{"v":919,"d":"919.000"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[542,"銲接鋼線網，線徑10mm，方孔10x10cm","0322006142","kg",10.296,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[543,"銲接鋼線網，線徑10mm，方孔15x15cm","0322006162","kg",6.864,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[544,"銲接鋼線網，線徑10mm，方孔20x20cm","0322006182","kg",5.152,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[545,"銲接鋼線網(不分類，線徑 10mm)","0322000079","kg",6.556,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[546,"8mm 點焊鋼絲網(10*10cm)連工帶料","032203082","m2",{"v":0.6,"d":"0.600"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[547,"結構用混凝土(純水泥)(不分類)","0331000003","m3",340.284,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[548,"結構用混凝土，預拌，140kgf/cm2","0331023003","m3",{"v":293.57,"d":"293.570"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[549,"結構用混凝土，預拌，175kgf/cm2","0331024003","m3",344.288,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[550,"結構用混凝土，預拌，210kgf/cm2","0331025003","m3",{"v":324.34,"d":"324.340"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[551,"結構用混凝土，預拌，245kgf/cm2","0331026003","m3",{"v":334.52,"d":"334.520"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[552,"結構用混凝土，預拌，280kgf/cm2","0331027003","m3",{"v":344.62,"d":"344.620"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[553,"結構用混凝土，預拌，350kgf/cm2","0331029003","m3",{"v":375.21,"d":"375.210"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[554,"結構用混凝土，預拌，420kgf/cm2","033102C003","m3",{"v":405.65,"d":"405.650"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[555,"結構用混凝土，混凝土小搬運費","0331000003","m3",{"v":17.12,"d":"17.120"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[556,"結構用混凝土，預拌，澆置及搗實","03310000Z3","m3",{"v":0.14,"d":"0.140"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[557,"混凝土表面處理，水泥拉毛處理(掃紋)","0336060002","m2",{"v":1.36,"d":"1.360"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[558,"控制性低強度回填材料(CLSm)","0337700013","m3",94.495,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[559,"預鑄混凝土，異形塊(不分類)","034000000A","塊",{"v":926.6544,"d":"926.654"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[560,"預鑄混凝土，異形塊，5t","03400C100A","塊",463.452,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[561,"預鑄混凝土，異形塊，10t","03400C200A","塊",883.717,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[562,"預鑄混凝土，異形塊，15t","03400C300A","塊",1348.259,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[563,"預鑄混凝土，異形塊，20t","03400C400A","塊",1735.132,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[564,"預鑄混凝土，預鑄樑模板，製作及裝拆","034000AA02","m2",{"v":8.28,"d":"8.280"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[565,"太空包(含所有一切費用)","03400010A1","包",{"v":2.55,"d":"2.550"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[566,"港灣用預鑄混凝土塊(不分類)","034390000A","塊",996.719,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[567,"港灣用預鑄混凝土塊，重10t","03439B000A","塊",680.227,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[568,"港灣用預鑄混凝土塊，重20t","03439E000A","塊",1313.211,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[569,"水泥砂漿(不分類)","0406100003","m3",238.504,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[570,"水泥砂漿，1:1","0406110003","m3",{"v":952,"d":"952.000"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[571,"水泥砂漿，1:2","0406120003","m3",{"v":625,"d":"625.000"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[572,"水泥砂漿，1:3","0406130003","m3",{"v":437,"d":"437.000"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[573,"水泥砂漿，1:4","0406140003","m3",{"v":390.95,"d":"390.950"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[574,"混凝土植草磚(磚材另計)","0422200002","m2",{"v":1.03,"d":"1.030"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[575,"金屬材料(不分類，鋼)","0506000009","kg",{"v":2.42,"d":"2.420"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[576,"金屬材料(不分類)","0506000009","kg",{"v":2.13,"d":"2.130"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[577,"直徑 20mm 鋼索","0506015851","m",{"v":4.88,"d":"4.880"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[578,"金屬材料，鐵線","0506020009","kg",{"v":2.13,"d":"2.130"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[579,"鋼索夾","05060D6008","組",{"v":70.55,"d":"70.550"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[580,"金屬製品，不銹鋼踏步(D=19mm實心)","05500f0001","m",3.895,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[581,"金屬製品，不鏽鋼踏步(不分類)","05500f0001","m",0.644,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[582,"金屬製品，不銹鋼踏步(D=19mm實心)","05500f0007","個",{"v":3.35,"d":"3.350"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[583,"金屬製品，不銹鋼踏步(D=19mm實心)","05500f0R08","組",{"v":3.35,"d":"3.350"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[584,"金屬製品，不銹鋼踏步(D=19mm實心)","05500f000A","支",{"v":3.35,"d":"3.350"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[585,"不銹鋼欄杆(不分類)","0552300001","m",18.505,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[586,"金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座(不分類)","0553000008","組",{"v":255.7945,"d":"255.795"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[587,"金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=60cm(52.6kg)","05530BD008","組",157.274,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[588,"金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=70cm(70.1kg)","05530BE008","組",209.599,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[589,"金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=80cm(99.5kg)","05530BF008","組",297.505,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[590,"金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=90cm(120kg)","05530BG008","組",{"v":358.8,"d":"358.800"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[591,"金屬格柵蓋板(不分類)","0553000008","組",{"v":24,"d":"24.000"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[592,"金屬格柵蓋板，鍍鋅格柵蓋板(鍍鋅鋼材 1kg 碳排放 0.93kgCO2e)","0553060008","組",{"v":33,"d":"33.000"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[593,"金屬格柵蓋板，鍍鋅格柵板及框座，W=40cm(鍍鋅鋼材 1kg 碳排放 0.93kgCO2e)","055307B008","組",{"v":15,"d":"15.000"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[594,"不銹鋼水尺","057330D008","組",100.323,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[595,"保麗龍填縫料","0792031102","m2",{"v":1.96,"d":"1.960"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[596,"水泥砂漿粉刷，1：3水泥砂漿，牆面，打底","0922030322","m2",{"v":9.83,"d":"9.830"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[597,"洗石子","0978000002","m2",8.089,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[598,"抿石子，(打底及工資)","0978000102","m2",3.518,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[599,"斬石子","0978100002","m2",{"v":122.32,"d":"122.320"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[600,"抿石子","0978200002","m2",8.089,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[601,"油漆，一底二度","0991002002","m2",{"v":1.7,"d":"1.700"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[602,"材料，水泥漆，水性水泥漆","099120A002","kg",1.33,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[603,"聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)(不分類)",1510720001,"m",{"v":11.3104,"d":"11.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[604,"聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=50mm(t=4.1mm)","1510727001","m",2.693,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[605,"聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=75mm(t=5.5mm)","1510729001","m",5.285,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[606,"聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=100mm(t=6.6mm)","151072B001","m",8.182,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[607,"聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=150mm(t=8.9mm)","151072D001","m",16.082,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[608,"聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=200mm(t=10.3mm)","151072E001","m",{"v":24.31,"d":"24.310"},"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[609,"產品，臨時擋土樁設施，鋼軌樁37kg/m，L=6m",null,"m",32.34,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[610,"產品，臨時擋土樁設施，鋼軌樁50kg/m，L=7m",null,"m",43.89189189,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[611,"產品，臨時擋土樁設施，鋼軌樁42kg/m，L=4m(永久性，堪用品)",null,"支",16.49,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[612,"產品，選擇性回填材料，透水材料，粗砂(含人工)",null,"m3",11.98,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[613,"產品，塊石(含運費)",null,"m3",2.4,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[614,"產品，選擇性回填材料，透水材料，碎石(含人工)",null,"m3",21.59,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[615,"產品，選擇性回填材料，級配粒料",null,"m3",15.16,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[616,"產品，選擇性回填材料，級配粒料，碎石級配",null,"m3",15.06,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[617,"產品，選擇性回填材料，級配粒料，天然級配",null,"m3",15.06,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[618,"產品，地工織物，土木工程用非織物，濾石網袋",null,"m",0.26,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[619,"產品，地工織物，土木工程用非織物，土包袋",null,"m",0.26,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[620,"鋼筋小搬運",null,"t",0.11,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[621,"產品，生態護坡，稻草蓆敷蓋",null,"m2",0.016,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[622,"產品，生態護坡，客土袋",null,"個",0.04,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[623,"產品，生態護坡，鋼筋樁，∮=13m/m，L=55cm~70cm",null,"支",7.77,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[624,"產品，邊坡穩定水平排水管，濾水袋",null,"個",0.03,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[625,"洩水管(B管，t≧5.0mm)",null,"m",6.84,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[626,"產品，卵、塊石",null,"m3",2.4,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[627,"產品，卵、塊石（約∮30cm)",null,"m3",2.4,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[628,"產品，塊石(外購)",null,"m3",12.222,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[629,"產品，大塊石",null,"m3",11.33,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[630,"產品，大塊石，現採",null,"m3",11.33,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[631,"產品，大塊石(外購)",null,"m3",12.222,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[632,"排水器(含安裝)",null,"組",1.2,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[633,"產品，級配粒料底、基層，碎石級配粒料(含運送及滾壓施作)",null,"m2",2.63,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[634,"產品，級配粒料底、基層，再生級配粒料(含運送及滾壓施作)",null,"m2",1.95,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[635,"PE土包袋(含堆疊施作)",null,"包",0.26,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[636,"客土袋(≧60cm*≧40cm)",null,"包",0.04,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[637,"客土袋堆疊施作",null,"m",5.37,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[638,"產品，再生混凝土，級配粒料",null,"m2",97.51,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[639,"卜特蘭水泥(Ⅱ型)",null,"kg",0.981,"搖籃到大門 ","產品碳足跡資訊網",null,2020,"農業部農村水保署",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                                  2.修正產品名稱 "]
[640,"產品，鋼模板",null,"m2",8.54,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[641,"產品，混凝土附屬品，保麗龍、伸縮縫或3分夾板",null,"組",1.96,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[642,"產品，擋土牆抽排水(市售排水器)",null,"m",13.54,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[643,"產品，金屬材料，鐵、鋼線",null,"kg",0.612,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[644,"產品，金屬材料，鐵、鋼線(鍍鋅)",null,"kg",1.56,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[645,"產品，金屬材料，鐵、鋼件(鍛造)",null,"kg",2.13,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[646,"石膏板",null,"kg",{"v":0.51,"d":"0.510"},"搖籃到大門 ","產品碳足跡資訊網",null,2015,"農業部農村水保署",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱及公告年分"]
[647,"水性水泥漆",null,"kg",{"v":1.33,"d":"1.330"},"搖籃到大門 ","產品碳足跡資訊網",null,2016,"農業部農村水保署",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱及公告年分"]
[648,"產品，白色油漆",null,"m2",1.7,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[649,"產品，無線傳訊模組數據機(租用)",null,"組",0.016,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[650,"產品，硬質聚氯乙烯塑膠管(B管厚管)，標稱80mm",null,"m",6.25,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[651,"產品，硬質聚氯乙烯塑膠管(B管厚管)，(標稱80mm，厚5.1mm)",null,"m",6.84,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[652,"產品，硬質聚氯乙烯塑膠管(B管厚管)，標稱125mm",null,"m",9.375,"規劃設計","水土保持工程減碳參考指引","尚未認證",2023,"農業部農村水保署"]
[653,"水泥(不分型號)","0305200009","kg",0.907,"搖籃到工地","產品碳足跡資訊網",null,2017,"內政部建築研究所",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳排放係數"]
[654,"一般水泥(卜特蘭)","0305200005","t",{"v":881.59,"d":"881.590"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[655,"卜特蘭水泥(I型) ",null,"kg",0.944,"搖籃到工地","低碳建築聯盟",null,2017,"內政部建築研究所",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正數據來源"]
[656,"卜特蘭水泥(II型) ","0305220009","kg",0.968,"搖籃到工地","低碳建築聯盟",null,2023,"內政部建築研究所",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正數據來源"]
[657,"白水泥","0305290005","t",{"v":968.4,"d":"968.400"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[658,"高爐水泥(爐石粉 30%)",null,"t",{"v":657.16,"d":"657.160"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[659,"高爐水泥(爐石粉 45%)",null,"t",{"v":534.35,"d":"534.350"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[660,"結構用混凝土，預拌，140kgf/cm2(2000psi)","0331023003","m3",{"v":243.78,"d":"243.780"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[661,"結構用混凝土，預拌，210kgf/cm2(3000psi)","0331025003","m3",{"v":327.75,"d":"327.750"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[662,"預拌高爐混凝土，210kgf/cm2(3000psi)","0331025003","m3",{"v":206.37,"d":"206.370"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[663,"結構用混凝土，預拌，280kgf/cm2(4000psi)","0331027003","m3",{"v":369.88,"d":"369.880"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[664,"預拌高爐混凝土，280kgf/cm2(4000psi)","0331027003","m3",{"v":231,"d":"231.000"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[665,"結構用混凝土，預拌，350kgf/cm2(5000psi)","0331029003","m3",{"v":433.45,"d":"433.450"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[666,"預拌高爐混凝土，350kgf/cm2(5000psi)","0331029003","m3",{"v":268.98,"d":"268.980"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[667,"結構用混凝土，預拌，420kgf/cm2(6000psi)","033102C003","m3",{"v":497.15,"d":"497.150"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[668,"預拌高爐混凝土，420kgf/cm2(6000psi)","033102C003","m3",{"v":306.23,"d":"306.230"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[669,"水中混凝土(210kgfcm2) ","033102C003","m3",{"v":242,"d":"242.000"},"搖籃到工地","產品碳足跡資訊網",null,2017,"內政部建築研究所",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳排放係數"]
[670,"水中混凝土(280kgf/cm2) ","033102C003","m3",{"v":275,"d":"275.000"},"搖籃到工地","產品碳足跡資訊網",null,2017,"內政部建築研究所",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳排放係數"]
[671,"噴凝土(210kgf/cm2)","0337202002","m3",{"v":404.12,"d":"404.120"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[672,"鋼纖維噴凝土(255kgf/cm2)","0337501003","m3",{"v":443.56,"d":"443.560"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[673,"1:1 水泥砂漿粉刷 2cm 厚","0406110002","m2",{"v":19.49,"d":"19.490"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[674,"1:2 水泥砂漿粉刷 2cm 厚","0406120002","m2",{"v":12.86,"d":"12.860"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[675,"1:3 水泥砂漿粉刷 2cm 厚","0406130002","m2",{"v":9.05,"d":"9.050"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[676,"普通玻璃","0881000009","kg",{"v":0.82,"d":"0.820"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[677,"1mm 普通玻璃","0881000102","m2",{"v":2.05,"d":"2.050"},"搖籃到工地","低碳建築聯盟","尚未認證",2019,"內政部建築研究所"]
[678,"平板玻璃","0881010009","kg",{"v":1.12,"d":"1.120"},"搖籃到大門","產品碳足跡資訊網",null,2017,"內政部建築研究所",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳排放係數"]
[679,"強化玻璃","0881030009","kg",{"v":1.75,"d":"1.750"},"搖籃到大門","產品碳足跡資訊網",null,2017,"內政部建築研究所",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱及碳排係數"]
[680,"強化玻璃","0881030009","kg",{"v":1.08,"d":"1.080"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[681,"強化玻璃(5mm)","0881030502","m2",{"v":22,"d":"22.000"},"搖籃到工地","低碳建築聯盟","尚未認證",2022,"內政部建築研究所"]
[682,"強化玻璃(8mm)","0881030802","m2",{"v":35.2,"d":"35.200"},"搖籃到工地","低碳建築聯盟","尚未認證",2022,"內政部建築研究所"]
[683,"強化玻璃(10mm)","0881030A02","m2",{"v":44,"d":"44.000"},"搖籃到工地","低碳建築聯盟","尚未認證",2022,"內政部建築研究所"]
[684,"反射玻璃",null,"kg",{"v":1.12,"d":"1.120"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[685,"5mm 反射玻璃",null,"m2",{"v":14,"d":"14.000"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[686,"6mm 反射玻璃",null,"m2",{"v":16.8,"d":"16.800"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[687,"8mm 反射玻璃",null,"m2",{"v":22.4,"d":"22.400"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[688,"10mm 反射玻璃",null,"m2",{"v":28,"d":"28.000"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[689,"12mm 反射玻璃",null,"m2",{"v":33.6,"d":"33.600"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[690,"1mm反射玻璃",null,"m2",{"v":2.8,"d":"2.800"},"搖籃到工地","低碳建築聯盟","尚未認證",2019,"內政部建築研究所"]
[691,"1+1mm反射玻璃",null,"m2",{"v":5.6,"d":"5.600"},"搖籃到工地","低碳建築聯盟","尚未認證",2019,"內政部建築研究所"]
[692,"1mm鏡面玻璃",null,"m2",{"v":2.5,"d":"2.500"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[693,"膠合安全玻璃","0881020009","kg",{"v":0.96,"d":"0.960"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[694,"雙層玻璃","0881060009","kg",{"v":0.95,"d":"0.950"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[695,"1+1mm雙層玻璃 ",null,"m2",{"v":4.75,"d":"4.750"},"搖籃到工地","低碳建築聯盟","尚未認證",2019,"內政部建築研究所"]
[696,"5+5mm雙層玻璃 ",null,"m2",{"v":20.63,"d":"20.630"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[697,"6+6mm雙層玻璃 ",null,"m2",{"v":24.76,"d":"24.760"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[698,"8+8mm雙層玻璃 ",null,"m2",{"v":33.01,"d":"33.010"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[699,"5+育璽 Hm-SC75+5mm 雙層玻璃",null,"m2",{"v":23.42,"d":"23.420"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[700,"6+育璽 Hm-SC75+6mm 雙層玻璃",null,"m2",{"v":27.56,"d":"27.560"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[701,"8+育璽 Hm-SC75+8mm 雙層玻璃",null,"m2",{"v":35.82,"d":"35.820"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[702,"5mm 普通或吸熱玻璃","0881080502","m2",{"v":10.25,"d":"10.250"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[703,"6mm 普通或吸熱玻璃","0881080602","m2",{"v":12.3,"d":"12.300"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[704,"8mm 普通或吸熱玻璃","0881080802","m2",{"v":16.4,"d":"16.400"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[705,"10mm 普通或吸熱玻璃","0881080A02","m2",{"v":20.5,"d":"20.500"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[706,"12mm 普通或吸熱玻璃","0881080C02","m2",{"v":24.6,"d":"24.600"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[707,"5＋5 mm 雙強化膠合玻璃","0881020502","m2",{"v":24,"d":"24.000"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[708,"6＋6 mm 雙強化膠合玻璃","0881020602","m2",{"v":28.8,"d":"28.800"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[709,"8＋8 mm 雙強化膠合玻璃","0881020802","m2",{"v":38.4,"d":"38.400"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[710,"5＋5 mm Low-E 玻璃","0881000502","m2",{"v":32.75,"d":"32.750"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[711,"6＋6 mm Low-E 玻璃","0881000602","m2",{"v":39.3,"d":"39.300"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[712,"8＋8 mm Low-E 玻璃","0881000802","m2",{"v":52.4,"d":"52.400"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[713,"南亞節能膜 NY-2039",null,"m2",{"v":0.86,"d":"0.860"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[714,"南亞節能膜 NY-2076",null,"m2",{"v":0.86,"d":"0.860"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[715,"Low-E 玻璃 ",null,"kg",{"v":1.31,"d":"1.310"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[716,"玻璃纖維絲",null,"kg",{"v":2.77,"d":"2.770"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[717,"玻璃纖維",null,"kg",{"v":2.53,"d":"2.530"},"搖籃到工地","低碳建築聯盟","尚未認證",2023,"內政部建築研究所"]
[718,"矽酸鈣","m092403300002","kg",{"v":0.22,"d":"0.220"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[719,"矽酸鈣板(6mm)","m092403300002","m2",{"v":1.36,"d":"1.360"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[720,"矽酸鈣板(9mm)","m092403500002","m2",{"v":1.92,"d":"1.920"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[721,"矽酸鈣板(12mm)","m092403800002","m2",{"v":2.54,"d":"2.540"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[722,"石膏板","0925010009","kg",{"v":0.51,"d":"0.510"},"搖籃到大門","產品碳足跡資訊網",null,2017,"內政部建築研究所",{"$nulls":7},"非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             ","刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             "]
[723,"石膏板(9mm) ","0925010019","m2",{"v":1.93,"d":"1.930"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[724,"石膏板(12mm) ","0925010039","m2",{"v":2.58,"d":"2.580"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[725,"石膏板(15mm) ","0925010059","m2",{"v":3.08,"d":"3.080"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[726,"貼磁磚外裝",null,"m2",{"v":28.7,"d":"28.700"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[727,"乾式石材外裝",null,"m2",{"v":12.79,"d":"12.790"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[728,"實木地板-軟木 ","0964010003","m3",{"v":195.13,"d":"195.130"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[729,"實木地板-硬木","0964010003","m3",{"v":394.49,"d":"394.490"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[730,"實木地板-竹","0964010003","m3",{"v":292.28,"d":"292.280"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[731,"實木地板(2cm)-軟木","0964010003","m2",{"v":3.9,"d":"3.900"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[732,"實木地板(2cm)-硬木","0964010003","m2",{"v":7.89,"d":"7.890"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[733,"實木地板(2cm)-竹","0964010003","m2",{"v":5.84,"d":"5.840"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[734,"實木皮木芯板(天然木化粧合板、複合木質、海島型木地板、木芯板)",null,"m3",{"v":382.75,"d":"382.750"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[735,"實木皮木芯板(天然木化粧合板、複合木質、海島型木地板、木芯板)(6 分板，18mm)",null,"m3",{"v":6.89,"d":"6.890"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[736,"合板 ",null,"m3",{"v":185.43,"d":"185.430"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[737,"合板(18mm) ",null,"m2",{"v":3.34,"d":"3.340"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[738,"單板層積材(LVL)",null,"m3",{"v":84,"d":"84.000"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[739,"單板層積材(LVL)(6分板18mm)",null,"m2",{"v":1.51,"d":"1.510"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[740,"集成材(集層材、膠合木)",null,"m3",{"v":159.66,"d":"159.660"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[741,"集成材(集層材、膠合木)(6分板18mm)",null,"m2",{"v":2.88,"d":"2.880"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[742,"高密度粒片板(塑合板，OSB定向粒片板、HDF，密度850kg/m3，18mm)",null,"m2",{"v":17.56,"d":"17.560"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[743,"中密度粒片板(密集板，mDF，密度 700kg/m3，18mm)",null,"m2",{"v":14.47,"d":"14.470"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[744,"原木(未乾燥防腐處理)-軟木",null,"m3",{"v":35.39,"d":"35.390"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[745,"原木(未乾燥防腐處理)-硬木",null,"m3",{"v":43.48,"d":"43.480"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[746,"原竹(未乾燥防腐處理)-竹",null,"m3",{"v":37.41,"d":"37.410"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[747,"木竹類製材(人工乾燥防腐\n處理)-軟木",null,"m3",{"v":89.94,"d":"89.940"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[748,"木竹類製材(人工乾燥防腐處理)-硬木",null,"m3",{"v":274.55,"d":"274.550"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[749,"木竹類製材(人工乾燥防腐處理)-竹",null,"m3",{"v":174.22,"d":"174.220"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[750,"竹籐編織",null,"m3",{"v":175.38,"d":"175.380"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[751,"竹籐編織(2.5mm) ",null,"m3",{"v":1.1,"d":"1.100"},"搖籃到工地","低碳建築聯盟","尚未認證",2017,"內政部建築研究所"]
[752,"RC 外牆 15cm",null,"m2",{"v":73.67,"d":"73.670"},"搖籃到工地","低碳建築聯盟","尚未認證",2021,"內政部建築研究所"]
[753,"RC 外牆 18cm",null,"m2",{"v":83.5,"d":"83.500"},"搖籃到工地","低碳建築聯盟","尚未認證",2021,"內政部建築研究所"]
[754,"清水混凝土外牆 20cm",null,"m2",{"v":102.15,"d":"102.150"},"搖籃到工地","低碳建築聯盟","尚未認證",2021,"內政部建築研究所"]
[755,"預鑄混凝土外牆 15cm",null,"m2",{"v":80.47,"d":"80.470"},"搖籃到工地","低碳建築聯盟","尚未認證",2021,"內政部建築研究所"]
[756,"空心磚牆",null,"m2",{"v":23.59,"d":"23.590"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[757,"1B 磚牆",null,"m2",{"v":106.79,"d":"106.790"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[758,"洗石子/斬石子/抿石子外裝",null,"m2",{"v":15.98,"d":"15.980"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[759,"玻璃帷幕牆",null,"m2",{"v":69.62,"d":"69.620"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[760,"鋁金屬帷幕牆",null,"m2",{"v":58.12,"d":"58.120"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[761,"花崗岩帷幕牆",null,"m2",{"v":39.95,"d":"39.950"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[762,"窗框-鋁框架構造（陽極或氟碳烤漆）",null,"m2",{"v":24.84,"d":"24.840"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[763,"窗框-不鏽鋼框架構造",null,"m2",{"v":25.6,"d":"25.600"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[764,"塑鋼窗框構造（含補強鐵件）",null,"m2",{"v":11.74,"d":"11.740"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[765,"軟木木窗框",null,"m2",{"v":1.71,"d":"1.710"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[766,"硬木木窗框",null,"m2",{"v":5.22,"d":"5.220"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[767,"鋁帷幕框架構造（陽極或氟碳烤漆）",null,"m2",{"v":30.32,"d":"30.320"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[768,"不鏽鋼帷幕框架構造",null,"m2",{"v":46.63,"d":"46.630"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[769,"塑鋼帷幕構造（含補強鐵件）",null,"m2",{"v":24.06,"d":"24.060"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[770,"抓釘式帷幕框架",null,"m2",{"v":46.63,"d":"46.630"},"搖籃到工地","低碳建築聯盟","尚未認證",2018,"內政部建築研究所"]
[771,"選擇性回填材料，透水材料，砂","0231911003","m3",7.939,null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[772,"級配粒料底層，碎石級配","0272610003","m3",6.428,null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[773,"瀝青混凝土鋪面，(第 1 類型，密級配)，黏度 AC-10，拌和廠交貨","0274210225","t",{"v":93.6889,"d":"93.689"},null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[774,"瀝青混凝土鋪面，(第 1 類型， 密級配)，黏度 AC-20，工地交貨","0274210335","t",{"v":68.7076,"d":"68.708"},null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[775,"瀝青混凝土鋪面，(第 1 類型，密級配)，粗粒料 19.0mm，拌和廠交貨","0274213025","t",{"v":78.6783,"d":"78.678"},null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[776,"瀝青混凝土鋪面，(第 1 類型，密級配)，粗粒料 19.0mm，針入度 60~70","0274213D03","m3",{"v":171.1707,"d":"171.171"},null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[777,"人行道面層鋪面磚(高壓)","0277850003","m2",{"v":49.5368,"d":"49.537"},null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[778,"透水性鋪面，多孔性瀝青混凝土","0279800005","t",{"v":67.3417,"d":"67.342"},null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[779,"透水性鋪面，塊狀及鏤空狀，植草磚，5≦面層厚＜10cm","0279800005","m2",27.048,null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[780,"粒料，粗粒料","0305021003","m3",{"v":6.518087631,"d":"6.518"},null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[781,"混凝土基本材料及施工方法\n粒料，細粒料","0305021003","m3",{"v":7.49131879,"d":"7.491"},null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[782,"粒料\n細粒料(細砂，粉光用)","0305022203","m3",{"v":9.4890038,"d":"9.489"},null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[783,"水泥砂漿1:3，第 1 型水泥","0406131003","m3",{"v":49.1908,"d":"49.191"},null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[784,"洗石子，宜蘭石","0406131003","kg",0.103,null,"成功大學-永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","尚未認證",null,"內政部國土管理署"]
[785,"鋼筋混凝土管涵(B 型)，100cmφ，Ⅲ級","025331D001","m",0.157,null,"南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","經BSI第三方查驗證",2022,"交通部公路局"]
[786,"鋼筋混凝土管涵(B 型)，60cmφ，Ⅲ級","0253319001","m",0.157,null,"南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","經BSI第三方查驗證",2022,"交通部公路局"]
[787,"竹節鋼筋，SD280W","0321040009","kg",{"v":0.81,"d":"0.810"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[788,"竹節鋼筋，SD420W","0321060009","kg",{"v":0.81,"d":"0.810"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[789,"竹節鋼筋，SD280W","0321040005","t",0.874,"規劃設計","2016年國內海光鋼鐵實際盤查","經BSI第三方查驗證",2019,"交通部公路局"]
[790,"竹節鋼筋，SD420W","0321060005","t",{"v":0.91,"d":"0.910"},"規劃設計","2017年國內海光鋼鐵實際盤","經BSI第三方查驗證",2019,"交通部公路局"]
[791,"預拌混凝土(80kgf/cm2)","0331021003","m3",{"v":207,"d":"207.000"},"搖籃到大門","產品碳足跡資訊網","經BSI第三方查驗證",2017,"交通部鐵道局南部工程分局",{"$nulls":7},"非本部公告之係數                                                                                                                                                                                                                                                                                                                                                                                                    ","1.修正產品名稱                                                                                                                                                                                                                                                                                                                                                                                                             2.修正提報單位"]
[792,"混凝土(175) ","0331024009","kg",{"v":215.17,"d":"215.170"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[793,"混凝土(210水中)","0331045009","kg",{"v":257.84,"d":"257.840"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[794,"混凝土(210)","0331025009","kg",{"v":230.54,"d":"230.540"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[795,"混凝土，280kgf/cm2，第 II 型水泥","0331027203","m3",{"v":237.07,"d":"237.070"},null,"2017年本團隊根基預拌廠實際盤查值",null,null,"交通部公路局"]
[796,"混凝土(280I I型 ) ","0331027209","kg",{"v":276.81,"d":"276.810"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[797,"混凝土(280水中 ) ","0331047009","kg",{"v":284.58,"d":"284.580"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[798,"混凝土，水中280kgf/cm2，第 II 型水泥","0331047003","m3",275.239,"規劃設計"," 南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","經BSI第三方查驗證",2022,"交通部公路局"]
[799,"混凝土，420kgf/cm2，第 II 型水泥","033102C203","m3",{"v":423.86,"d":"423.860"},null,"2017年本團隊根基預拌廠實際盤查值",null,null,"交通部公路局"]
[800,"噴凝土(210) ","0337202003","m3",{"v":394.37,"d":"394.370"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[801,"鋼纖維噴凝土(255)","0337501003","m3",{"v":432.77,"d":"432.770"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[802,"鋼橋，鋼梁，Gr.50(不含側推工法)","051211C005","t",2.839,null,"南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","經BSI第三方查驗證",2022,"交通部公路局"]
[803,"UIC60 鋼軌","05651H0001","m",0.947,null,"2014年本團隊東和鋼鐵高雄廠實際盤查",null,2014,"交通部公路局"]
[804,"16CH 矩陣式多工數位主機","137046000B","套",220,null,"南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","經BSI第三方查驗證",2022,"交通部公路局"]
[805,"混凝土(420SCC)",null,"kg",333.99,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[806,"混凝土(350SCCR1)",null,"kg",310.92,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[807,"混凝土(420早強)",null,"kg",343.5,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[808,"混凝土(245)",null,"kg",247.75,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[809,"鋼管",null,"kg",{"v":2.46,"d":"2.460"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[810,"鐵板",null,"kg",{"v":1.95,"d":"1.950"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[811,"標線",null,"kg",{"v":20.37,"d":"20.370"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[812,"玻璃珠",null,"kg",{"v":0.12,"d":"0.120"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[813,"防眩板",null,"kg",{"v":2.13,"d":"2.130"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[814,"高鍍鋅鐵線(5mm)",null,"kg",{"v":0.63,"d":"0.630"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[815,"熱浸鍍鋅格柵板",null,"kg",{"v":2.31,"d":"2.310"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[816,"PVC 塑膠硬質管 (2\"*3.0*4m)",null,"kg",{"v":3.23,"d":"3.230"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[817,"盤式支承(橡膠)",null,"kg",{"v":3.34,"d":"3.340"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[818,"盤式支承(鍛鋼)",null,"kg",{"v":2.31,"d":"2.310"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[819,"預力套管",null,"kg",{"v":2.47,"d":"2.470"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[820,"續接器",null,"kg",{"v":2.31,"d":"2.310"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[821,"預力鋼絞線(15.2mm)",null,"kg",{"v":2.16,"d":"2.160"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[822,"免拆網",null,"kg",{"v":0.63,"d":"0.630"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[823,"保麗龍",null,"kg",{"v":2.84,"d":"2.840"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[824,"路緣石",null,"kg",{"v":0.93,"d":"0.930"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[825,"人孔鑄鐵蓋",null,"kg",{"v":2.25,"d":"2.250"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[826,"防震拉條",null,"kg",{"v":0.81,"d":"0.810"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[827,"橋面洩水孔",null,"kg",{"v":2.31,"d":"2.310"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[828,"波型鋼版",null,"kg",{"v":1.95,"d":"1.950"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[829,"鋼結構",null,"kg",{"v":2.31,"d":"2.310"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[830,"油漆",null,"kg",{"v":2.45,"d":"2.450"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[831,"外置預力斜索-端錨",null,"kg",{"v":2.31,"d":"2.310"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[832,"外置預力斜索 (披覆 HDPE護套鋼 絞線)",null,"kg",{"v":2.16,"d":"2.160"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[833,"HDPE 外套管",null,"kg",{"v":1.6,"d":"1.600"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[834,"強力螺栓",null,"kg",{"v":2.25,"d":"2.250"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[835,"剪力釘",null,"kg",{"v":2.25,"d":"2.250"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[836,"預力鋼絞線(12.7mm)",null,"kg",{"v":2.16,"d":"2.160"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[837,"鍍鋅承壓板 (300*300*40mm)",null,"kg",{"v":1.95,"d":"1.950"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[838,"點焊鋼線網 (5*100*100mm)",null,"kg",{"v":0.63,"d":"0.630"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[839,"管幕鋼管、先撐鋼管",null,"kg",{"v":2.46,"d":"2.460"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[840,"預力地錨護管(平面、浪型)",null,"kg",{"v":1.6,"d":"1.600"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[841,"全螺紋岩釘(D25)",null,"kg",{"v":0.84,"d":"0.840"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[842,"PVC 防水膜",null,"kg",{"v":2.13,"d":"2.130"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[843,"拉線箱蓋版及框",null,"kg",{"v":3.47,"d":"3.470"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[844,"乳膠漆",null,"kg",{"v":2.45,"d":"2.450"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[845,"石英磚",null,"kg",{"v":0.2,"d":"0.200"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[846,"磁磚",null,"kg",{"v":0.2,"d":"0.200"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[847,"CH4排放係數(人員 化糞池排放源)",null,"人時",{"v":0.0398,"d":"0.040"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[848,"一般廢棄物處置排放 係數(人員)",null,"人時",0.504,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[849,"全拖車、大貨車(35t)",null,"tkm",{"v":0.14,"d":"0.140"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[850,"全拖車(43t)",null,"tkm",{"v":0.0996,"d":"0.100"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[851,"大貨車(傾卸 車)(20t、21t)",null,"tkm",0.333,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[852,"大貨車(預拌 車)(20t、21t)",null,"tkm",0.575,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[853,"小貨車(3t、3.49t)",null,"tkm",{"v":1.99,"d":"1.990"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[854,"預拌混凝土車",null,"tkm",10.052,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[855,"填縫劑",null,"包",{"v":0.94,"d":"0.940"},null,"南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","經BSI第三方查驗證",2022,"交通部公路局"]
[856,"混凝土(350SCCR1)",null,"kg",{"v":310.92,"d":"310.920"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[857,"混凝土(420SCC) ",null,"kg",{"v":333.99,"d":"333.990"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[858,"混凝土(420早強)",null,"kg",{"v":343.5,"d":"343.500"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[859,"水泥",null,null,0.96,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[860,"竹節鋼筋(SD280W、 SD420W)",null,"kg",0.81,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[861,"瀝青混凝土(1\"粗級配)",null,"kg",0.0883,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[862,"瀝青混凝土(3/4\"密級 配)",null,"kg",0.0875,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[863,"瀝青混凝土(1/2\"密級 配)",null,"kg",0.0834,"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2019,"交通部公路局"]
[864,"土方工作(不分類)","0230000003","m3",{"v":8.65,"d":"8.650"},"規劃設計","國道5號頭城交流道工程碳盤查","經BSI第三方查驗證",2019,"交通部高速公路局"]
[865,"瀝青處理底層(BtB)","0271400005","t",{"v":77.79,"d":"77.790"},"搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證","2023","交通部高速公路局"]
[866,"瀝青處理底層(BtB)","0271400003","m3",{"v":185.84,"d":"185.840"},"搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證",2023,"交通部高速公路局"]
[867,"瀝青處理底層(BtB) ","0271400005","t",{"v":75.41,"d":"75.410"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C713標)","經BSI第三方查驗證",2023,"交通部高速公路局"]
[868,"瀝青處理底層(BtB) ","0271400005","t",{"v":76.47,"d":"76.470"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C714標)","經BSI第三方查驗證",2023,"交通部高速公路局"]
[869,"瀝青混凝土","0274200009","kg",{"v":0.07,"d":"0.070"},"搖籃到大門","國道5號頭城交流道工程碳盤查","經BSI第三方查驗證",2019,"交通部高速公路局"]
[870,"開放級配瀝青混凝土(OGAC)","0274280005","t",{"v":89.21,"d":"89.210"},"搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證",2023,"交通部高速公路局"]
[871,"開放級配瀝青混凝土(OGAC)","0274280003","m3",{"v":196.25,"d":"196.250"},"搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證",2023,"交通部高速公路局"]
[872,"石膠泥瀝青混凝土(SmA)","0274300005","t",{"v":140.76,"d":"140.760"},"搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證","2023","交通部高速公路局"]
[873,"石膠泥瀝青混凝土(SmA)","0274300003","m3",{"v":327.14,"d":"327.140"},"搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證","2023","交通部高速公路局"]
[874,"石膠泥瀝青混凝土(SmA)","0274300005","t",{"v":143.83,"d":"143.830"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C713標)","經BSI第三方查驗證","2023","交通部高速公路局"]
[875,"石膠泥瀝青混凝土(SmA)","0274300005","t",{"v":147.73,"d":"147.730"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C714標)","經BSI第三方查驗證","2023","交通部高速公路局"]
[876,"密級配瀝青混凝土(DGAC)","0279600005","t","79.59","搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證",2023,"交通部高速公路局"]
[877,"密級配瀝青混凝土(DGAC)","0279600003","m3","188.64","搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證",2023,"交通部高速公路局"]
[878,"改質密級配瀝青混凝土\n(改質 DGAC)","0279600005","t",{"v":89.69,"d":"89.690"},"搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證",2023,"交通部高速公路局"]
[879,"改質密級配瀝青混凝土\n(改質 DGAC)","0279600003","m3",{"v":214.28,"d":"214.280"},"搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證",2023,"交通部高速公路局"]
[880,"密級配改質瀝青混凝土(改質 DGAC) ","0279600005","t",{"v":56.77,"d":"56.770"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C714標)","經BSI第三方查驗證",2023,"交通部高速公路局"]
[881,"密級配瀝青混凝土(3/4\"DGAC)","0279605005","t",{"v":77.39,"d":"77.390"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C713標)","經BSI第三方查驗證",2023,"交通部高速公路局"]
[882,"密級配瀝青混凝土(3/4\"DGAC) ","0279605005","t",{"v":77.65,"d":"77.650"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C714標)","經BSI第三方查驗證",2023,"交通部高速公路局"]
[883,"熱鑄膠泥瀝青混凝土\n(GUSS Asphalt)",null,"t",{"v":125.36,"d":"125.360"},"搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證","2023","交通部高速公路局"]
[884,"熱鑄膠泥瀝青混凝土\n(GUSS Asphalt)",null,"m3",{"v":298.1,"d":"298.100"},"搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證","2023","交通部高速公路局"]
[885,"熱鑄膠泥瀝青混凝土(GUSS) ",null,"t",{"v":122.41,"d":"122.410"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查 - 鴻運瀝青廠(C714標)","尚未認證","2023","交通部高速公路局"]
[886,"多孔隙瀝青混凝土(PAC)","0279800005","t",{"v":100.76,"d":"100.760"},"搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證","2023","交通部高速公路局"]
[887,"多孔隙瀝青混凝土(PAC)","0279800003","m3",{"v":200.2,"d":"200.200"},"搖籃到大門","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","尚未認證",2023,"交通部高速公路局"]
[888,"多孔隙瀝青混凝土(PAC)","0279800005","t",{"v":101.17,"d":"101.170"},"搖籃到大門","禾鑫瀝青廠","經BSI第三方查驗證","2023","交通部高速公路局"]
[889,"多孔隙瀝青混凝土(PAC)","0279800005","t",{"v":102.77,"d":"102.770"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C714標)","經BSI第三方查驗證","2023","交通部高速公路局"]
[890,"亞東 350 自充填混凝土 I 型","030504H103","m3",{"v":296.31,"d":"296.310"},"搖籃到大門","亞東混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[891,"卜特蘭水泥(乾式)","0305200009","kg",{"v":0.94,"d":"0.940"},"搖籃到大門","產品碳足跡資訊網",null,2014,"交通部高速公路局"]
[892,"水泥(不分型號)(亞泥 2019)","0305200009","kg",{"v":1.0348,"d":"1.035"},"搖籃到大門","亞泥查證聲明書",null,2020,"交通部高速公路局"]
[893,"卜特蘭 I 型水泥(晉瑜 2020) ","0305200009","kg",0.906,"搖籃到大門","晉瑜查證聲明書",null,2020,"交通部高速公路局"]
[894,"宜聯鋼筋","0321000009","kg",{"v":0.96,"d":"0.960"},"搖籃到大門","國道5號頭城交流道工程碳盤查-宜聯鋼鐵廠","經BSI第三方查驗證",2019,"交通部高速公路局"]
[895,"竹節鋼筋(不分類)","0321000009","kg",{"v":0.89,"d":"0.890"},"搖籃到大門","東和桃園廠查證聲明書",null,2021,"交通部高速公路局"]
[896,"竹節鋼筋(不分類)(豐興 2017) ","0321000009","kg",{"v":0.9074,"d":"0.907"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-豐興鋼鐵廠","經BSI第三方查驗證",2017,"交通部高速公路局"]
[897,"竹節鋼筋(不分類)(豐興 2018) ","0321000009","kg",{"v":0.9788,"d":"0.979"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-豐興鋼鐵廠","經BSI第三方查驗證",2018,"交通部高速公路局"]
[898,"竹節鋼筋(豐興 2019) ","0321000009","kg",{"v":0.8459,"d":"0.846"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-豐興鋼鐵廠","經BSI第三方查驗證",2019,"交通部高速公路局"]
[899,"竹節鋼筋(豐興，C714\n標運輸量加權平均)","0321000009","kg",{"v":0.8955,"d":"0.896"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-豐興鋼鐵廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[900,"竹節鋼筋，SD280W","0321040009","kg",0.667,"搖籃到大門","東和桃園廠查證聲明書",null,2019,"交通部高速公路局"]
[901,"竹節鋼筋，SD420W","0321060009","kg",0.667,"搖籃到大門","東和桃園廠查證聲明書",null,2019,"交通部高速公路局"]
[902,"廣達 80 混凝土 I 型","0331021103","m3",{"v":146.51,"d":"146.510"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-廣達混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[903,"甲騰 80 混凝土 I 型","0331021103","m3",{"v":144.75,"d":"144.750"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[904,"亞東 80 混凝土 I 型 ","0331021103","m3",{"v":149.77,"d":"149.770"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[905,"立泰混凝土，175kgf/cm2","0331024103","m3",{"v":237.68,"d":"237.680"},"搖籃到大門","國道5號頭城交流道工程碳盤查-立泰預拌混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[906,"廣達 175 混凝土 I 型 ","0331024103","m3",{"v":188.94,"d":"188.940"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-廣達混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[907,"甲騰 175 噴凝土 I 型 ","0331024103","m3",{"v":414.99,"d":"414.990"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[908,"甲騰 175 混凝土 I 型","0331024103","m3",{"v":187.39,"d":"187.390"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[909,"甲騰 175 低鹼混凝土 I 型",null,"t",{"v":189.44,"d":"189.440"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證","2023","交通部高速公路局"]
[910,"亞東 175 混凝土 I 型","0331024103","m3",{"v":187.38,"d":"187.380"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[911,"立泰混凝土，245kgf/cm2","0331026003","m3",{"v":289.24,"d":"289.240"},"規劃設計","國道5號頭城交流道工程碳盤查-立泰預拌混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[912,"甲騰 210 噴凝土 I 型 ","0337202003","m3",{"v":462.98,"d":"462.980"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[913,"甲騰 210 混凝土 I 型 ","0331025103","m3",{"v":463.34,"d":"463.340"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[914,"廣達 245 混凝土 I 型 ","0331026103","m3",{"v":243.27,"d":"243.270"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-廣達混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[915,"甲騰 245 混凝土 I 型 ","0331026103","m3",{"v":244.15,"d":"244.150"},"搖籃到大門","甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[916,"亞東 245 混凝土 I 型 ","0331026103","m3",{"v":241.42,"d":"241.420"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[917,"甲騰 255 鋼纖噴凝土 I 型","0337501003","m3",{"v":523.75,"d":"523.750"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[918,"立泰混凝土，280kgf/cm2","0331027003","m3",{"v":310.34,"d":"310.340"},"規劃設計","國道5號頭城交流道工程碳盤查-立泰預拌混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[919,"廣達280 混凝土 I 型 ","0331027103","m3",{"v":270.43,"d":"270.430"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-廣達混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[920,"甲騰280 混凝土 I 型 ","0331027103","m3",{"v":270.84,"d":"270.840"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[921,"亞東280 混凝土 I 型 ","0331027103","m3",{"v":262.92,"d":"262.920"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[922,"甲騰 280 低鹼混凝土 I 型 ",null,"m3",{"v":271.3,"d":"271.300"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證","2023","交通部高速公路局"]
[923,"廣達 315 水中混凝土 I 型","0331048103","m3",{"v":271.27,"d":"271.270"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-廣達混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[924,"甲騰 315 水中混凝土 I 型","0331048103","m3",{"v":281.06,"d":"281.060"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[925,"亞東 315 水中混凝土 I 型","0331048103","m3",{"v":265.14,"d":"265.140"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[926,"立泰混凝土，350kgf/cm2",331029003,"m3",{"v":359.64,"d":"359.640"},"搖籃到大門","國道5號頭城交流道工程碳盤查-立泰預拌混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[927,"廣達 350 自充填混凝土 I 型",331029003,"m3",{"v":311.96,"d":"311.960"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-廣達混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[928,"甲騰 350 自充填混凝土 I 型 ",331029003,"m3",{"v":323.88,"d":"323.880"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[929,"甲騰 350 低鹼填混凝土 I 型-1 ",null,"m3",{"v":279.85,"d":"279.850"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證","2023","交通部高速公路局"]
[930,"甲騰 350 低鹼填混凝土 I 型-2 ",null,"m3",{"v":309.82,"d":"309.820"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證","2023","交通部高速公路局"]
[931,"亞東 350 混凝土 I 型 ","0331029103","m3",{"v":296.53,"d":"296.530"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[932,"亞東 350 自充填混凝土 I 型","0331029103","m3",{"v":296.31,"d":"296.310"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[933,"混凝土(245)","0331026009","kg",{"v":247.75,"d":"247.750"},"規劃設計","蘇花改計畫施工期間工程碳管理委託服務工作成果","經BSI第三方查驗證",2023,"交通部高速公路局"]
[934,"立泰混凝土315(水中) ","0331048003","m3",{"v":342.01,"d":"342.010"},"搖籃到大門","國道5號頭城交流道工程碳盤查-立泰預拌混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[935,"甲騰420 無收縮混凝土I型 ","0337107003","m3",{"v":415.19,"d":"415.190"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[936,"甲騰 420 早強噴凝土 I 型",null,"m3",{"v":427.6,"d":"427.600"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[937,"亞東 420 混凝土 I 型 ","033102C103","m3",{"v":375.89,"d":"375.890"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[938,"亞東 420 早強混凝土 I 型",null,"m3",{"v":453.54,"d":"453.540"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","經BSI第三方查驗證","2023","交通部高速公路局"]
[939,"亞東 420 自充填混凝土 I 型",null,"m3",{"v":306.88,"d":"306.880"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","經BSI第三方查驗證","2023","交通部高速公路局"]
[940,"亞東420 無收縮混凝土 I 型","0337107003","m3",{"v":437.42,"d":"437.420"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[941,"CLSm","0337700013","m3",{"v":66.91,"d":"66.910"},"搖籃到大門","國道5號頭城交流道工程碳盤查","經BSI第三方查驗證",2019,"交通部高速公路局"]
[942,"型鋼(不分類)(豐興 2019)","0512000009","kg",{"v":0.9282,"d":"0.928"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-豐興鋼鐵廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[943,"鋼構(不分類)(中鋼構) ","0512000009","kg",{"v":3.0049,"d":"3.005"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-中鋼結構公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[944,"盤式支承(CC-GB300-225)(單向活動型，標稱載重300t，水平支承225t，無抗上揚力)","0582126408","組",{"v":1.18,"d":"1.180"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[945,"盤式支承(CC-GB350-250)(單向活動型，標稱載重350t，水平支承250t，無抗上揚力)","0582127508","組",{"v":1.28,"d":"1.280"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[946,"盤式支承(CC-GB400-300)(單向活動型，標稱載重400t，水平支承300t，無抗上揚力)","0582128608","組",{"v":1.45,"d":"1.450"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[947,"盤式支承(CC-GB500-225)(單向活動型，標稱載重500t，水平支承225t，無抗上揚力)","058212A408","組",{"v":1.74,"d":"1.740"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[948,"盤式支承(CC-GB500-400)(單向活動型，標稱載重500t，水平支承400t，無抗上揚力)","058212A808","組",{"v":2.29,"d":"2.290"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[949,"盤式支承(CC-GB600-400)(單向活動型，標稱載重600t，水平支承400t，無抗上揚力)","058212B808","組",{"v":2.61,"d":"2.610"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[950,"盤式支承(SC-FB450-475)(固定型，標稱載重450t，水平支承475t，無抗上揚力)","0582119908","組",{"v":1.74,"d":"1.740"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[951,"盤式支承(SC-FB450-650)(固定型，標稱載重450t，水平支承650t，無抗上揚力)","0582119B08","組",{"v":3.92,"d":"3.920"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[952,"盤式支承(SC-FB1600-700)(固定型，標稱載重1600t，水平支承700t，無抗上揚力)","058211mC08","組",{"v":7.96,"d":"7.960"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[953,"盤式支承(SC-FB1800-850)(固定型，標稱載重1800t，水平支承850t，無抗上揚力)","058211PD08","組",{"v":10.8,"d":"10.800"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[954,"盤式支承(SC-FB2200-800)(固定型，標稱載重2200t，水平支承800t，無抗上揚力)","058211tD08","組",{"v":10.51,"d":"10.510"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[955,"盤式支承(SC-GB450-325 )(單向活動型，標稱載重450t，水平支承800t，無抗上揚力)","0582129D08","組",{"v":1.94,"d":"1.940"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[956,"盤式支承(SC-GB1800-550)(單向活動型，標稱載重1800t，水平支承550t，無抗上揚力)","058212PA08","組",{"v":9.86,"d":"9.860"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[957,"盤式支承(SC-GB2300-550)(單向活動型，標稱載重2300t，水平支承550t，無抗上揚力)","058212UA08","組",{"v":12.64,"d":"12.640"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[958,"盤式支承(CC-FB400-450)(固定型，標稱載重400t，水平支承450t，無抗上揚力)","0582118908","組",{"v":2.57,"d":"2.570"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[959,"盤式支承(CC-FB700-300)(固定型，標稱載重700t，水平支承300t，無抗上揚力)","058211C608","組",{"v":3.33,"d":"3.330"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[960,"盤式支承(CC-FU350-445-100)(固定型，標稱載重350t，水平支承445t，抗上揚力100t)","0582117828","組",{"v":2.39,"d":"2.390"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[961,"盤式支承(CC-GB350-50 )(單向活動型，標稱載重350t，水平支承445t，無抗上揚力)","0582127808","組",{"v":0.85,"d":"0.850"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[962,"盤式支承(CC-GB350-175 )(單向活動型，標稱載重350t，水平支承175t，無抗上揚力)","0582127308","組",{"v":1.23,"d":"1.230"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[963,"盤式支承(CC-GB450-125)(單向活動型，標稱載重450t，水平支承125t，無抗上揚力)","0582129208","組",{"v":1.32,"d":"1.320"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[964,"盤式支承(CC-GB800-325)(單向活動型，標稱載重800t，水平支承325t，無抗上揚力)","058212D608","組",{"v":3.67,"d":"3.670"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[965,"盤式支承(CC-GU300-200-125)(單向活動型，標稱載重300t，水平支承200t，抗上揚力125t)","0582126428","組",{"v":1.52,"d":"1.520"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[966,"盤式支承(CC-GU350-100-24)(單向活動型，標稱載重350t，水平支承100t，抗上揚力24t)","0582127218","組",{"v":1.08,"d":"1.080"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[967,"盤式支承(CC-GU500-75-150)(單向活動型，標稱載重500t，水平支承75t，抗上揚力150t)","058212A128","組",{"v":1.7,"d":"1.700"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[968,"盤式支承(CC-SB1000)(雙向活動型，標稱載重1000t)","0582130008","組",{"v":2.78,"d":"2.780"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[969,"盤式支承(CC-GB400-600)(單向活動型，標稱載重400t，水平支承600t，無抗上揚力)","0582128B08","組",{"v":3.18,"d":"3.180"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[970,"盤式支承(CC-GB600-600)(單向活動型，標稱載重600t，水平支承600t，無抗上揚力)","058212BB08","組",{"v":3.4,"d":"3.400"},"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","經BSI第三方查驗證",2023,"交通部高速公路局"]
[971,"柴油（於鐵路運輸與非道路運輸移動源使用，2020）",null,"L",{"v":3.61,"d":"3.610"},"搖籃到大門","產品碳足跡資訊網",null,2022,"交通部高速公路局"]
[972,"柴油(於公路運輸移動源使用，2020)",null,"L",{"v":3.38,"d":"3.380"},"搖籃到大門","產品碳足跡資訊網",null,2022,"交通部高速公路局"]
[973,"柴油(於固定源使用，2020)",null,"L",{"v":3.34,"d":"3.340"},"搖籃到大門","產品碳足跡資訊網",null,2022,"交通部高速公路局"]
[974,"車用汽油(於移動源使用，2020)",null,"L",{"v":3.01,"d":"3.010"},"搖籃到大門","產品碳足跡資訊網",null,2022,"交通部高速公路局"]
[975,"車用汽油(於固定源使用，2020)",null,"L",{"v":2.93,"d":"2.930"},"搖籃到大門","產品碳足跡資訊網",null,2022,"交通部高速公路局"]
[976,"液化石油氣(於固定源使用，2020)",null,"L",{"v":2.22,"d":"2.220"},"搖籃到大門","產品碳足跡資訊網",null,2022,"交通部高速公路局"]
[977,"電力碳足跡(2020)",null,"度",{"v":0.59,"d":"0.590"},"搖籃到大門","產品碳足跡資訊網",null,2022,"交通部高速公路局"]
[978,"臺灣自來水(2020)",null,"m3",0.233,"搖籃到大門","產品碳足跡資訊網",null,2022,"交通部高速公路局"]
[979,"全拖車、大貨車(35t)",null,"tkm",0.14,"搖籃到大門","國5頭城交流道改善工程碳盤查","經BSI第三方查驗證",2019,"交通部高速公路局"]
[980,"營業大貨車(柴油)",null,"tkm",0.131,"搖籃到大門","產品碳足跡資訊網",null,2022,"交通部高速公路局"]
[981,"營業小貨車(柴油)",null,"tkm",0.587,"搖籃到大門","產品碳足跡資訊網",null,2022,"交通部高速公路局"]
[982,"傾卸卡車(21t、21.5t)",null,"m3km",0.337,"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-C713標","經BSI第三方查驗證",2023,"交通部高速公路局"]
[983,"傾卸卡車(21t)",null,"m3km",0.5413,"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-C714標","經BSI第三方查驗證",2023,"交通部高速公路局"]
[984,"傾卸卡車(21t)",null,"km",2.5388,"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-C714標","經BSI第三方查驗證",2023,"交通部高速公路局"]
[985,"混凝土運輸(甲騰)",null,"m3km",0.5819,"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-C713標","經BSI第三方查驗證",2023,"交通部高速公路局"]
[986,"混凝土運輸(廣達)",null,"m3km",0.5222,"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-C713標","經BSI第三方查驗證",2023,"交通部高速公路局"]
[987,"國際海運貨物運輸服務(燃料油動力)",null,"tkm",0.0198,"搖籃到大門","產品碳足跡資訊網",null,2016,"交通部高速公路局",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱"]
[988,"以柴油動力垃圾車清 除運輸一般廢棄物",null,"tkm",{"v":1.31,"d":"1.310"},"搖籃到大門","產品碳足跡資訊網",null,2018,"交通部高速公路局"]
[989,"廢棄物焚化處理服務(岡山垃圾焚化廠)",null,"公噸(mt)",{"v":360,"d":"360.000"},"搖籃到墳墓","產品碳足跡資訊網",null,2020,"交通部高速公路局",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱、宣告單位及係數"]
[990,"不鏽鋼(電弧爐製程， SS304)",null,"kg",{"v":2.01,"d":"2.010"},"搖籃到大門","產品碳足跡資訊網",null,2013,"交通部高速公路局"]
[991,"螺絲(不含球化、表面皮膜處理與電鍍)",null,"kg",{"v":3.37,"d":"3.370"},"搖籃到大門","產品碳足跡資訊網",null,2016,"交通部高速公路局"]
[992,"砂、石",null,"kg",0.0048,"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","經BSI第三方查驗證",2023,"交通部高速公路局"]
[993,"高爐石粉",null,"kg",0.0522,"搖籃到大門","中聯資源",null,2014,"交通部高速公路局"]
[994,"生石灰",null,"kg",{"v":1.25,"d":"1.250"},"搖籃到大門","產品碳足跡資訊網",null,2015,"交通部高速公路局"]
[995,"聚氨基甲酸乙酯樹脂",null,"kg",{"v":3.17,"d":"3.170"},"搖籃到大門","產品碳足跡資訊網",null,2015,"交通部高速公路局",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱"]
[996,"地工格網",null,"kg",4.3566,"搖籃到大門","國道4號臺中環線豐原潭子段工程碳盤查-盟鑫工業","經BSI第三方查驗證",2023,"交通部高速公路局"]
[997,"氧氣",null,"kg",{"v":0.16,"d":"0.160"},"搖籃到大門","產品碳足跡資訊網",null,2015,"交通部高速公路局"]
[998,"乙炔",null,"kg",{"v":6.08,"d":"6.080"},"搖籃到大門","產品碳足跡資訊網",null,2015,"交通部高速公路局"]
[999,"高密度聚乙烯(HDPE)",null,"kg",{"v":2.25,"d":"2.250"},"搖籃到大門","產品碳足跡資訊網",null,2015,"交通部高速公路局"]
[1000,"乙酸酐",null,"kg",{"v":2.69,"d":"2.690"},"搖籃到大門","產品碳足跡資訊網",null,2017,"交通部高速公路局"]
[1001,"鏡面無縫紙管",null,"kg",{"v":2.39,"d":"2.390"},"搖籃到大門","產品碳足跡資訊網",null,2018,"交通部高速公路局"]
[1002,"反應性黑色紡織染料(適用於浸染、連續染色＆冷壓染色，紙箱包裝)",null,"kg",{"v":14.5,"d":"14.500"},"搖籃到大門","產品碳足跡資訊網",null,2017,"交通部高速公路局",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱"]
[1003,"聚氯乙烯(膠膜，膠布，電線電纜用)",null,"kg",{"v":2.21,"d":"2.210"},"搖籃到大門","產品碳足跡資訊網",null,2013,"交通部高速公路局",{"$nulls":7},"非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             ","刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             "]
[1004,"環氧樹脂",null,"kg",{"v":3.02,"d":"3.020"},"搖籃到大門","產品碳足跡資訊網",null,2013,"交通部高速公路局"]
[1005,"電力碳足跡(2016)",null,"kwh",{"v":0.66,"d":"0.660"},"搖籃到大門","產品碳足跡資訊網",null,2018,"交通部高速公路局"]
[1006,"柴油(於固定源使用，2016)",null,"L",{"v":3.35,"d":"3.350"},"搖籃到大門","產品碳足跡資訊網",null,2018,"交通部高速公路局"]
[1007,"柴油(於公路運輸移動源使用，2016)",null,"L",{"v":3.38,"d":"3.380"},"搖籃到大門","產品碳足跡資訊網",null,2018,"交通部高速公路局",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱"]
[1008,"柴油（於鐵路運輸與非道路運輸移動源使用，2016）",null,"L",{"v":3.61,"d":"3.610"},"搖籃到大門","產品碳足跡資訊網",null,2018,"交通部高速公路局"]
[1009,"車用汽油(於固定源使用，2016)",null,"L",{"v":2.93,"d":"2.930"},"搖籃到大門","產品碳足跡資訊網",null,2018,"交通部高速公路局"]
[1010,"車用汽油(於移動源使用，2016)",null,"L",{"v":3.01,"d":"3.010"},"搖籃到大門","產品碳足跡資訊網",null,2018,"交通部高速公路局"]
[1011,"液化石油氣(於固定源使用，2015)",null,"L",{"v":2.26,"d":"2.260"},"搖籃到大門","產品碳足跡資訊網",null,2017,"交通部高速公路局"]
[1012,"臺北自來水(2013)",null,"m3",{"v":0.17,"d":"0.170"},"搖籃到大門","產品碳足跡資訊網",null,2014,"交通部高速公路局"]
[1013,"卜特蘭水泥(乾式)",null,"kg",{"v":0.94,"d":"0.940"},"搖籃到大門","產品碳足跡資訊網",null,2014,"交通部高速公路局"]
[1014,"生石灰",null,"kg",{"v":1.25,"d":"1.250"},"搖籃到大門","產品碳足跡資訊網",null,2015,"交通部高速公路局"]
[1015,"飛灰爐石粉(太空包裝)",null,"mt",{"v":52.5,"d":"52.500"},"搖籃到大門","產品碳足跡資訊網",null,2016,"交通部高速公路局",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱、宣告單位及係數"]
[1016,"土方",null,"m3",8.65,"搖籃到大門","國道5號頭城交流道工程碳盤查","經BSI第三方查驗證",2019,"交通部高速公路局"]
[1017,"R45",null,"m3",434.19,"搖籃到大門","國道5號頭城交流道工程碳盤查-宜聯鋼鐵廠","經BSI第三方查驗證",2019,"交通部高速公路局"]
[1018,"玻璃纖維絲",null,"kg",{"v":2.76,"d":"2.760"},"搖籃到大門","產品碳足跡資訊網",null,2014,"交通部高速公路局"]
[1019,"不飽和聚酯樹脂",null,"kg",{"v":5.5,"d":"5.500"},"搖籃到大門","產品碳足跡資訊網",null,2017,"交通部高速公路局"]
[1020,"乙炔",null,"kg",{"v":6.08,"d":"6.080"},"搖籃到大門","產品碳足跡資訊網",null,2015,"交通部高速公路局"]
[1021," 高密度聚乙烯(HDPE)",null,"kg",{"v":2.25,"d":"2.250"},"搖籃到大門","產品碳足跡資訊網",null,2015,"交通部高速公路局"]
[1022,"A2 標宜興 175II, A2-1-175II",null,"kg",171.23,"搖籃到大門","國道5號頭城交流道工程碳盤查","經BSI第三方查驗證",2019,"交通部高速公路局"]
[1023,"瀝青混凝土",null,"kg",0.07,"搖籃到大門","國道5號頭城交流道工程碳盤查","經BSI第三方查驗證",2019,"交通部高速公路局"]
[1024,"混凝土預拌車",null,"m3 -km",0.66,"搖籃到大門","國道5號頭城交流道工程碳盤查","經BSI第三方查驗證",2019,"交通部高速公路局"]
[1025,"土方及塊石運輸",null,"tkm",0.14,"搖籃到大門","國道5號頭城交流道工程碳盤查","經BSI第三方查驗證",2019,"交通部高速公路局"]
[1026,"營業大貨車(柴油)",null,"tkm",0.235,"搖籃到大門","產品碳足跡資訊網",null,2014,"交通部高速公路局"]
[1027,"營業小貨車(柴油)",null,"tkm",0.647,"搖籃到大門","產品碳足跡資訊網",null,2014,"交通部高速公路局"]
[1028,"3.49噸常溫貨車服務(裝載率84％，包含營業據點排放)",null,"tkm",0.833,"搖籃到墳墓","產品碳足跡資訊網",null,2017,"交通部高速公路局",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱"]
[1029,"廢棄物焚化處理服務(苗栗縣垃圾焚化廠)",null,"kg",{"v":0.34,"d":"0.340"},"搖籃到墳墓","產品碳足跡資訊網",null,2018,"交通部高速公路局",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱及碳足跡"]
[1030,"廢棄物焚化處理服務(臺南市城西垃圾焚化廠)",null,"kg",{"v":0.33,"d":"0.330"},"搖籃到墳墓","產品碳足跡資訊網",null,2017,"交通部高速公路局",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱及碳足跡"]
[1031,"廢棄物焚化處理服務(臺南市城西垃圾焚化廠)",null,"kg",{"v":0.33,"d":"0.330"},"搖籃到墳墓","產品碳足跡資訊網",null,2017,"交通部高速公路局",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱及碳足跡"]
[1032,"密級配瀝青混凝土 (混和料比例 2.9%)","0274290009","kg",0.129,null,"公路總局西部濱海公路南區臨時工程處","尚未認證",2020,"交通部鐵道局中部工程分局"]
[1033,"鋼筋混凝土用鋼筋 (SD280W)","0321040009","kg",0.835,null,"公路總局西部濱海公路南區臨時工程處",null,2020,"交通部鐵道局中部工程分局"]
[1034,"鋼筋混凝土用鋼筋 (SD420W)","0321060009","kg",0.834,null,"公路總局西部濱海公路南區臨時工程處",null,2020,"交通部鐵道局中部工程分局"]
[1035,"預拌混凝土(210 kgf/cm2 )","0331025003","m3",{"v":238,"d":"238.000"},null,"公路總局西部濱海公路南區臨時工程處",null,2020,"交通部鐵道局中部工程分局"]
[1036,"預拌混凝土(140 kgf/cm2 )","0331023003","m3",200,null,"公路總局西部濱海公路南區臨時工程處",null,2020,"交通部鐵道局中部工程分局"]
[1037,"預拌混凝土(210 kgf/cm2 )","0331025003","m3",238,null,"公路總局西部濱海公路南區臨時工程處",null,2020,"交通部鐵道局中部工程分局"]
[1038,"預拌混凝土(280 kgf/cm2 )","0331027003","m3",338,null,"公路總局西部濱海公路南區臨時工程處",null,2020,"交通部鐵道局中部工程分局"]
[1039,"無收縮混凝土(420kgf/cm2)","0331027003","m3",493,null,"公路總局西部濱海公路南區臨時工程處",null,2019,"交通部鐵道局中部工程分局"]
[1040,"水泥砂漿粉刷(1:3)","0922030002","m2",9.83,"搖籃到大門","產品碳足跡資訊網",null,2015," 交通部鐵道局中部工程分局",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正產品名稱及碳足跡"]
[1041,"鋼筋，SD420W",null,"kg",0.901,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1042,"鋼筋，SD280",null,"kg",0.874,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1043,"結構用混凝土，預 拌，420kgf/cm2",null,"m3",424,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1044,"結構用混凝土，預 拌，280kgf/cm2",null,"m3",237,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1045,"結構用混凝土，預 拌，80kgf/cm2",null,"m3",207,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1046,"預力鋼腱",null,"kg",3.2,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1047,"密級配瀝青混凝土",null,"kg",0.129,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1048,"接地扁鋼條",null,"kg",1.296,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1049,"不銹鋼欄杆及扶手",null,"kg",1.75,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1050,"鍍鋅格柵板",null,"kg",3.16,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1051,"鋼軌",null,"kg",0.947,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1052,"防振橡膠墊",null,"kg",3.04,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1053,"彈性 PC 軌枕",null,"支",42,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1054,"碎石道碴",null,"kg",0.006,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1055,"固定式圍籬",null,"公尺",3.16,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1056,"鐵絲網柵欄",null,"公尺",0.9,null,"鐵道局南部工程分局-南迴計畫碳管理暨碳\n足跡盤查服務報告",null,2020," 交通部鐵道局中部工程分局"]
[1057,"鋼胚(電弧爐製程， 不分型號)",null,"kg",0.678,null,"公路總局蘇花公路改善工程處",null,2017," 交通部鐵道局中部工程分局"]
[1058,"變性環氧",null,"加侖",{"v":21.17,"d":"21.170"},null,"南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","經BSI第三方查驗證",2022,"交通部鐵道局南部工程分局"]
[1059,"鋼胚(電弧爐製程， 不分型號)",null,"kg",0.678,null,"公路總局蘇花公路改善工程處",null,2017,"交通部鐵道局南部工程分局"]
[1060,"門窗鋁框",null,"m2",{"v":14.4,"d":"14.400"},"搖籃到大門","產品碳足跡資訊網",null,2015,"交通部鐵道局南部工程分局",{"$nulls":7},"1.建議修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          2.建議修正數據來源","1.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                             2.修正數據來源"]
[1061,"纖維水泥板/矽酸鈣板",null,"kg",{"v":1.12,"d":"1.120"},"搖籃到大門","產品碳足跡資訊網",null,2014,"交通部鐵道局南部工程分局",{"$nulls":7},"1.建議修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          2.建議修正數據來源","1.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                             2.修正數據來源"]
[1062,"不鏽鋼 (電弧爐製程，SS304)",null,"kg",{"v":2.01,"d":"2.010"},null,"經濟部產業發展署",null,null,"交通部鐵道局南部工程分局"]
[1063,"石質地磚",null,"kg",{"v":4.5,"d":"4.500"},null,"宏洲窯業股份有限公司",null,2015,"交通部鐵道局南部工程分局"]
[1064,"磨石子地磚，30cm*30cm*2cm",null,"片",{"v":1.7,"d":"1.700"},null,"晶泰水泥加工廠股份有限公司",null,2016,"交通部鐵道局南部工程分局"]
[1065,"再生高壓透水混凝土 地磚 (20cm*20cm*6cm)",null,"片",{"v":1.18,"d":"1.180"},null,"健源有限公司",null,2020,"交通部鐵道局南部工程分局"]
[1066,"輕質骨材混凝土 (175kgf/cm2 )",null,"m3",{"v":317,"d":"317.000"},null,"公路總局西部濱海公路南區臨時工程處",null,2019,"交通部鐵道局南部工程分局"]
[1067,"B 型∮600 ㎜膠圈",null,"條",{"v":3.04,"d":"3.040"},null,"南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","經BSI第三方查驗證",2022,"交通部鐵道局南部工程分局"]
[1068,"變性環氧",null,"加侖",{"v":21.17,"d":"21.170"},null,"南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","經BSI第三方查驗證",2022,"交通部鐵道局南部工程分局"]
[1069,"鋼胚(電弧爐製程， 不分型號)",null,"kg",0.678,null,"公路總局蘇花公路改善工程處",null,2017,"交通部鐵道局南部工程分局"]
[1070,"門窗鋁框",null,"m2",{"v":14.4,"d":"14.400"},"搖籃到大門","產品碳足跡資訊網",null,2015,"交通部鐵道局南部工程分局",{"$nulls":7},"1.建議修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          2.建議修正數據來源","1.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                             2.修正數據來源"]
[1071,"纖維水泥板/矽酸鈣板",null,"kg",{"v":1.12,"d":"1.120"},"搖籃到大門","產品碳足跡資訊網",null,2014,"交通部鐵道局南部工程分局",{"$nulls":7},"1.建議修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          2.建議修正數據來源","1.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                             2.修正數據來源"]
[1072,"不鏽鋼 (電弧爐製程，SS304)",null,"kg",{"v":2.01,"d":"2.010"},null,"經濟部產業發展署",null,null,"交通部鐵道局南部工程分局"]
[1073,"石質地磚",null,"kg",{"v":4.5,"d":"4.500"},null,"宏洲窯業股份有限公司",null,2015,"交通部鐵道局南部工程分局"]
[1074,"磨石子地磚，30cm*30cm*2cm",null,"片",{"v":1.7,"d":"1.700"},null,"晶泰水泥加工廠股份有限公司",null,2016,"交通部鐵道局南部工程分局"]
[1075,"再生高壓透水混凝土 地磚 (20cm*20cm*6cm)",null,"片",{"v":1.18,"d":"1.180"},null,"健源有限公司",null,2020,"交通部鐵道局南部工程分局"]
[1076,"輕質骨材混凝土 (175kgf/cm2 )",null,"m3",{"v":317,"d":"317.000"},null,"公路總局西部濱海公路南區臨時工程處",null,2019,"交通部鐵道局南部工程分局"]
[1077,"50N 鋼軌",null,"支",0.947,null,"2014年本團隊東和鋼鐵高雄廠實際盤查"]
[1078,"清除及掘除","0223100003","m3",1.325,"規劃設計","水土保持工程減碳參考指引","經BSI第三方查驗證",2022,"國防部"]
[1079,"臨時擋土樁設施，打拔(不分類)","0225500031","m",0.483,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部"]
[1080,"土方工作，挖方","02300C0003","m3",0.981,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.修正產品名稱                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                                 3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      4.修正查驗單位                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    5.修正公告年分"]
[1081,"土方工作，回填方","02300F0003","m3",0.736,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.修正產品名稱                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                                 3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      4.修正查驗單位                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    5.修正公告年分"]
[1082,"土方工作，回填方","02300F0003","m3",0.736,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.修正產品名稱                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                                 3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      4.修正查驗單位                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    5.修正公告年分"]
[1083,"構造物開挖，機械挖","0231600703","m3",1.325,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部"]
[1084,"排水管涵，鋼筋混凝土管(不分類)","0261020001","m",{"v":205.49,"d":"205.490"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部"]
[1085,"級配粒料底層，碎石級配，鋪設及滾壓","0272610053","m3",{"v":5.74,"d":"5.740"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部"]
[1086,"瀝青混凝土鋪面，厚10cm","027420J002","m2",21.133,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部"]
[1087,"瀝青混凝土面層刨除(不分類，厚5cm)","0296100002","m2",2.094,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部"]
[1088,"場鑄結構混凝土用模板，普通模板，建築","0311011502","m2",1.202,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.修正產品名稱                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                                 3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      4.修正查驗單位                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    5.修正公告年分"]
[1089,"場鑄結構混凝土用模板，清水模板","0311020002","m2",1.204,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.修正產品名稱                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                                 3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      4.修正查驗單位                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    5.修正公告年分"]
[1090,"鋼筋，SD280W，連工帶料","0321030075","t",{"v":893.62,"d":"893.620"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.修正產品名稱                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                                 3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      4.修正查驗單位                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    5.修正公告年分"]
[1091,"鋼筋，SD420W，連工帶料","0321050075","t",{"v":892.56,"d":"892.560"},"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.修正產品名稱                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                                 3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      4.修正查驗單位                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    5.修正公告年分"]
[1092,"銲接鋼線網，線徑10mm，方孔20x20cm","0322006182","m2",5.152,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部"]
[1093,"結構用混凝土，預拌，140kgf/cm2","0331023003","m3",304.785,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.修正產品名稱                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                                 3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      4.修正查驗單位                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    5.修正公告年分"]
[1094,"預拌混凝土(2000psi)","0331023003","m3",{"v":255,"d":"255.000"},"搖籃到大門","產品碳足跡資訊網",null,2015,"國防部",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.修正產品名稱                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                                 3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      4.刪除國家公告係數                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    5.修正公告年分"]
[1095,"結構用混凝土，預拌，280kgf/cm2","0331027003","m3",433.785,"規劃設計","水利工程減碳作業參考指引","經BSI第三方查驗證",2022,"國防部",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.非本部公告之係數","1.修正產品名稱                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                                 3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      4.修正查驗單位                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    5.修正公告年分"]
[1096,"單結晶矽電池BIPV鋼板太陽光電模組(24片6吋)",null,"片",{"v":182,"d":"182.000"},"搖籃到大門","產品碳足跡資訊網",null,2022,"台糖公司",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.建議修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          3.建議修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                        4.建議修正公告年分","1.刪除國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                        4.修正公告年分"]
[1097,"多結晶矽電池太陽光電模組(72片6吋)",null,"片",{"v":336,"d":"336.000"},"搖籃到大門","產品碳足跡資訊網",null,2020,"台糖公司",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.建議修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          3.建議修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                        4.建議修正公告年分","1.刪除國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                        4.修正公告年分"]
[1098,"單結晶矽電池太陽光電模組(72片6吋)",null,"片",{"v":465,"d":"465.000"},"搖籃到大門","產品碳足跡資訊網",null,2020,"台糖公司",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.建議修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          3.建議修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                        4.建議修正公告年分","1.刪除國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                        4.修正公告年分"]
[1099,"多結晶矽電池太陽光電模組(60片6吋)",null,"片",{"v":320,"d":"320.000"},"搖籃到大門","產品碳足跡資訊網",null,2019,"台糖公司",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.建議修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          3.建議修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                        4.建議修正公告年分","1.刪除國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                        4.修正公告年分"]
[1100,"單結晶矽電池太陽光電模組(60片6吋)",null,"片",{"v":418,"d":"418.000"},"搖籃到大門","產品碳足跡資訊網",null,2019,"台糖公司",{"$nulls":7},"1.非國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.建議修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          3.建議修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                        4.建議修正公告年分","1.刪除國家公告之係數                                                                                                                                                                                                                                                                                                                                                                                                             2.修正碳足跡                                                                                                                                                                                                                                                                                                                                                                                                          3.修正數據來源                                                                                                                                                                                                                                                                                                                                                                                                        4.修正公告年分"]
[1101,"結構用混凝土，280kgf/cm2，含澆置","0331027003","m3",{"v":401.33,"d":"401.330"},null,"永續綠色工程資訊網","尚未認證",null,"臺中市政府"]
[1102,"控制性低強度回填材料(CLSm)",null,"m3",76.985,"搖籃到大門","全興資源再生股份有限公司","經Afnor第三方查驗證",2023,"臺南市政府"]