{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["公共工程碳排放係數資料總表","公共工程碳排放係數資料"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"公共工程碳排放係數資料總表","index":0,"n_rows":10,"n_cols":12,"rows_kept":10,"merged":[[0,0,0,12],[1,1,1,3],[1,4,1,6],[1,7,1,9],[1,10,1,12],[2,1,2,3],[2,4,2,6],[2,7,2,9],[2,10,2,12],[3,1,3,12],[5,1,5,3],[5,4,5,6],[7,1,7,12],[8,1,8,12],[9,1,9,12]]}
["公共工程碳排放係數資料總表"]
["項目","油水電類",null,null,"材料類",null,null,"機具類",null,null,"工項類"]
["數量",35,null,null,545,549,null,198,191,null,1272,1273]
["總計",{"$f":"B3+E3+H3+K3","v":2050}]
[]
[]
["備註："]
[1,"公共工程碳排放係數資料，係供工程機關進行碳排放量初步估算與減碳策略研擬之參考工具。"]
[2,"本表部分碳排放係數之原始資料欄位未臻完整，係依原提供資料如實彙整，未另行補值、推估或作任何假設。"]
[3,"使用本資料時，應注意各係數所對應之盤查範疇、適用年分及使用條件；相關應用應先參考資料來源所界定之適用範圍，避免不當延伸使用。"]

{"sheet":"公共工程碳排放係數資料","index":1,"n_rows":2051,"n_cols":11,"rows_kept":2051}
["編號","類別","項目名稱","生命週期範疇","公告年分","宣告單位","碳排放係數","查驗狀態","資料來源","提報單位","對應篇章"]
[1,"油水電類","柴油(於固定源使用，2016)","搖籃到大門",2018,"L",{"v":3.35,"d":"3.350"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[2,"油水電類","柴油(於公路運輸移動源使用，2016)","搖籃到大門",2018,"L",{"v":3.38,"d":"3.380"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[3,"油水電類","柴油（於鐵路運輸與非道路運輸移動源使用，2016）","搖籃到大門",2018,"L",{"v":3.61,"d":"3.610"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[4,"油水電類","車用汽油(於固定源使用，2016)","搖籃到大門",2018,"L",{"v":2.93,"d":"2.930"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[5,"油水電類","車用汽油(於移動源使用，2016)","搖籃到大門",2018,"L",{"v":3.01,"d":"3.010"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[6,"油水電類","柴油（於鐵路運輸與非道路運輸移動源使用，2020）","搖籃到大門",2022,"L",{"v":3.61,"d":"3.610"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[7,"油水電類","柴油(於公路運輸移動源使用，2020)","搖籃到大門",2022,"L",{"v":3.38,"d":"3.380"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[8,"油水電類","柴油(於固定源使用，2020)","搖籃到大門",2022,"L",{"v":3.34,"d":"3.340"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[9,"油水電類","車用汽油(於移動源使用，2020)","搖籃到大門",2022,"L",{"v":3.01,"d":"3.010"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[10,"油水電類","車用汽油(於固定源使用，2020)","搖籃到大門",2022,"L",{"v":2.93,"d":"2.930"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[11,"油水電類","基本產品需求，燃料油，(蒸餘油/重油使用)","搖籃到大門",2025,"L",{"v":3.88,"d":"3.880"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[12,"油水電類","基本產品需求，燃料油，(蒸餘油/重油未燃燒)","搖籃到大門",2025,"L",0.764,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[13,"油水電類","基本產品需求，柴油，未燃燒【不分類】","搖籃到大門",2025,"L",0.673,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[14,"油水電類","液化石油氣(於固定源使用，2015)","搖籃到大門",2017,"L",{"v":2.26,"d":"2.260"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[15,"油水電類","液化石油氣(於固定源使用，2020)","搖籃到大門",2022,"L",{"v":2.22,"d":"2.220"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[16,"油水電類","電力碳足跡(2020)","搖籃到大門",2022,"度",{"v":0.59,"d":"0.590"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[17,"油水電類","電力碳足跡(2016)","搖籃到大門",2018,"kwh",{"v":0.66,"d":"0.660"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[18,"油水電類","臺灣自來水(2020)","搖籃到大門",2022,"m3",0.233,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[19,"油水電類","臺北自來水(2013)","搖籃到大門",2014,"m3",{"v":0.17,"d":"0.170"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[20,"油水電類","廢棄物焚化處理服務(岡山垃圾焚化廠)","搖籃到墳墓",2020,"公噸(mt)",{"v":360,"d":"360.000"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[21,"油水電類","廢棄物焚化處理服務(苗栗縣垃圾焚化廠)","搖籃到墳墓",2018,"kg",{"v":0.34,"d":"0.340"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[22,"油水電類","廢棄物焚化處理服務(臺南市城西垃圾焚化廠)","搖籃到墳墓",2017,"kg",{"v":0.33,"d":"0.330"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[23,"油水電類","CH4排放係數(人員 化糞池排放源)","未載明",2019,"人時",{"v":0.0398,"d":"0.040"},"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[24,"油水電類","一般廢棄物處置排放 係數(人員)","未載明",2019,"人時",0.504,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[25,"油水電類","廢棄物運離工地及棄置，一般廢棄物清運處理費，【含施工】","搖籃到大門",2025,"M3",36.737,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[26,"油水電類","單結晶矽電池BIPV鋼板太陽光電模組(24片6吋)","搖籃到大門",2022,"片",{"v":182,"d":"182.000"},"未載明","產品碳足跡資訊網","台糖公司"]
[27,"油水電類","多結晶矽電池太陽光電模組(72片6吋)","搖籃到大門",2020,"片",{"v":336,"d":"336.000"},"未載明","產品碳足跡資訊網","台糖公司"]
[28,"油水電類","單結晶矽電池太陽光電模組(72片6吋)","搖籃到大門",2020,"片",{"v":465,"d":"465.000"},"未載明","產品碳足跡資訊網","台糖公司"]
[29,"油水電類","多結晶矽電池太陽光電模組(60片6吋)","搖籃到大門",2019,"片",{"v":320,"d":"320.000"},"未載明","產品碳足跡資訊網","台糖公司"]
[30,"油水電類","單結晶矽電池太陽光電模組(60片6吋)","搖籃到大門",2019,"片",{"v":418,"d":"418.000"},"未載明","產品碳足跡資訊網","台糖公司"]
[31,"油水電類","氧氣","搖籃到大門",2015,"kg",{"v":0.16,"d":"0.160"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[32,"油水電類","乙炔","搖籃到大門",2015,"kg",{"v":6.08,"d":"6.080"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[33,"油水電類","乙酸酐","搖籃到大門",2017,"kg",{"v":2.69,"d":"2.690"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[34,"油水電類","鏡面無縫紙管","搖籃到大門",2018,"kg",{"v":2.39,"d":"2.390"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[35,"油水電類","反應性黑色紡織染料(適用於浸染、連續染色＆冷壓染色，紙箱包裝)","搖籃到大門",2017,"kg",{"v":14.5,"d":"14.500"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[36,"材料類","粒料，粗粒料","未載明","未載明","m3",{"v":6.518087631,"d":"6.518"},"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署"]
[37,"材料類","混凝土基本材料及施工方法\n粒料，細粒料","未載明","未載明","m3",{"v":7.49131879,"d":"7.491"},"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署"]
[38,"材料類","粒料\n細粒料(細砂，粉光用)","未載明","未載明","m3",{"v":9.4890038,"d":"9.489"},"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署"]
[39,"材料類","砂、石","搖籃到大門",2023,"kg",0.0048,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局"]
[40,"材料類","水泥(不分型號)","搖籃到工地",2017,"kg",0.907,"未載明","產品碳足跡資訊網","內政部建築研究所","03052"]
[41,"材料類","一般水泥(卜特蘭)","搖籃到工地",2017,"t",{"v":881.59,"d":"881.590"},"未載明","低碳建築聯盟","內政部建築研究所","03052"]
[42,"材料類","卜特蘭水泥(I型) ","搖籃到工地",2017,"kg",0.944,"未載明","低碳建築聯盟","內政部建築研究所","03052"]
[43,"材料類","卜特蘭水泥(II型) ","搖籃到工地",2023,"kg",0.968,"未載明","低碳建築聯盟","內政部建築研究所","03052"]
[44,"材料類","白水泥","搖籃到工地",2017,"t",{"v":968.4,"d":"968.400"},"未載明","低碳建築聯盟","內政部建築研究所","03052"]
[45,"材料類","高爐水泥(爐石粉 30%)","搖籃到工地",2017,"t",{"v":657.16,"d":"657.160"},"未載明","低碳建築聯盟","內政部建築研究所","03052"]
[46,"材料類","高爐水泥(爐石粉 45%)","搖籃到工地",2017,"t",{"v":534.35,"d":"534.350"},"未載明","低碳建築聯盟","內政部建築研究所","03052"]
[47,"材料類","水泥","未載明",2019,"kg",0.96,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03052"]
[48,"材料類","卜特蘭水泥(乾式)","搖籃到大門",2014,"kg",{"v":0.94,"d":"0.940"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局","03052"]
[49,"材料類","水泥(不分型號)(亞泥 2019)","搖籃到大門",2020,"kg",{"v":1.0348,"d":"1.035"},"經BSI第三方查驗證","亞泥查證聲明書","交通部高速公路局","03052"]
[50,"材料類","卜特蘭 I 型水泥(晉瑜 2020) ","搖籃到大門",2020,"kg",0.906,"經BSI第三方查驗證","晉瑜查證聲明書","交通部高速公路局","03052"]
[51,"材料類","卜特蘭水泥，第 2 型水泥，袋裝 ，【1包40kg】","搖籃到大門",2025,"包",39.24,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03052"]
[52,"材料類","卜特蘭水泥，第 1 型水泥","搖籃到大門",2025,"KG",0.944,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03052"]
[53,"材料類","卜特蘭水泥，第 1 型水泥，袋裝 ，【1 包40kg】","搖籃到大門",2025,"包",37.76,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03052"]
[54,"材料類","卜特蘭水泥，第 2 型水泥","搖籃到大門",2025,"KG",0.981,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03052"]
[55,"材料類","產品，鋼筋，SD280，D16mm","未載明",2022,"T",893.62,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03210"]
[56,"材料類","產品，鋼筋，SD420W，D19mm","未載明",2022,"T",892.56,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03210"]
[57,"材料類","產品，鋼筋，SD420W，D22mm","未載明",2022,"T",892.56,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03210"]
[58,"材料類","產品，鋼筋，SD280(含運費)","未載明",2022,"KG",0.89362,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03210"]
[59,"材料類","產品，預拌混凝土材料費，140kgf/cm2，第1 型水泥","搖籃到大門",2022,"M3",304.785,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03050"]
[60,"材料類","產品，預拌混凝土材料費，210kgf/cm2，第1 型水泥","搖籃到大門",2022,"M3",384.285,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03050"]
[61,"材料類","產品，預拌混凝土材料費，（140kgf/cm2，水中用），第1型水泥","未載明",2022,"M3",274.4203130489,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03050"]
[62,"材料類","產品，預拌混凝土材料費，（210kgf/cm2， 水中用），第1型水泥","未載明",2022,"M3",346,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03050"]
[63,"材料類","產品，控制性低強度回填材料","未載明",2022,"M3",94.495,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03377"]
[64,"材料類","產品，控制性低強度回填材料，再生粒料","搖籃到大門",2022,"M3",76.485926,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03377"]
[65,"材料類","水泥混凝土舖面，抗壓210 kgf/cm2，t=10cm","未載明",2022,"M3",321.285,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02751"]
[66,"材料類","結構用混凝土，人工拌合，(樹脂水泥基座)","未載明",2022,"M3",387.629,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","03310"]
[67,"材料類","產品，預拌混凝土材料費，140kgf/cm2，第1 型水泥","搖籃到大門",2022,"M3",304.785,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03050"]
[68,"材料類","產品，預拌混凝土材料費，175kgf/cm2，第1 型水泥","搖籃到大門",2022,"M3",344.288,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03050"]
[69,"材料類","產品，預拌混凝土材料費，210kgf/cm2，第1 型水泥","搖籃到大門",2022,"M3",384.285,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03050"]
[70,"材料類","產品，預拌混凝土材料費，140kgf/cm2","搖籃到大門",2022,"M3",304.785,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03050"]
[71,"材料類","產品，預拌混凝土材料費，280kgf/cm2","搖籃到大門",2022,"M3",433.785,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03050"]
[72,"材料類","產品，高流動性無收縮水泥砂漿，抗壓強 度420kgf/cm2","未載明",2002,"M3",952,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03050"]
[73,"材料類","產品，普通模板","未載明",2022,"M2",1.202,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M03110"]
[74,"材料類","高鍍鋅鐵線(5mm)","未載明",2019,"kg",0.63,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[75,"材料類","熱浸鍍鋅格柵板","未載明",2019,"kg",2.31,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","05330"]
[76,"材料類","預力鋼絞線(15.2mm)","未載明",2019,"kg",2.16,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[77,"材料類","強力螺栓","未載明",2019,"kg",2.25,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[78,"材料類","剪力釘","未載明",2019,"kg",2.25,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[79,"材料類","預力鋼絞線(12.7mm)","未載明",2019,"kg",2.16,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[80,"材料類","點焊鋼線網 (5*100*100mm)","未載明",2019,"kg",0.63,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[81,"材料類","鋼管","未載明",2019,"kg",2.46,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[82,"材料類","鐵板","未載明",2019,"kg",1.95,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[83,"材料類","鍍鋅承壓板 (300*300*40mm)","未載明",2019,"kg",1.95,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[84,"材料類","管幕鋼管、先撐鋼管","未載明",2019,"kg",2.46,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[85,"材料類","油漆","未載明",2019,"kg",2.45,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","09910"]
[86,"材料類","乳膠漆","未載明",2019,"kg",2.45,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","09910"]
[87,"材料類","16CH 矩陣式多工數位主機","未載明",2022,"套",220,"經BSI第三方查驗證","南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","交通部公路局"]
[88,"材料類","防眩板","未載明",2019,"kg",2.13,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[89,"材料類","預力套管","未載明",2019,"kg",2.47,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[90,"材料類","續接器","未載明",2019,"kg",2.31,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[91,"材料類","免拆網","未載明",2019,"kg",0.63,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[92,"材料類","保麗龍","未載明",2019,"kg",2.84,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[93,"材料類","路緣石","未載明",2019,"kg",0.93,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[94,"材料類","人孔鑄鐵蓋","未載明",2019,"kg",2.25,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[95,"材料類","防震拉條","未載明",2019,"kg",0.81,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[96,"材料類","橋面洩水孔","未載明",2019,"kg",2.31,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[97,"材料類","波型鋼版","未載明",2019,"kg",1.95,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[98,"材料類","不鏽鋼(電弧爐製程， SS304)","搖籃到大門",2013,"kg",2.01,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[99,"材料類","螺絲(不含球化、表面皮膜處理與電鍍)","搖籃到大門",2016,"kg",3.37,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[100,"材料類","高爐石粉","搖籃到大門",2014,"kg",0.0522,"經BSI第三方查驗證","中聯資源","交通部高速公路局"]
[101,"材料類","生石灰","搖籃到大門",2015,"kg",1.25,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[102,"材料類","聚氨基甲酸乙酯樹脂","搖籃到大門",2015,"kg",3.17,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[103,"材料類","高密度聚乙烯(HDPE)","搖籃到大門",2015,"kg",2.25,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[104,"材料類","聚氯乙烯(膠膜，膠布，電線電纜用)","搖籃到大門",2013,"kg",2.21,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[105,"材料類","環氧樹脂","搖籃到大門",2013,"kg",3.02,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[106,"材料類","飛灰爐石粉(太空包裝)","搖籃到大門",2016,"mt",52.5,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[107,"材料類","R45","搖籃到大門",2019,"m3",434.19,"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查-宜聯鋼鐵廠","交通部高速公路局"]
[108,"材料類","玻璃纖維絲","搖籃到大門",2014,"kg",2.76,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[109,"材料類","不飽和聚酯樹脂","搖籃到大門",2017,"kg",5.5,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[110,"材料類","A2 標宜興 175II, A2-1-175II","搖籃到大門",2019,"kg",171.23,"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查","交通部高速公路局"]
[111,"材料類","接地扁鋼條","未載明",2020,"kg",1.296,"未載明","鐵道局南部工程分局-南迴計畫碳管理暨碳足跡盤查服務報告"," 交通部鐵道局中部工程分局"]
[112,"材料類","不銹鋼焊接管(2016)","搖籃到大門",2016,"kg",1.75,"未載明","產品碳足跡資訊網"," 交通部鐵道局中部工程分局"]
[113,"材料類","熱浸鍍鋅鋼捲(2013)","搖籃到大門",2013,"kg",2.99,"未載明","產品碳足跡資訊網"," 交通部鐵道局中部工程分局"]
[114,"材料類","鋼胚(電弧爐製程， 不分型號)","未載明",2017,"kg",0.678,"未載明","公路總局蘇花公路改善工程處"," 交通部鐵道局中部工程分局"]
[115,"材料類","不鏽鋼 (電弧爐製程，SS304)","未載明",null,"kg",2.01,"未載明","經濟部產業發展署","交通部鐵道局南部工程分局"]
[116,"材料類","Railway Steel(土耳其-2021)","搖籃到大門",2021,"kg",0.999,"未載明","第三類產品環境宣告(EPD)"," 交通部鐵道局中部工程分局"]
[117,"材料類","門窗鋁框","搖籃到大門",2015,"m2",14.4,"未載明","產品碳足跡資訊網","交通部鐵道局南部工程分局"]
[118,"材料類","防振橡膠墊","未載明",2020,"kg",3.04,"未載明","鐵道局南部工程分局-南迴計畫碳管理暨碳足跡盤查服務報告"," 交通部鐵道局中部工程分局"]
[119,"材料類","Railway sleepers SBR25ML withfastening system, 100 % Portland cement and 0 %green PC-steel, manufactured in Kungsör(瑞典2023)(2,500 mm/支，257 kg/支)","搖籃到大門",2023,"支",53.2,"未載明","第三類產品環境宣告(EPD)"," 交通部鐵道局中部工程分局"]
[120,"材料類","變性環氧","未載明",2022,"加侖",21.17,"經BSI第三方查驗證","南迴計畫潮枋段土建及一般機電工程碳足跡盤查清冊暨查證結果報告","交通部鐵道局南部工程分局"]
[121,"材料類","產品，洗石子磚，厚60mm","搖籃到工地",2018,"M2",15.98,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02786"]
[122,"材料類","產品，高壓混凝土地磚，厚60mm","搖籃到墳墓",2013,"M2",55,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02786"]
[123,"材料類","產品，固定鐵件，SUS304","搖籃到大門",2013,"組",2.01,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[124,"材料類","產品，不銹鋼鑄鋼件，膨脹螺栓","未載明",2021,"式",3.01337145,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[125,"材料類","產品，浪型鋼板","未載明",2022,"M2",11.109,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[126,"材料類","產品，金屬製品，不銹鋼吊鉤，直徑13mm，#304不銹鋼，包覆塑膠","未載明",2022,"支",3.35,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[127,"材料類","產品，金屬材料，鐵線","未載明",2014,"KG",2.13,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[128,"材料類","2cm厚擋土板或鋼板","未載明",2013,"式",2.01,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02255"]
[129,"材料類","產品，纖維水泥板，厚9.0mm","搖籃到大門",2021,"M2",12.096,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[130,"材料類","產品，玻璃纖維強化塑膠格柵蓋板，格柵透 空型(含框座)","搖籃到大門",2017,"塊",9.707467,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[131,"材料類","矽酸鈣","搖籃到工地",2017,"kg",0.22,"未載明","低碳建築聯盟","內政部建築研究所"]
[132,"材料類","矽酸鈣板(6mm)","搖籃到工地",2017,"m2",1.36,"未載明","低碳建築聯盟","內政部建築研究所"]
[133,"材料類","矽酸鈣板(9mm)","搖籃到工地",2017,"m2",1.92,"未載明","低碳建築聯盟","內政部建築研究所"]
[134,"材料類","矽酸鈣板(12mm)","搖籃到工地",2017,"m2",2.54,"未載明","低碳建築聯盟","內政部建築研究所"]
[135,"材料類","窗框-鋁框架構造（陽極或氟碳烤漆）","搖籃到工地",2018,"m2",24.84,"未載明","低碳建築聯盟","內政部建築研究所"]
[136,"材料類","窗框-不鏽鋼框架構造","搖籃到工地",2018,"m2",25.6,"未載明","低碳建築聯盟","內政部建築研究所"]
[137,"材料類","塑鋼窗框構造（含補強鐵件）","搖籃到工地",2018,"m2",11.74,"未載明","低碳建築聯盟","內政部建築研究所"]
[138,"材料類","軟木木窗框","搖籃到工地",2018,"m2",1.71,"未載明","低碳建築聯盟","內政部建築研究所"]
[139,"材料類","硬木木窗框","搖籃到工地",2018,"m2",5.22,"未載明","低碳建築聯盟","內政部建築研究所"]
[140,"材料類","普通玻璃","搖籃到工地",2017,"kg",0.82,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[141,"材料類","1mm 普通玻璃","搖籃到工地",2019,"m2",2.05,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[142,"材料類","平板玻璃","搖籃到大門",2017,"kg",1.13,"未載明","產品碳足跡資訊網","內政部建築研究所","08810"]
[143,"材料類","強化玻璃","搖籃到大門",2017,"kg",1.76,"未載明","產品碳足跡資訊網","內政部建築研究所","08810"]
[144,"材料類","強化玻璃","搖籃到工地",2023,"kg",1.08,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[145,"材料類","強化玻璃(5mm)","搖籃到工地",2022,"m2",22,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[146,"材料類","強化玻璃(8mm)","搖籃到工地",2022,"m2",35.2,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[147,"材料類","強化玻璃(10mm)","搖籃到工地",2022,"m2",44,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[148,"材料類","反射玻璃","搖籃到工地",2023,"kg",1.12,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[149,"材料類","5mm 反射玻璃","搖籃到工地",2018,"m2",14,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[150,"材料類","6mm 反射玻璃","搖籃到工地",2018,"m2",16.8,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[151,"材料類","8mm 反射玻璃","搖籃到工地",2018,"m2",22.4,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[152,"材料類","10mm 反射玻璃","搖籃到工地",2018,"m2",28,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[153,"材料類","12mm 反射玻璃","搖籃到工地",2018,"m2",33.6,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[154,"材料類","1mm反射玻璃","搖籃到工地",2019,"m2",2.8,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[155,"材料類","1+1mm反射玻璃","搖籃到工地",2019,"m2",5.6,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[156,"材料類","1mm鏡面玻璃","搖籃到工地",2023,"m2",2.5,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[157,"材料類","膠合安全玻璃","搖籃到工地",2023,"kg",0.96,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[158,"材料類","雙層玻璃","搖籃到工地",2017,"kg",0.95,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[159,"材料類","1+1mm雙層玻璃 ","搖籃到工地",2019,"m2",4.75,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[160,"材料類","5+5mm雙層玻璃 ","搖籃到工地",2023,"m2",20.63,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[161,"材料類","6+6mm雙層玻璃 ","搖籃到工地",2023,"m2",24.76,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[162,"材料類","8+8mm雙層玻璃 ","搖籃到工地",2023,"m2",33.01,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[163,"材料類","5+育璽 Hm-SC75+5mm 雙層玻璃","搖籃到工地",2023,"m2",23.42,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[164,"材料類","6+育璽 Hm-SC75+6mm 雙層玻璃","搖籃到工地",2023,"m2",27.56,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[165,"材料類","8+育璽 Hm-SC75+8mm 雙層玻璃","搖籃到工地",2023,"m2",35.82,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[166,"材料類","5mm 普通或吸熱玻璃","搖籃到工地",2018,"m2",10.25,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[167,"材料類","6mm 普通或吸熱玻璃","搖籃到工地",2018,"m2",12.3,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[168,"材料類","8mm 普通或吸熱玻璃","搖籃到工地",2018,"m2",16.4,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[169,"材料類","10mm 普通或吸熱玻璃","搖籃到工地",2018,"m2",20.5,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[170,"材料類","12mm 普通或吸熱玻璃","搖籃到工地",2018,"m2",24.6,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[171,"材料類","5＋5 mm 雙強化膠合玻璃","搖籃到工地",2018,"m2",24,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[172,"材料類","6＋6 mm 雙強化膠合玻璃","搖籃到工地",2018,"m2",28.8,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[173,"材料類","8＋8 mm 雙強化膠合玻璃","搖籃到工地",2018,"m2",38.4,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[174,"材料類","5＋5 mm Low-E 玻璃","搖籃到工地",2018,"m2",32.75,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[175,"材料類","6＋6 mm Low-E 玻璃","搖籃到工地",2018,"m2",39.3,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[176,"材料類","8＋8 mm Low-E 玻璃","搖籃到工地",2018,"m2",52.4,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[177,"材料類","南亞節能膜 NY-2039","搖籃到工地",2017,"m2",0.86,"未載明","低碳建築聯盟","內政部建築研究所"]
[178,"材料類","南亞節能膜 NY-2076","搖籃到工地",2017,"m2",0.86,"未載明","低碳建築聯盟","內政部建築研究所"]
[179,"材料類","Low-E 玻璃 ","搖籃到工地",2023,"kg",1.31,"未載明","低碳建築聯盟","內政部建築研究所","08810"]
[180,"材料類","玻璃纖維絲","搖籃到工地",2023,"kg",2.77,"未載明","低碳建築聯盟","內政部建築研究所"]
[181,"材料類","玻璃纖維","搖籃到工地",2023,"kg",2.53,"未載明","低碳建築聯盟","內政部建築研究所"]
[182,"材料類","產品，選擇性回填材料，透水材料，砂","未載明",2022,"M3",8.213,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02319"]
[183,"材料類","產品，選擇性回填材料，級配粒料，碎石級配","未載明",2022,"M3",7.428,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02319"]
[184,"材料類","產品，選擇性回填材料，再生粒料，MRC","未載明",2022,"M3",9.073926,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02319"]
[185,"材料類","產品，地盤灌漿處理，化學灌漿","搖籃到大門",2022,"M3",230.1103684211,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02341"]
[186,"材料類","產品，鋼筋混凝土管(B型)，D=500mm，三 級管","搖籃到大門",2022,"M",156.2569683,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02610"]
[187,"材料類","產品，鋼筋混凝土管(B型)，D=600mm，三 級管","搖籃到大門",2022,"M",174.6015981,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02610"]
[188,"材料類","產品，鋼筋混凝土管(B型)，D=800mm，三 級管","搖籃到大門",2022,"M",247.8613976,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02610"]
[189,"材料類","產品，鋼筋混凝土管(B型)，D=1000mm， 三級管","搖籃到大門",2022,"M",309.5539251,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02610"]
[190,"材料類","產品，鋼筋混凝土管(B型)，D=1200mm， 三級管","搖籃到大門",2022,"M",391.050965,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02610"]
[191,"材料類","產品，瀝青混凝土舖面","搖籃到大門",2022,"M3",13.465,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02742"]
[192,"材料類","產品，瀝青混凝土舖面，工地交貨","未載明",2022,"M3",13.465,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02742"]
[193,"材料類","產品，瀝青混凝土舖面，防剝劑","搖籃到大門",2021,"KG",1.59,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02742"]
[194,"材料類","產品，鋪築粘層或透層","未載明",2022,"M2",2E-3,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02747"]
[195,"材料類","產品，標線，熱塑性塑膠","搖籃到大門",2017,"KG",2.73,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02898"]
[196,"材料類","產品，標線，玻璃珠","未載明",2022,"KG",1.435,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02898"]
[197,"材料類","產品，順T型接頭，聚氯乙烯塑膠硬質管，標稱管徑200x300mm","搖籃到大門",2021,"只",66.44,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[198,"材料類","產品，圓形鋼襯板工作井，加強環","搖籃到大門",2013,"M",28.677,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02531"]
[199,"材料類","產品，圓形鋼襯板工作井，CP型鋼襯板","搖籃到大門",2013,"片",176.66982036,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02531"]
[200,"材料類","產品，橢圓形鋼襯板工作井，SP型鋼襯板","搖籃到大門",2013,"片",176.66982036,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02531"]
[201,"材料類","產品，橢圓形鋼襯板工作井，JP型鋼襯板","搖籃到大門",2013,"片",176.66982036,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02531"]
[202,"材料類","產品，橢圓形鋼襯板工作井，CP型鋼襯板","搖籃到大門",2013,"片",176.66982036,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02531"]
[203,"材料類","產品，鋼套管推進，直徑800mm鋼管，鋼套 管材料費","搖籃到大門",2020,"M",702.709,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02531"]
[204,"材料類","產品，鋼套管推進，直徑1000mm鋼管，鋼套 管材料費","搖籃到大門",2020,"M",1000.5714,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02531"]
[205,"材料類","產品，鋼套管推進，直徑1200mm鋼管，鋼套 管材料費","搖籃到大門",2020,"M",1309.9002,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02531"]
[206,"材料類","產品，鋼套管推進，直徑1500mm鋼管，鋼套 管材料費","搖籃到大門",2020,"M",1928.1384,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02531"]
[207,"材料類","產品，污水管線另件，橡膠圈","未載明",2021,"條",6.72345036,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[208,"材料類","產品，污水管線附屬工作，污水管線另件， 水膨脹橡膠止水封","未載明",2021,"M",1.21275,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[209,"材料類","產品，污水管線附屬工作，污水管線另件， 擠壓式填縫帶","未載明",2021,"M",6.72345036,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[210,"材料類","產品，污水管線附屬工作，A型圓形預鑄污水人孔，標稱直徑1200mm，大小頭","搖籃到大門",2017,"個",231.0031776416,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[211,"材料類","產品，污水管線附屬工作，A型圓形預鑄污水人孔，標稱直徑1200mm，底座","搖籃到大門",2017,"個",554,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[212,"材料類","產品，污水管線附屬工作，A型圓形預鑄污水人孔，標稱直徑1200mm，300mm短管","搖籃到大門",2017,"個",111,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[213,"材料類","產品，污水管線附屬工作，A型圓形預鑄污水人孔，標稱直徑1200mm，600mm短管","搖籃到大門",2017,"個",226.9026150878,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[214,"材料類","產品，污水管線附屬工作，A型圓形預鑄污水 人孔，標稱直徑1200mm，900mm短管","搖籃到大門",2017,"個",338,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[215,"材料類","產品，污水管線附屬工作，A型圓形預鑄污水 人孔，標稱直徑1200mm，1200mm短管","搖籃到大門",2017,"個",452,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[216,"材料類","產品，污水管線附屬工作，B型圓形預鑄污水 人孔，標稱直徑1500mm，大小頭","搖籃到大門",2017,"個",319.1651307193,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[217,"材料類","產品，污水管線附屬工作，B型圓形預鑄污水人孔，標稱直徑1500mm，底座","搖籃到大門",2017,"個",1120,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[218,"材料類","產品，污水管線附屬工作，B型圓形預鑄污水人孔，標稱直徑1500mm，1200mm短管","搖籃到大門",2017,"個",669,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[219,"材料類","產品，污水管線附屬工作，C型圓形預鑄污水 人孔，標稱直徑1800mm，大小頭","搖籃到大門",2017,"個",575,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[220,"材料類","產品，污水管線附屬工作，C型圓形預鑄污水 人孔，標稱直徑1800mm，底座","搖籃到大門",2017,"個",2090,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[221,"材料類","產品，污水管線附屬工作，C型圓形預鑄污水 人孔，標稱直徑1800mm，600mm短管","搖籃到大門",2017,"個",501,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[222,"材料類","產品，污水管線附屬工作，C型圓形預鑄污水 人孔，標稱直徑1800mm，900mm短管","搖籃到大門",2017,"個",755,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[223,"材料類","產品，污水管線附屬工作，C型圓形預鑄污水 人孔，標稱直徑1800mm，1200mm短管","搖籃到大門",2017,"個",957,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[224,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔，標稱直徑750mm，50mm頂部環圈","搖籃到大門",2017,"個",14.0928795997,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[225,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔，標稱直徑750mm，100mm頂部環圈","搖籃到大門",2017,"個",22.7131591994,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[226,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔，標稱直徑750mm，150mm頂部環圈","搖籃到大門",2017,"個",31.3334387991,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[227,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔，標稱直徑750mm，300mm頂部環圈","搖籃到大門",2017,"個",57.1942775983,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[228,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔，標稱直徑900mm，50mm頂部環圈","搖籃到大門",2017,"個",15.5964167392,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[229,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔，標稱直徑900mm，100mm頂部環圈","搖籃到大門",2017,"個",25.7202334784,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[230,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔，標稱直徑900mm，150mm頂部環圈","搖籃到大門",2017,"個",35.8440502176,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[231,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P900型），頂部斜管","搖籃到大門",2017,"個",117.9371813838,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[232,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P900型），底板","搖籃到大門",2017,"個",175.0078029098,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[233,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P900型），300mm調整直管","搖籃到大門",2017,"個",66.2155004352,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[234,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P900型），600mm調整直管","搖籃到大門",2017,"個",126.9584008704,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[235,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P900型），900mm調整直管","搖籃到大門",2017,"個",187.7013013056,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[236,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P900型），1200mm調整直管","搖籃到大門",2017,"個",248.4442017407,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[237,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P900型），600mm底座直管","搖籃到大門",2017,"個",126.9584008704,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[238,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P900型），900mm底座直管","搖籃到大門",2017,"個",187.7013013056,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[239,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P900型），1200mm底座直管","搖籃到大門",2017,"個",248.4442017407,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[240,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P900型），1500mm底座直管","搖籃到大門",2017,"個",309.1871021759,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[241,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），頂部斜管","搖籃到大門",2017,"個",231.0031776416,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[242,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），頂部平板","搖籃到大門",2017,"個",180.8852662732,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[243,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），中間平板","搖籃到大門",2017,"個",182.1382138895,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[244,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），底板","搖籃到大門",2017,"個",279.1277498191,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[245,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），300mm調整直管","搖籃到大門",2017,"個",96.0265413553,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[246,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），600mm調整直管","搖籃到大門",2017,"個",186.5804827107,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[247,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），900mm調整直管","搖籃到大門",2017,"個",277.134424066,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[248,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），1200mm調整直管","搖籃到大門",2017,"個",367.6883654213,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[249,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），1500mm調整直管","搖籃到大門",2017,"個",458.2423067767,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[250,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），1800mm調整直管","搖籃到大門",2017,"個",548.796248132,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[251,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），2100mm調整直管","搖籃到大門",2017,"個",639.3501894874,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[252,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），2400mm調整直管","搖籃到大門",2017,"個",729.9041308427,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[253,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），600mm底座直管","搖籃到大門",2017,"個",186.5804827107,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[254,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），900mm底座直管","搖籃到大門",2017,"個",277.134424066,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[255,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），1200mm底座直管","搖籃到大門",2017,"個",367.6883654213,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[256,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1200型），1500mm底座直管","搖籃到大門",2017,"個",458.2423067767,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[257,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），頂部斜管","搖籃到大門",2017,"個",319.1651307193,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[258,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），頂部平板","搖籃到大門",2017,"個",371.4472082701,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[259,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），中間平板","搖籃到大門",2017,"個",251.5059500975,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[260,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），底板","搖籃到大門",2017,"個",581.1450774967,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[261,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），600mm調整直管","搖籃到大門",2017,"個",276.1092851073,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[262,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），900mm調整直管","搖籃到大門",2017,"個",411.4276276609,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[263,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），1200mm調整直管","搖籃到大門",2017,"個",546.7459702145,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[264,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），1500mm調整直管","搖籃到大門",2017,"個",682.0643127682,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[265,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），1800mm調整直管","搖籃到大門",2017,"個",817.3826553218,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[266,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），2100mm調整直管","搖籃到大門",2017,"個",952.7009978754,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[267,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），2400mm調整直管","搖籃到大門",2017,"個",1088.0193404291,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[268,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），1200mm底座直管","搖籃到大門",2017,"個",546.7459702145,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[269,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），1500mm底座直管","搖籃到大門",2017,"個",682.0643127682,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[270,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1500型），1800mm底座直管","搖籃到大門",2017,"個",817.3826553218,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[271,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1800型），頂部平板","搖籃到大門",2017,"個",560.4144896644,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[272,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1800型），中間平板","搖籃到大門",2017,"個",440.4732314919,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[273,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1800型），底板","搖籃到大門",2017,"個",812.7695300075,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[274,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1800型），600mm調整直管","搖籃到大門",2017,"個",383.4071627887,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[275,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1800型），900mm調整直管","搖籃到大門",2017,"個",572.374444183,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[276,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1800型），1200mm調整直管","搖籃到大門",2017,"個",761.3417255774,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[277,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1800型），1500mm調整直管","搖籃到大門",2017,"個",950.3090069717,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[278,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1800型），2100mm調整直管","搖籃到大門",2017,"個",1328.2435697604,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[279,"材料類","污水管線附屬工作，圓形預鑄污水人孔（P1800型），2400mm調整直管","搖籃到大門",2017,"個",1517.2108511547,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[280,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1800型），1800mm底座直管","搖籃到大門",2017,"個",1139.2762883661,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[281,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P1800型），2100mm底座直管","搖籃到大門",2017,"個",1328.2435697604,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[282,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2000型），頂部平板","搖籃到大門",2017,"個",729.0703511562,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[283,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2000型），中間平板","搖籃到大門",2017,"個",609.1290929837,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[284,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2000型），600mm調整直管","搖籃到大門",2017,"個",512.9573901345,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[285,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2000型），900mm調整直管","搖籃到大門",2017,"個",766.6997852017,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[286,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2000型），1200mm調整直管","搖籃到大門",2017,"個",1020.442180269,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[287,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2000型），1500mm調整直管","搖籃到大門",2017,"個",1274.1845753362,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[288,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2000型），1800mm調整直管","搖籃到大門",2017,"個",1527.9269704034,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[289,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2000型），2400mm調整直管","搖籃到大門",2017,"個",2035.4117605379,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[290,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2000型），1500mm底座直管","搖籃到大門",2017,"個",1274.1845753362,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[291,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2000型），1800mm底座直管","搖籃到大門",2017,"個",1527.9269704034,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[292,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2000型），2100mm底座直管","搖籃到大門",2017,"個",1781.6693654707,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[293,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2000型），2400mm底座直管","搖籃到大門",2017,"個",2035.4117605379,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[294,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），頂部平板","搖籃到大門",2017,"個",874.024999922,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[295,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），中間平板","搖籃到大門",2017,"個",754.0837417495,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[296,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），底板","搖籃到大門",2017,"個",1193.9572004252,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[297,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），600mm調整直管","搖籃到大門",2017,"個",573.2355609084,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[298,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），900mm調整直管","搖籃到大門",2017,"個",857.1170413626,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[299,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），1200mm調整直管","搖籃到大門",2017,"個",1140.9985218167,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[300,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），1500mm調整直管","搖籃到大門",2017,"個",1424.8800022709,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[301,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），1800mm調整直管","搖籃到大門",2017,"個",1708.7614827251,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[302,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），2100mm調整直管","搖籃到大門",2017,"個",1992.6429631793,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[303,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），2400mm調整直管","搖籃到大門",2017,"個",2276.5244436335,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[304,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），1800mm底座直管","搖籃到大門",2017,"個",1708.7614827251,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[305,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），2100mm底座直管","搖籃到大門",2017,"個",1992.6429631793,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[306,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔（P2200型），2400mm底座直管","搖籃到大門",2017,"個",2276.5244436335,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[307,"材料類","產品，污水管線附屬工作，人孔蓋及蓋座， 標稱直徑600mm，球狀石墨鑄鐵，含防止位移及墜落設施","搖籃到大門",2017,"只",171,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[308,"材料類","產品，污水管線附屬工作，人孔蓋及蓋座， 標稱直徑750mm，球狀石墨鑄鐵，含防止位移及墜落設施","搖籃到大門",2017,"只",267.1875,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[309,"材料類","產品，污水管線附屬工作，人孔蓋及蓋座， 標稱直徑900mm，球狀石墨鑄鐵，含防止位移及墜落設施","搖籃到大門",2017,"只",384.75,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[310,"材料類","產品，污水管管材，聚乙烯塑膠管，標稱管徑200mm","搖籃到大門",2023,"M",14.0076293106,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[311,"材料類","產品，污水管管材，聚乙烯塑膠管，標稱管徑315mm","搖籃到大門",2023,"M",34.147140753,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[312,"材料類","產品，污水管管材，聚乙烯塑膠管，標稱管徑400mm","搖籃到大門",2023,"M",55.3109573121,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[313,"材料類","產品，污水管管材，標稱管徑300mm，全鋁質水泥混凝土管","搖籃到大門",2018,"M",94.8,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[314,"材料類","產品，污水管管材，標稱管徑300mm，卜作嵐混凝土管","搖籃到大門",2020,"M",74.9314936187,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[315,"材料類","產品，污水管管材，標稱管徑400mm，全鋁質水泥混凝土管","搖籃到大門",2017,"M",106.1310181241,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[316,"材料類","產品，污水管管材，標稱管徑400mm，卜作嵐混凝土管","搖籃到大門",2020,"M",124.4649867402,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[317,"材料類","產品，鋼筋混凝土管，標稱管徑200mm","未載明",2022,"M",85.8509637457,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[318,"材料類","產品，鋼筋混凝土管，標稱管徑300mm","未載明",2022,"M",105.8302242015,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[319,"材料類","產品，鋼筋混凝土管，標稱管徑400mm","未載明",2022,"M",123.8316335801,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[320,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 300mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",105.8302242015,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[321,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 300mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（全鋁質水泥混凝土管）","搖籃到大門",2017,"M",94.8,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[322,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 300mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",62.4366324567,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[323,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 300mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",105.8302242015,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[324,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 300mm，四級管特厚管，含接頭、膠圈及必要之緩衝材，（全鋁質水泥混凝土管）","搖籃到大門",2022,"M",151.876221397,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[325,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 300mm，四級管特厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",120.1101936615,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[326,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 400mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",123.8316335801,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[327,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 400mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（全鋁質水泥混凝土管）","搖籃到大門",2017,"M",106.1310181241,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[328,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 400mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",101.7021510534,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[329,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 400mm，四級管特厚管，含接頭、膠圈及必要之緩衝材，（全鋁質水泥混凝土管）","搖籃到大門",2017,"M",217.2218473698,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[330,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 400mm，四級管特厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",210.0535235458,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[331,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 500mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",156.2569682985,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[332,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 500mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（全鋁質水泥混凝土管）","搖籃到大門",2017,"M",183.8353105211,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[333,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 500mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",169.8627451118,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[334,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 600mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",174.6015981095,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[335,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 600mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（鋁質水泥混凝土內襯管）","未載明",2022,"M",228.4425658431,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[336,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 600mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",198.2973549135,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[337,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 700mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",193.2963820988,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[338,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 700mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（鋁質水泥混凝土內襯管）","未載明",2022,"M",262.4248855524,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[339,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 700mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",229.2124568435,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[340,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 800mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",205.708,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[341,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 800mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（鋁質水泥混凝土內襯管）","未載明",2022,"M",333.6121828635,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[342,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 800mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","未載明",2022,"M",304.9157466285,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[343,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 900mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2022,"M",277.797607157,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[344,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 900mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（鋁質水泥混凝土內襯管）","未載明",2022,"M",379.3212904035,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[345,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 900mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",354.5288503737,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[346,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1000mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",309.5539251027,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[347,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1000mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（鋁質水泥混凝土內襯管）","未載明",2022,"M",426.8505062967,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[348,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1000mm，四級管厚管，含接頭、膠圈及必要之緩衝材，卜作嵐混凝土管","搖籃到大門",2020,"M",407.2094541189,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[349,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1200mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",391.0509649601,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[350,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1200mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（鋁質水泥混凝土內襯管）","未載明",2022,"M",540.5000448333,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[351,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1200mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",544.7794116094,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[352,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1350mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",464.4382416396,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[353,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1350mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（鋁質水泥混凝土內襯管）","未載明",2022,"M",638.2140414967,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[354,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1350mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",669.2163588939,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[355,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1650mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",657.1892369353,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[356,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1650mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（鋁質水泥混凝土內襯管）","未載明",2022,"M",879.3757956466,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[357,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1650mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",968.0128797102,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[358,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1800mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",753.5982639844,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[359,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1800mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（鋁質水泥混凝土內襯管）","未載明",2022,"M",1000.1115426797,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[360,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 1800mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",1129.7532830839,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[361,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 2000mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",967.1403822278,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[362,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 2000mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（鋁質水泥混凝土內襯管）","未載明",2022,"M",1248.2329707398,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[363,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 2000mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",1499.3483812043,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[364,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 2200mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",1070.8692964964,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[365,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 2200mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（鋁質水泥混凝土內襯管）","未載明",2022,"M",1382.9009781188,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[366,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 2200mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",2603.5460699184,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[367,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 2400mm，四級管厚管，含接頭、膠圈及必要之緩衝材","未載明",2022,"M",1202.8098902391,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[368,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 2400mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（鋁質水泥混凝土內襯管）","未載明",2022,"M",1546.3873677564,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[369,"材料類","產品，推進用鋼筋混凝土管，標稱管徑 2400mm，四級管厚管，含接頭、膠圈及必要之緩衝材，（卜作嵐混凝土管）","搖籃到大門",2020,"M",3667.0657857994,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[370,"材料類","產品，聚酯樹脂混凝土管，標稱管徑300mm","搖籃到大門",2017,"M",55.2,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[371,"材料類","產品，聚酯樹脂混凝土管，標稱管徑300mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",55.2,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[372,"材料類","產品，聚酯樹脂混凝土管，標稱管徑300mm，四級管特厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",109.24013929,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[373,"材料類","產品，聚酯樹脂混凝土管，標稱管徑400mm","搖籃到大門",2017,"M",91.3,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[374,"材料類","產品，聚酯樹脂混凝土管，標稱管徑400mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",91.3,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[375,"材料類","產品，聚酯樹脂混凝土管，標稱管徑400mm，四級管特厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",153.2598094857,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[376,"材料類","產品，聚酯樹脂混凝土管，標稱管徑500mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",147.1361711721,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[377,"材料類","產品，聚酯樹脂混凝土管，標稱管徑600mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",189.7455757553,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[378,"材料類","產品，聚酯樹脂混凝土管，標稱管徑700mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",237.374569807,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[379,"材料類","產品，聚酯樹脂混凝土管，標稱管徑800mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",327.1088462925,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[380,"材料類","產品，聚酯樹脂混凝土管，標稱管徑900mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",388.2265906809,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[381,"材料類","產品，聚酯樹脂混凝土管，標稱管徑1000mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",465.4739492279,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[382,"材料類","產品，聚酯樹脂混凝土管，標稱管徑1200mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",634.8027483418,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[383,"材料類","產品，聚酯樹脂混凝土管，標稱管徑1350mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",766.1412925673,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[384,"材料類","產品，聚酯樹脂混凝土管，標稱管徑1650mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",1101.3393364719,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[385,"材料類","產品，聚酯樹脂混凝土管，標稱管徑1800mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",1261.3123445728,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[386,"材料類","產品，聚酯樹脂混凝土管，標稱管徑2000mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",1585.4740945807,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[387,"材料類","產品，聚酯樹脂混凝土管，標稱管徑2200mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",1910.9696212189,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[388,"材料類","產品，聚酯樹脂混凝土管，標稱管徑2400mm，四級管厚管，含接頭、膠圈及必要之緩衝材","搖籃到大門",2017,"M",2267.2997688776,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[389,"材料類","產品，延性鑄鐵管，標稱管徑200mm","搖籃到大門",2015,"M",39.0150453036,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[390,"材料類","產品，延性鑄鐵管，標稱管徑300mm","搖籃到大門",2015,"M",57.8174767752,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[391,"材料類","產品，延性鑄鐵管，標稱管徑400mm","搖籃到大門",2015,"M",87.0489902364,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[392,"材料類","產品，聚氯乙烯塑膠硬質管，標稱管徑200mm","未載明",2022,"M",24.31,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[393,"材料類","產品，聚氯乙烯塑膠硬質管，標稱管徑300mm","未載明",2022,"M",62.7254158464,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[394,"材料類","產品，聚氯乙烯塑膠硬質管，標稱管徑400mm","未載明",2022,"M",110.7600102092,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[395,"材料類","產品，聚氯乙烯塑膠硬質管，標稱管徑150mm","未載明",2022,"M",16.2073261433,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[396,"材料類","產品，L型接頭（90度），聚氯乙烯塑膠硬質管，標稱管徑150mm","搖籃到大門",2021,"只",7.91,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[397,"材料類","產品，L型接頭（90度），聚氯乙烯塑膠硬質管，標稱管徑200mm","搖籃到大門",2021,"只",16.49,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[398,"材料類","產品，順T型接頭，聚氯乙烯塑膠硬質管，標稱管徑200x150mm","搖籃到大門",2021,"只",21.08,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[399,"材料類","產品，順T型接頭，聚氯乙烯塑膠硬質管，標稱管徑200x200mm","搖籃到大門",2021,"只",22.08,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[400,"材料類","產品，順T型接頭，聚氯乙烯塑膠硬質管，標稱管徑400x200mm","搖籃到大門",2021,"只",166.1,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[401,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P900型)，頂部斜管","搖籃到大門",2017,"個",117.9371813838,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[402,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P900型)，頂部平板","搖籃到大門",2017,"個",68.5209240491,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[403,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P900型)，底板","搖籃到大門",2017,"個",175.0078029098,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[404,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P900型)，300mm調整直管","搖籃到大門",2017,"個",66.2155004352,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[405,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P900型)，600mm調整直管","搖籃到大門",2017,"個",126.9584008704,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[406,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P900型)，900mm調整直管","搖籃到大門",2017,"個",187.7013013056,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[407,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P900型)，1200mm調整直管","搖籃到大門",2017,"個",248.4442017407,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[408,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P900型)，600mm底座直管","搖籃到大門",2017,"個",126.9584008704,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[409,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P900型)，900mm底座直管","搖籃到大門",2017,"個",187.7013013056,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[410,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P900型)，1200mm底座直管","搖籃到大門",2017,"個",248.4442017407,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[411,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P900型)，1500mm底座直管","搖籃到大門",2017,"個",309.1871021759,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[412,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，頂部斜管","搖籃到大門",2017,"個",231.0031776416,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[413,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，頂部平板","搖籃到大門",2017,"個",180.8852662732,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[414,"材料類","產品，污水管線附屬工作，圓形預鑄污水人 孔(P1200型)，中間平板","搖籃到大門",2017,"個",182.1382138895,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[415,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，底板","搖籃到大門",2017,"個",279.1277498191,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[416,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，300mm調整直管","搖籃到大門",2017,"個",96.0265413553,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[417,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，600mm調整直管","搖籃到大門",2017,"個",186.5804827107,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[418,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，900mm調整直管","搖籃到大門",2017,"個",277.134424066,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[419,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，1200mm調整直管","搖籃到大門",2017,"個",367.6883654213,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[420,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，1500mm調整直管","搖籃到大門",2017,"個",458.2423067767,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[421,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，1800mm調整直管","搖籃到大門",2017,"個",548.796248132,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[422,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，2100mm調整直管","搖籃到大門",2017,"個",639.3501894874,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[423,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，2400mm調整直管","搖籃到大門",2017,"個",729.9041308427,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[424,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，600mm底座直管","搖籃到大門",2017,"個",186.5804827107,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[425,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，900mm底座直管","搖籃到大門",2017,"個",277.134424066,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[426,"材料類","產品，污水管線附屬工作，圓形預鑄污水人孔(P1200型)，1500mm底座直管","搖籃到大門",2017,"個",458.2423067767,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[427,"材料類","產品，污水管線附屬工作，陰井，底座","搖籃到大門",2017,"個",73.3778046269,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[428,"材料類","產品，污水管線附屬工作，陰井，300mm短管","搖籃到大門",2017,"個",39.4252023135,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[429,"材料類","產品，污水管線附屬工作，陰井，400mm短管","搖籃到大門",2017,"個",50.7427364179,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[430,"材料類","產品，污水管線附屬工作，陰井，600mm短管","搖籃到大門",2017,"個",73.3778046269,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[431,"材料類","產品，污水管線附屬工作，陰井，900mm短管","搖籃到大門",2017,"個",107.3304069404,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[432,"材料類","產品，污水管線附屬工作，人孔蓋及蓋座， 標稱直徑750mm，球狀石墨鑄鐵，含防止位移及墜落設施","搖籃到大門",2017,"只",267.1875,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[433,"材料類","產品，聚氯乙烯塑膠硬質管，標稱管徑200mm","未載明",2022,"M",24.8539659037,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[434,"材料類","產品，聚乙烯塑膠管，標稱管徑200mm","搖籃到大門",2022,"M",24.0874338243,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[435,"材料類","產品，污水下水道用戶接管工程埋設施工， 聚氯乙烯塑膠硬質管，標稱管徑50mm","未載明",2022,"M",2.693,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02533"]
[436,"材料類","產品，污水下水道用戶接管工程埋設施工， 聚氯乙烯塑膠硬質管，標稱管徑80mm","未載明",2022,"M",5.9524169355,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[437,"材料類","產品，污水下水道用戶接管工程埋設施工， 聚氯乙烯塑膠硬質管，標稱管徑100mm","未載明",2022,"M",8.182,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[438,"材料類","產品，污水下水道用戶接管工程埋設施工， 聚氯乙烯塑膠硬質管，標稱管徑150mm","未載明",2022,"M",16.082,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[439,"材料類","產品，污水下水道用戶接管工程埋設施工， 聚氯乙烯塑膠硬質管，標稱管徑65mm","未載明",2017,"M",4.1293268968,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[440,"材料類","產品，污水下水道用戶接管工程埋設施工， 聚乙烯塑膠管，標稱管徑63mm","搖籃到大門",2023,"M",1.3840115824,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[441,"材料類","產品，污水下水道用戶接管工程埋設施工， 聚乙烯塑膠管，標稱管徑75mm","搖籃到大門",2023,"M",1.98332636,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[442,"材料類","產品，污水下水道用戶接管工程埋設施工， 聚乙烯塑膠管，標稱管徑90mm","搖籃到大門",2023,"M",2.8430253031,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[443,"材料類","產品，污水下水道用戶接管工程埋設施工， 聚乙烯塑膠管，標稱管徑110mm","搖籃到大門",2023,"M",4.2689969232,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[444,"材料類","產品，污水下水道用戶接管工程埋設施工， 聚乙烯塑膠管，標稱管徑160mm","搖籃到大門",2023,"M",8.95336392,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[445,"材料類","產品，糞管（重力管），聚乙烯塑膠管，標稱管徑110mm，單接糞管或側匯流接頭","搖籃到大門",2023,"只",6.3206,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[446,"材料類","產品，雨水連接管（A管），聚氯乙烯塑膠硬 質管，標稱管徑80mm","搖籃到大門",2017,"支",3.379008282,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[447,"材料類","產品，雨水連接管（A管），聚氯乙烯塑膠硬 質管，標稱管徑100mm","搖籃到大門",2017,"支",4.8250526754,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[448,"材料類","產品，塞頭，聚氯乙烯塑膠硬質管，標稱管徑50mm","搖籃到大門",2021,"只",0.39,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[449,"材料類","產品，塞頭，聚氯乙烯塑膠硬質管，標稱管徑80mm","搖籃到大門",2021,"只",0.91,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[450,"材料類","產品，塞頭，聚氯乙烯塑膠硬質管，標稱管徑100mm","搖籃到大門",2021,"只",1.93,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[451,"材料類","產品，塞頭，聚氯乙烯塑膠硬質管，標稱管徑150mm","搖籃到大門",2021,"只",5.29,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[452,"材料類","產品，塞頭，聚氯乙烯塑膠硬質管，標稱管徑200mm","搖籃到大門",2021,"只",9.66,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[453,"材料類","產品，塞頭，聚乙烯塑膠管，標稱管徑110mm","搖籃到大門",2015,"只",0.27,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[454,"材料類","產品，塞頭，聚乙烯塑膠管，標稱管徑200mm","搖籃到大門",2015,"只",1.24,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[455,"材料類","產品，L型接頭(45度)，聚氯乙烯塑膠硬質管，標稱管徑50mm","搖籃到大門",2021,"只",0.66,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[456,"材料類","產品，L型接頭(45度)，聚氯乙烯塑膠硬質管，標稱管徑80mm","搖籃到大門",2021,"只",1.39,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[457,"材料類","產品，L型接頭(45度)，聚氯乙烯塑膠硬質管，標稱管徑100mm","搖籃到大門",2021,"只",2.54,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[458,"材料類","產品，L型接頭(45度)，聚氯乙烯塑膠硬質管，標稱管徑150mm","搖籃到大門",2021,"只",7.1,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[459,"材料類","產品，L型接頭(45度)，聚氯乙烯塑膠硬質管，標稱管徑200mm","搖籃到大門",2021,"只",13.41,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[460,"材料類","產品，L型接頭(45度)，聚乙烯塑膠管，標稱管徑63mm","搖籃到大門",2015,"只",0.29,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[461,"材料類","產品，L型接頭(45度)，聚乙烯塑膠管，標稱管徑90mm","搖籃到大門",2015,"只",0.59,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[462,"材料類","產品，L型接頭(45度)，聚乙烯塑膠管，標稱管徑110mm","搖籃到大門",2015,"只",0.97,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[463,"材料類","產品，L型接頭(45度)，聚乙烯塑膠管，標稱管徑160mm","搖籃到大門",2015,"只",2.81,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[464,"材料類","產品，L型接頭(45度)，聚乙烯塑膠管，標稱管徑200mm","搖籃到大門",2015,"只",13.41,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[465,"材料類","產品，L型接頭(90度)，聚氯乙烯塑膠硬質管，標稱管徑50mm","搖籃到大門",2021,"只",0.69,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[466,"材料類","產品，L型接頭(90度)，聚氯乙烯塑膠硬質管，標稱管徑80mm","搖籃到大門",2021,"只",1.57,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[467,"材料類","產品，L型接頭(90度)，聚氯乙烯塑膠硬質管，標稱管徑100mm","搖籃到大門",2021,"只",3.26,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[468,"材料類","產品，L型接頭(90度)，聚氯乙烯塑膠硬質管，標稱管徑150mm","搖籃到大門",2021,"只",7.91,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[469,"材料類","產品，L型接頭(90度)，聚氯乙烯塑膠硬質管，標稱管徑200mm","搖籃到大門",2021,"只",16.49,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[470,"材料類","產品，L型接頭(90度)，聚乙烯塑膠管，標稱管徑63mm","搖籃到大門",2015,"只",0.29,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[471,"材料類","產品，L型接頭(90度)，聚乙烯塑膠管，標稱 管徑90mm","搖籃到大門",2015,"只",0.68,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[472,"材料類","產品，L型接頭(90度)，聚乙烯塑膠管，標稱管徑110mm","搖籃到大門",2015,"只",1.04,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[473,"材料類","產品，L型接頭(90度)，聚乙烯塑膠管，標稱管徑160mm","搖籃到大門",2015,"只",3.04,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[474,"材料類","產品，L型接頭(90度)，聚乙烯塑膠管，標稱管徑200mm","搖籃到大門",2015,"只",6.59,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[475,"材料類","產品，清除孔孔蓋，標稱管徑100mm","搖籃到大門",2021,"個",0.51,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[476,"材料類","產品，清除孔孔蓋，標稱管徑150mm","搖籃到大門",2021,"個",1.42,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[477,"材料類","產品，清除孔孔蓋，聚氯乙烯塑膠硬質管， 標稱管徑300mm","搖籃到大門",2021,"個",8.88,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[478,"材料類","產品，清除孔孔蓋，聚乙烯塑膠管，標稱管徑110mm","搖籃到大門",2015,"個",0.25,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[479,"材料類","產品，清除孔孔蓋，聚乙烯塑膠管，標稱管徑160mm","搖籃到大門",2015,"個",0.79,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[480,"材料類","產品，清除孔孔蓋，聚乙烯塑膠管，標稱管徑315mm","搖籃到大門",2015,"個",4.64,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[481,"材料類","產品，清除孔八角型孔蓋，聚氯乙烯塑膠硬質管，標稱管徑50mm","搖籃到大門",2015,"個",0.48,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[482,"材料類","產品，清除孔八角型孔蓋，聚氯乙烯塑膠硬質管，標稱管徑80mm","搖籃到大門",2015,"個",1.36,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[483,"材料類","產品，清除孔八角型孔蓋，聚氯乙烯塑膠硬 質管，標稱管徑100mm","搖籃到大門",2015,"個",2.72,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[484,"材料類","產品，清除孔八角型孔蓋，聚氯乙烯塑膠硬 質管，標稱管徑150mm","搖籃到大門",2015,"個",5.13,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[485,"材料類","產品，Y型接頭，聚氯乙烯塑膠硬質管，標稱 管徑80x50mm","搖籃到大門",2021,"只",2.7784,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[486,"材料類","產品，Y型接頭，聚氯乙烯塑膠硬質管，標稱管徑100x50mm","搖籃到大門",2021,"只",3.11,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[487,"材料類","產品，Y型接頭，聚氯乙烯塑膠硬質管，標稱管徑100x80mm","搖籃到大門",2021,"只",4.26,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[488,"材料類","產品，Y型接頭，聚氯乙烯塑膠硬質管，標稱管徑100x100mm","搖籃到大門",2021,"只",5.59,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[489,"材料類","產品，Y型接頭，聚氯乙烯塑膠硬質管，標稱管徑200x150mm","搖籃到大門",2021,"只",22.23,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[490,"材料類","產品，Y型接頭，聚乙烯塑膠管，標稱管徑200x160mm","搖籃到大門",2015,"只",7.67,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[491,"材料類","產品，Y型接頭，聚乙烯塑膠管，標稱管徑63x63mm","搖籃到大門",2015,"只",0.68,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[492,"材料類","產品，Y型接頭，聚乙烯塑膠管，標稱管徑90x90mm","搖籃到大門",2015,"只",1.22,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[493,"材料類","產品，Y型接頭，聚乙烯塑膠管，標稱管徑110x63mm","搖籃到大門",2015,"只",1.26,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[494,"材料類","產品，Y型接頭，聚乙烯塑膠管，標稱管徑110x90mm","搖籃到大門",2015,"只",1.53,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[495,"材料類","產品，順T型接頭，聚氯乙烯塑膠硬質管，標稱管徑80x50mm","搖籃到大門",2015,"只",2.27,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[496,"材料類","產品，順T型接頭，聚氯乙烯塑膠硬質管，標稱管徑80x80mm","搖籃到大門",2015,"只",2.93,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[497,"材料類","產品，順T型接頭，聚氯乙烯塑膠硬質管，標稱管徑100x50mm","搖籃到大門",2021,"只",3.35,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[498,"材料類","產品，順T型接頭，聚氯乙烯塑膠硬質管，標稱管徑100x100mm","搖籃到大門",2021,"只",5.62,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[499,"材料類","產品，順T型接頭，聚氯乙烯塑膠硬質管，標稱管徑150x150mm","搖籃到大門",2021,"只",12.11,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[500,"材料類","產品，順T型接頭，聚氯乙烯塑膠硬質管，標稱管徑200x100mm","搖籃到大門",2021,"只",13.68,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[501,"材料類","產品，順T型接頭，聚乙烯塑膠管，標稱管徑63x63mm","搖籃到大門",2015,"只",0.56,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[502,"材料類","產品，順T型接頭，聚乙烯塑膠管，標稱管徑90x90mm","搖籃到大門",2015,"只",1.01,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[503,"材料類","產品，順T型接頭，聚乙烯塑膠管，標稱管徑110x63mm","搖籃到大門",2015,"只",1.13,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[504,"材料類","產品，順T型接頭，聚乙烯塑膠管，標稱管徑110x90mm","搖籃到大門",2015,"只",1.4,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[505,"材料類","產品，異徑接頭，聚乙烯塑膠管，標稱管徑110mm，(PVC轉PE活套單放口接頭)","搖籃到大門",2015,"只",0.97,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[506,"材料類","產品，異徑接頭，聚乙烯塑膠管，標稱管徑63mm，(PVC轉PE活套單放口接頭)","搖籃到大門",2015,"只",0.25,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[507,"材料類","產品，異徑接頭，聚乙烯塑膠管，標稱管徑90mm，(PVC轉PE活套單口放接頭","搖籃到大門",2015,"只",0.52,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[508,"材料類","產品，異徑接頭，聚乙烯塑膠管，標稱管徑110x90mm","搖籃到大門",2015,"只",0.92,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[509,"材料類","產品，異徑接頭，聚乙烯塑膠管，標稱管徑90x63mm","搖籃到大門",2015,"只",0.65,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[510,"材料類","產品，異徑接頭，聚乙烯塑膠管，標稱管徑160x110mm","搖籃到大門",2015,"只",2.59,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[511,"材料類","產品，異徑接頭，聚乙烯塑膠管，標稱管徑200x160mm","搖籃到大門",2015,"只",3.83,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[512,"材料類","產品，同徑接頭，聚氯乙烯塑膠硬質管，標稱管徑100x100mm，(污水防臭接頭)","搖籃到大門",2021,"只",2.42,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[513,"材料類","產品，同徑接頭，聚乙烯塑膠管，標稱管徑63x63mm，(雙防臭匯流接頭)","搖籃到大門",2015,"只",0.23,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[514,"材料類","產品，同徑接頭，聚乙烯塑膠管，標稱管徑90x90mm，(雙防臭匯流接頭)","搖籃到大門",2015,"只",0.5,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[515,"材料類","產品，同徑接頭，聚乙烯塑膠管，標稱管徑110x110mm","搖籃到大門",2015,"只",0.86,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[516,"材料類","產品，同徑接頭，聚乙烯塑膠管，標稱管徑160x160mm","搖籃到大門",2015,"只",2.41,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[517,"材料類","產品，同徑接頭，聚乙烯塑膠管，標稱管徑200x200mm","搖籃到大門",2015,"只",3.78,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[518,"材料類","產品，鑽孔接頭，聚氯乙烯塑膠硬質管，標 稱管徑100x300mm，含連接及安裝","搖籃到大門",2021,"只",1.6,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[519,"材料類","產品，鑽孔接頭，聚氯乙烯塑膠硬質管，標 稱管徑150x300mm，含連接及安裝","搖籃到大門",2021,"只",4.71,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02534"]
[520,"材料類","產品，下水道用戶接管附屬設施，組合式連接井，調整環，高度25mm","搖籃到大門",2023,"個",2.2283266941,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[521,"材料類","產品，下水道用戶接管附屬設施，組合式連 接井，墊層，高度100mm","搖籃到大門",2023,"個",8.9133067763,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[522,"材料類","產品，下水道用戶接管附屬設施，組合式連 接井，墊層，高度300mm","搖籃到大門",2023,"個",26.7399203288,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[523,"材料類","產品，下水道用戶接管附屬設施，組合式連 接井，中層，(高度150mm，6孔，標稱孔徑100mm)","搖籃到大門",2023,"個",6.2393147434,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[524,"材料類","產品，下水道用戶接管附屬設施，組合式連 接井，底層，(高度255mm，4孔，標稱孔徑200mm)","搖籃到大門",2023,"個",3.7138778234,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[525,"材料類","產品，下水道用戶接管附屬設施，組合式連 接井，框蓋，石墨鑄鐵","搖籃到大門",2015,"組",42.787652451,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[526,"材料類","產品，下水道用戶接管附屬設施，直管式連 接井(標稱直徑300mm)，底座，兩側合流， (聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",35.85,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[527,"材料類","產品，下水道用戶接管附屬設施，直管式連 接井(標稱直徑300mm)，底座，兩側合流， (聚乙烯塑膠管)","搖籃到大門",2021,"只",16.88,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[528,"材料類","產品，下水道用戶接管附屬設施，直管式連接井(標稱直徑300mm)，底座，90度彎管 (90L)，(聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",31.23,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[529,"材料類","產品，下水道用戶接管附屬設施，直管式連接井(標稱直徑300mm)，90度彎管，(聚乙烯 塑膠管)","搖籃到大門",2021,"只",15.14,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[530,"材料類","產品，下水道用戶接管附屬設施，直管式連接井(標稱直徑300mm)，底座，30度彎管 (30L)，(聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",30.08,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[531,"材料類","產品，下水道用戶接管附屬設施，直管式連 接井(標稱直徑300mm)，30度彎管，(聚乙烯 塑膠管)","搖籃到大門",2021,"只",21.76,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[532,"材料類","產品，下水道用戶接管附屬設施，直管式連 接井(標稱直徑300mm)，底座，單側跌落， (聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",17.09,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[533,"材料類","產品，下水道用戶接管附屬設施，直管式連 接井(標稱直徑300mm)，底座，單側跌落， (聚乙烯塑膠管)","搖籃到大門",2021,"只",13.41,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[534,"材料類","產品，下水道用戶接管附屬設施，直管式連 接井(標稱直徑300mm)，底座，起點，(聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",17.09,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[535,"材料類","產品，下水道用戶接管附屬設施，直管式連 接井(標稱直徑300mm)，底座，起點，(聚乙烯塑膠管)","搖籃到大門",2021,"只",13.34,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[536,"材料類","產品，下水道用戶接管附屬設施，直管式連接井(標稱直徑300mm)，底座，單接側通， (聚乙烯塑膠管)","搖籃到大門",2021,"只",38.1225,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[537,"材料類","產品，下水道用戶接管附屬設施，直管式連接井(標稱直徑300mm)，底座，雙接側通， (聚乙烯塑膠管)","搖籃到大門",2023,"只",18.83,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[538,"材料類","產品，下水道用戶接管附屬設施，直管式連接井(標稱直徑300mm)，底座，直型，(聚乙烯塑膠管)","搖籃到大門",2021,"只",20.32,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[539,"材料類","產品，下水道用戶接管附屬設施，直管式連接井(標稱直徑300mm)，豎井，(聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"M",66.32,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[540,"材料類","產品，下水道用戶接管附屬設施，直管式連接井(標稱直徑300mm)，豎井，(聚乙烯塑膠管)","搖籃到大門",2021,"M",39.74,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[541,"材料類","產品，下水道用戶接管附屬設施，直管式連接井(標稱直徑300mm)，井蓋(隱密型)，塑膠內蓋，連接及安裝","搖籃到大門",2023,"個",3.44,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[542,"材料類","產品，下水道用戶接管附屬設施，直管式連接井(標稱直徑300mm)，井蓋(隱密型)，塑膠內蓋","搖籃到大門",2023,"個",3.44,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[543,"材料類","產品，下水道用戶接管附屬設施，直管式連接井(標稱直徑300mm)，(框蓋，含預鑄混凝土基座)，石墨鑄鐵","搖籃到大門",2017,"組",63.1013510548,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[544,"材料類","產品，下水道用戶接管附屬設施，匯流井，直型，(聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",4.53,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[545,"材料類","產品，下水道用戶接管附屬設施，匯流井，兩側合流，(聚乙烯塑膠管)","搖籃到大門",2021,"只",2.81,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[546,"材料類","產品，下水道用戶接管附屬設施，匯流井，單側跌落，(聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",4.832,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[547,"材料類","產品，下水道用戶接管附屬設施，匯流井，單側跌落，(聚乙烯塑膠管)","搖籃到大門",2021,"只",2.7,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[548,"材料類","產品，下水道用戶接管附屬設施，匯流井，雙側跌落，(聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",5.2548,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[549,"材料類","產品，下水道用戶接管附屬設施，匯流井，雙側跌落，(聚乙烯塑膠管)","搖籃到大門",2021,"只",2.75,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[550,"材料類","產品，下水道用戶接管附屬設施，匯流井， 單接存水彎，(聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",6.1306,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[551,"材料類","產品，下水道用戶接管附屬設施，匯流井，單接存水彎，(防臭、高低差調整匯流接頭)，(聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",6.1306,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[552,"材料類","產品，下水道用戶接管附屬設施，匯流井， 單接存水彎，(聚乙烯塑膠管)","搖籃到大門",2021,"只",3.74,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[553,"材料類","產品，下水道用戶接管附屬設施，匯流井， 單接存水彎，含連接及安裝，(跌落)，(聚乙烯塑膠管)","搖籃到大門",2021,"只",3.74,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[554,"材料類","產品，下水道用戶接管附屬設施，匯流井， 雙接存水彎，(聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",6.7346,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[555,"材料類","產品，下水道用戶接管附屬設施，匯流井， 雙接存水彎，(聚乙烯塑膠管)","搖籃到大門",2021,"只",4.34,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[556,"材料類","產品，下水道用戶接管附屬設施，匯流井， 單接糞管側通，(聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",5.738,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[557,"材料類","產品，下水道用戶接管附屬設施，匯流井， 單接糞管側通，(聚乙烯塑膠管)","搖籃到大門",2021,"只",3.65,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[558,"材料類","產品，下水道用戶接管附屬設施，匯流井，單接糞管及存水彎側通，(聚氯乙烯塑膠硬質管)","搖籃到大門",2023,"只",8.6372,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[559,"材料類","產品，下水道用戶接管附屬設施，匯流井， 單接糞管及存水彎側通，(聚乙烯塑膠管)","搖籃到大門",2021,"只",3.47,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[560,"材料類","產品，下水道用戶接管附屬設施，匯流井， 井蓋，塑膠蓋，300mm","搖籃到大門",2021,"個",3.0804,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[561,"材料類","產品，下水道用戶接管附屬設施，匯流井， 井蓋，塑膠蓋，標稱管徑150mm","搖籃到大門",2021,"個",1.45,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02535"]
[562,"材料類","產品，污水管線附屬工作，人孔蓋及蓋座，標稱直徑900mm，球狀石墨鑄鐵，含防止位移及墜落設施","搖籃到大門",2017,"只",384.75,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[563,"材料類","污水管路系統，聚氯乙烯管(B管厚管)，橘色管(不分類)","未載明",2022,"m",{"v":11.3104,"d":"11.31"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署",15151]
[564,"材料類","污水管路系統，聚氯乙烯管(B管厚管)，橘色管，D=50mm(t=4.1mm)","未載明",2022,"m",{"v":2.693,"d":"2.69"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署",15151]
[565,"材料類","污水管路系統，聚氯乙烯管(B管厚管)，橘色管，D=75mm(t=5.5mm)","未載明",2022,"m",{"v":5.285,"d":"5.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署",15151]
[566,"材料類","污水管路系統，聚氯乙烯管(B管厚管)，橘色管，D=100mm(t=6.6mm)","未載明",2022,"m",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署",15151]
[567,"材料類","污水管路系統，聚氯乙烯管(B管厚管)，橘色管，D=150mm(t=8.9mm)","未載明",2022,"m",{"v":16.082,"d":"16.08"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署",15151]
[568,"材料類","污水管路系統，聚氯乙烯管(B管厚管)，橘色管，D=200mm(t=10.3mm)","未載明",2022,"m",24.31,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署",15151]
[569,"材料類","材料，再生纖維水泥板(不分類)","未載明",2022,"kg",1.12,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[570,"材料類","材料，再生纖維水泥板，纖維水泥板","未載明",2022,"kg",1.12,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[571,"材料類","材料，再生纖維水泥板，矽酸鈣板","未載明",2022,"kg",1.12,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[572,"材料類","材料，玻璃(不分類)","未載明",2022,"kg",{"v":1.435,"d":"1.44"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","08810"]
[573,"材料類","材料，玻璃，普通平板玻璃","未載明",2022,"kg",1.12,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","08810"]
[574,"材料類","材料，玻璃，強化玻璃","未載明",2022,"kg",1.75,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","08810"]
[575,"材料類","材料，水泥漆，水性水泥漆","未載明",2022,"kg",1.33,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","09912"]
[576,"材料類","玻璃，【不分類】","搖籃到大門",2025,"KG",{"v":1.435,"d":"1.44"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","08810"]
[577,"材料類","玻璃，普通平板玻璃","搖籃到大門",2025,"KG",1.12,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","08810"]
[578,"材料類","玻璃，強化玻璃","搖籃到大門",2025,"KG",1.75,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","08810"]
[579,"材料類","油漆","搖籃到大門",2025,"KG",1.33,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09910"]
[580,"材料類","產品，基本產品需求，滑材費","搖籃到大門",2020,"只",15.94,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[581,"機具類","預拌混凝土車","未載明",2019,"tkm",10.052,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[582,"機具類","傾卸卡車(21t、21.5t)","搖籃到大門",2023,"m3km",0.337,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-C713標","交通部高速公路局"]
[583,"機具類","傾卸卡車(21t)","搖籃到大門",2023,"m3km",0.5413,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-C714標","交通部高速公路局"]
[584,"機具類","傾卸卡車(21t)","搖籃到大門",2023,"km",2.5388,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-C714標","交通部高速公路局"]
[585,"機具類","混凝土預拌車","搖籃到大門",2019,"m3 -km",0.66,"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查","交通部高速公路局"]
[586,"機具類","開挖機，70~79KW，（作為破碎機用）","搖籃到大門",2023,"時",46.812,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[587,"機具類","開挖機，履帶式","搖籃到大門",2022,"時",42.526,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[588,"機具類","開挖機，履帶式，90~99KW，(作為破碎機 用)","未載明",2022,"時",54.358,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[589,"機具類","施工機具，混凝土泵","未載明",2022,"天",{"v":902.016,"d":"902.02"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[590,"機具類","施工機具，混凝土泵(1式3天)","未載明",2023,"式",{"v":2706.048,"d":"2706.05"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[591,"機具類","施工機具，混凝土泵","未載明",2022,"趟",{"v":902.016,"d":"902.02"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[592,"機具類","施工機具，灑水車","搖籃到大門",2025,"天",392.544,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[593,"機具類","施工機具，灑水車，8.0~8.9m3","搖籃到大門",2025,"時",74.82,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[594,"機具類","施工機具，灑水車，8.0~8.9m3","搖籃到大門",2025,"天",598.56,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[595,"機具類","施工機具，傾卸貨車，【不分類】","搖籃到大門",2025,"時",{"v":65.662,"d":"65.66"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[596,"機具類","施工機具，傾卸貨車，【不分類】","搖籃到大門",2025,"天",{"v":525.296,"d":"525.30"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[597,"機具類","施工機具，傾卸貨車 15T","搖籃到大門",2025,"天",{"v":368.552,"d":"368.55"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[598,"機具類","施工機具，傾卸貨車 21T","搖籃到大門",2025,"時",{"v":65.133,"d":"65.13"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[599,"機具類","施工機具，傾卸貨車 21T","搖籃到大門",2025,"天",{"v":521.064,"d":"521.06"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[600,"機具類","施工機具，傾卸貨車 35T","搖籃到大門",2025,"時",{"v":85.784,"d":"85.78"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[601,"機具類","施工機具，傾卸貨車 35T","搖籃到大門",2025,"天",{"v":686.272,"d":"686.27"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[602,"機具類","施工機具，混凝土泵","搖籃到大門",2025,"時",{"v":112.752,"d":"112.75"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[603,"機具類","施工機具，開挖機，【不分類】","搖籃到大門",2025,"時",{"v":54.358,"d":"54.36"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[604,"機具類","施工機具，開挖機，【不分類】","搖籃到大門",2025,"天",{"v":434.864,"d":"434.86"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[605,"機具類","施工機具，開挖機，60~69KW","搖籃到大門",2025,"時",42.526,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[606,"機具類","施工機具，開挖機，110~119KW","搖籃到大門",2025,"時",49.068,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[607,"機具類","施工機具，開挖機，190~199KW","搖籃到大門",2025,"時",33.556,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[608,"機具類","施工機具，開挖機，260~279KW","搖籃到大門",2025,"時",67.84,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[609,"機具類","施工機具，開挖機，0.40~0.49m3","搖籃到大門",2025,"時",{"v":42.526,"d":"42.53"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[610,"機具類","施工機具，開挖機，0.40~0.49m3","搖籃到大門",2025,"天",{"v":340.208,"d":"340.21"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[611,"機具類","施工機具，開挖機，0.70~0.79m3","搖籃到大門",2025,"時",{"v":49.068,"d":"49.07"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[612,"機具類","施工機具，開挖機，0.70~0.79m3","搖籃到大門",2025,"天",{"v":392.544,"d":"392.54"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[613,"機具類","施工機具，開挖機，1.30~1.39m3","搖籃到大門",2025,"時",{"v":57.998,"d":"58.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[614,"機具類","施工機具，開挖機，1.30~1.39m3","搖籃到大門",2025,"天",{"v":463.984,"d":"463.98"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[615,"機具類","施工機具，開挖機，1.80~1.89m3","搖籃到大門",2025,"時",67.84,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[616,"機具類","施工機具，開挖機，1.80~1.89m3","搖籃到大門",2025,"天",542.72,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[617,"機具類","傾卸貨車，總重15-15.9t","未載明",2022,"時",46.069,"經ARES、BSI第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[618,"機具類","吊卡車","未載明",2022,"時",118.912,"經ARES、BSI第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[619,"機具類","全拖車、大貨車(35t)","未載明",2019,"tkm",0.14,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[620,"機具類","全拖車(43t)","未載明",2019,"tkm",0.0996,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[621,"機具類","大貨車(傾卸 車)(20t、21t)","未載明",2019,"tkm",0.333,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[622,"機具類","大貨車(預拌 車)(20t、21t)","未載明",2019,"tkm",0.575,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[623,"機具類","小貨車(3t、3.49t)","未載明",2019,"tkm",1.99,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[624,"機具類","全拖車、大貨車(35t)","搖籃到大門",2019,"tkm",0.14,"經BSI第三方查驗證","國5頭城交流道改善工程碳盤查","交通部高速公路局"]
[625,"機具類","營業大貨車(柴油)","搖籃到大門",2022,"tkm",0.131,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[626,"機具類","營業小貨車(柴油)","搖籃到大門",2022,"tkm",0.587,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[627,"機具類","混凝土運輸(甲騰)","搖籃到大門",2023,"m3km",0.5819,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-C713標","交通部高速公路局"]
[628,"機具類","混凝土運輸(廣達)","搖籃到大門",2023,"m3km",0.5222,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-C713標","交通部高速公路局"]
[629,"機具類","國際海運貨物運輸服務(燃料油動力)","搖籃到大門",2016,"tkm",0.0198,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[630,"機具類","以柴油動力垃圾車清 除運輸一般廢棄物","搖籃到大門",2018,"tkm",1.31,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[631,"機具類","土方及塊石運輸","搖籃到大門",2019,"tkm",0.14,"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查","交通部高速公路局"]
[632,"機具類","營業大貨車(柴油)","搖籃到大門",2014,"tkm",0.235,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[633,"機具類","營業小貨車(柴油)","搖籃到大門",2014,"tkm",0.647,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[634,"機具類","3.49噸常溫貨車服務(裝載率84％，包含營業據點排放)","搖籃到墳墓",2017,"tkm",0.833,"經BSI第三方查驗證","產品碳足跡資訊網","交通部高速公路局"]
[635,"機具類","推進機組，D=300mm，礫石","搖籃到大門",2023,"M",2.0037255996,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[636,"機具類","推進機組，D=300mm，卵礫石","搖籃到大門",2023,"M",2.3329090909,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[637,"機具類","推進機組，D=300mm，岩盤","搖籃到大門",2023,"M",2.3329090909,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[638,"機具類","推進機組，D=300mm，複合地質","搖籃到大門",2023,"M",2.162962071,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[639,"機具類","推進機組，D=300mm，砂土","搖籃到大門",2023,"M",2.0037255996,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[640,"機具類","推進機組，D=300mm，黏土","搖籃到大門",2023,"M",2.0037255996,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[641,"機具類","推進機組，D=400mm，礫石","搖籃到大門",2023,"M",3.5766287879,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[642,"機具類","推進機組，D=400mm，卵礫石","搖籃到大門",2023,"M",4.1202763636,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[643,"機具類","推進機組，D=400mm，岩盤","搖籃到大門",2023,"M",4.1202763636,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[644,"機具類","推進機組，D=400mm，複合地質","搖籃到大門",2023,"M",3.843541384,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[645,"機具類","推進機組，D=400mm，砂土","搖籃到大門",2023,"M",3.5766287879,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[646,"機具類","推進機組，D=400mm，黏土","搖籃到大門",2023,"M",3.5766287879,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[647,"機具類","推進機組，D=500mm，礫石","搖籃到大門",2023,"M",5.9291781818,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[648,"機具類","推進機組，D=500mm，卵礫石","搖籃到大門",2023,"M",6.2809090909,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[649,"機具類","推進機組，D=500mm，岩盤","搖籃到大門",2023,"M",6.2809090909,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[650,"機具類","推進機組，D=500mm，複合地質","搖籃到大門",2023,"M",6.1251840721,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[651,"機具類","推進機組，D=500mm，砂土","搖籃到大門",2023,"M",5.9291781818,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[652,"機具類","推進機組，D=500mm，黏土","搖籃到大門",2023,"M",5.9291781818,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[653,"機具類","推進機組，D=600mm，礫石","搖籃到大門",2023,"M",8.9340517241,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[654,"機具類","推進機組，D=600mm，卵礫石","搖籃到大門",2023,"M",12.3375,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[655,"機具類","推進機組，D=600mm，岩盤","搖籃到大門",2023,"M",12.3375,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[656,"機具類","推進機組，D=600mm，複合地質","搖籃到大門",2023,"M",11.6443820225,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[657,"機具類","推進機組，D=600mm，砂土","搖籃到大門",2023,"M",13.6667929293,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[658,"機具類","推進機組，D=600mm，黏土","搖籃到大門",2023,"M",13.6667929293,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[659,"機具類","推進機組，D=700mm，礫石","搖籃到大門",2023,"M",13.6667929293,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[660,"機具類","推進機組，D=700mm，卵礫石","搖籃到大門",2023,"M",24.1969448584,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[661,"機具類","推進機組，D=700mm，岩盤","搖籃到大門",2023,"M",24.1969448584,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[662,"機具類","推進機組，D=700mm，複合地質","搖籃到大門",2023,"M",19.4212320574,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[663,"機具類","推進機組，D=700mm，砂土","搖籃到大門",2023,"M",13.6667929293,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[664,"機具類","推進機組，D=700mm，黏土","搖籃到大門",2023,"M",13.6667929293,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[665,"機具類","推進機組，D=800mm","搖籃到大門",2023,"M",26.032715311,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[666,"機具類","推進機組，D=800mm，(中押千斤頂設備)","搖籃到大門",2023,"M",1.23965311,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[667,"機具類","推進機組，D=800mm，礫石","搖籃到大門",2023,"M",18.3193181818,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[668,"機具類","推進機組，D=800mm，卵礫石","搖籃到大門",2023,"M",32.4342026826,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[669,"機具類","推進機組，D=800mm，岩盤","搖籃到大門",2023,"M",32.4342026826,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[670,"機具類","推進機組，D=800mm，複合地質","搖籃到大門",2023,"M",26.032715311,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[671,"機具類","推進機組，D=800mm，砂土","搖籃到大門",2023,"M",18.3193181818,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[672,"機具類","推進機組，D=800mm，黏土","搖籃到大門",2023,"M",18.3193181818,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[673,"機具類","推進機組，D=900mm，(中押千斤頂設備)","搖籃到大門",2023,"M",3.6363157895,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[674,"機具類","推進機組，D=900mm，礫石","搖籃到大門",2023,"M",26.4612373737,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[675,"機具類","推進機組，D=900mm，卵礫石","搖籃到大門",2023,"M",46.8494038748,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[676,"機具類","推進機組，D=900mm，岩盤","搖籃到大門",2023,"M",46.8494038748,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[677,"機具類","推進機組，D=900mm，複合地質","搖籃到大門",2023,"M",37.6028110048,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[678,"機具類","推進機組，D=900mm，砂土","搖籃到大門",2023,"M",26.4612373737,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[679,"機具類","推進機組，D=900mm，黏土","搖籃到大門",2023,"M",26.4612373737,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[680,"機具類","推進機組，D=1000mm","搖籃到大門",2023,"M",54.6608845209,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[681,"機具類","推進機組，D=1000mm，(中押千斤頂設備)","搖籃到大門",2023,"M",2.5463144963,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[682,"機具類","推進機組，D=1000mm，礫石","搖籃到大門",2023,"M",40.0485688569,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[683,"機具類","推進機組，D=1000mm，卵礫石","搖籃到大門",2023,"M",68.5577195686,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[684,"機具類","推進機組，D=1000mm，岩盤","搖籃到大門",2023,"M",68.5577195686,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[685,"機具類","推進機組，D=1000mm，複合地質","搖籃到大門",2023,"M",54.6608845209,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[686,"機具類","推進機組，D=1000mm，砂土","搖籃到大門",2023,"M",40.0485688569,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[687,"機具類","推進機組，D=1000mm，黏土","搖籃到大門",2023,"M",40.0485688569,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[688,"機具類","推進機組，D=1200mm","搖籃到大門",2023,"M",80.124029484,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[689,"機具類","推進機組，D=1200mm，(中押千斤頂設備)","搖籃到大門",2023,"M",2.5463144963,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[690,"機具類","推進機組，D=1200mm，礫石","搖籃到大門",2023,"M",58.7047344734,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[691,"機具類","推進機組，D=1200mm，卵礫石","搖籃到大門",2023,"M",100.4945454545,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[692,"機具類","推進機組，D=1200mm，岩盤","搖籃到大門",2023,"M",100.4945454545,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[693,"機具類","推進機組，D=1200mm，複合地質裝","搖籃到大門",2023,"M",80.124029484,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[694,"機具類","推進機組，D=1200mm，砂土","搖籃到大門",2023,"M",58.7047344734,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[695,"機具類","推進機組，D=1200mm，黏土","搖籃到大門",2023,"M",58.7047344734,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[696,"機具類","推進機組，D=1350mm，(中押千斤頂設備)","搖籃到大門",2023,"M",2.5463144963,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[697,"機具類","推進機組，D=1350mm，礫石","搖籃到大門",2023,"M",71.1421782178,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[698,"機具類","推進機組，D=1350mm，卵礫石","搖籃到大門",2023,"M",121.7857627119,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[699,"機具類","推進機組，D=1350mm，岩盤","搖籃到大門",2023,"M",121.7857627119,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[700,"機具類","推進機組，D=1350mm，複合地質","搖籃到大門",2023,"M",97.0994594595,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[701,"機具類","推進機組，D=1350mm，砂土","搖籃到大門",2023,"M",71.1421782178,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[702,"機具類","推進機組，D=1350mm，黏土","搖籃到大門",2023,"M",71.1421782178,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[703,"機具類","推進機組，D=1500mm","搖籃到大門",2023,"M",128.4731404959,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[704,"機具類","推進機組，D=1650mm，(中押千斤頂設備)","搖籃到大門",2023,"M",7.042231405,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[705,"機具類","推進機組，D=1650mm，礫石","搖籃到大門",2023,"M",101.809154334,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[706,"機具類","推進機組，D=1650mm，卵礫石","搖籃到大門",2023,"M",165.1997598628,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[707,"機具類","推進機組，D=1650mm，岩盤","搖籃到大門",2023,"M",165.1997598628,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[708,"機具類","推進機組，D=1650mm，複合地質","搖籃到大門",2023,"M",132.6604132231,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[709,"機具類","推進機組，D=1650mm，砂土","搖籃到大門",2023,"M",101.809154334,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[710,"機具類","推進機組，D=1650mm，黏土","搖籃到大門",2023,"M",101.809154334,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[711,"機具類","推進機組，D=1800mm，(中押千斤頂設備)","搖籃到大門",2023,"M",7.042231405,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[712,"機具類","推進機組，D=1800mm，礫石","搖籃到大門",2023,"M",113.4945665962,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[713,"機具類","推進機組，D=1800mm，卵礫石","搖籃到大門",2023,"M",184.1609948542,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[714,"機具類","推進機組，D=1800mm，岩盤","搖籃到大門",2023,"M",184.1609948542,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[715,"機具類","推進機組，D=1800mm，複合地質","搖籃到大門",2023,"M",147.8868595041,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[716,"機具類","推進機組，D=1800mm，砂土","搖籃到大門",2023,"M",113.4945665962,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[717,"機具類","推進機組，D=1800mm，黏土","搖籃到大門",2023,"M",113.4945665962,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[718,"機具類","推進機組，D=2000mm，(中押千斤頂設備)","搖籃到大門",2023,"M",7.042231405,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[719,"機具類","推進機組，D=2000mm，礫石","搖籃到大門",2023,"M",151.5682535885,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[720,"機具類","推進機組，D=2000mm，卵礫石","搖籃到大門",2023,"M",239.9830681818,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[721,"機具類","推進機組，D=2000mm，岩盤","搖籃到大門",2023,"M",239.9830681818,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[722,"機具類","推進機組，D=2000mm，複合地質","搖籃到大門",2023,"M",191.9864545455,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[723,"機具類","推進機組，D=2000mm，砂土","搖籃到大門",2023,"M",151.5682535885,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[724,"機具類","推進機組，D=2000mm，黏土","搖籃到大門",2023,"M",151.5682535885,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[725,"機具類","推進機組，D=2200mm，(中押千斤頂設備)","搖籃到大門",2023,"M",7.042231405,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[726,"機具類","推進機組，D=2200mm，礫石","搖籃到大門",2023,"M",154.8739952153,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[727,"機具類","推進機組，D=2200mm，卵礫石","搖籃到大門",2023,"M",245.2171590909,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[728,"機具類","推進機組，D=2200mm，岩盤","搖籃到大門",2023,"M",245.2171590909,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[729,"機具類","推進機組，D=2200mm，複合地質","搖籃到大門",2023,"M",196.1737272727,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[730,"機具類","推進機組，D=2200mm，砂土","搖籃到大門",2023,"M",154.8739952153,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[731,"機具類","推進機組，D=2200mm，黏土","搖籃到大門",2023,"M",154.8739952153,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[732,"機具類","推進機組，D=2400mm，(中押千斤頂設備)","搖籃到大門",2023,"M",10.4681818182,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[733,"機具類","推進機組，D=2400mm，礫石","搖籃到大門",2023,"M",204.4601196172,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[734,"機具類","推進機組，D=2400mm，卵礫石","搖籃到大門",2023,"M",323.7285227273,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[735,"機具類","推進機組，D=2400mm，岩盤","搖籃到大門",2023,"M",323.7285227273,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[736,"機具類","推進機組，D=2400mm，複合地質","搖籃到大門",2023,"M",258.9828181818,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[737,"機具類","推進機組，D=2400mm，砂土","搖籃到大門",2023,"M",204.4601196172,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[738,"機具類","推進機組，D=2400mm，黏土","搖籃到大門",2023,"M",204.4601196172,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[739,"機具類","搖管機","搖籃到大門",2023,"時",114.208,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[740,"機具類","機具不分類，通風排氣設備","搖籃到大門",2023,"時",0.6909,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[741,"機具類","移動式起重機","搖籃到大門",2022,"時",183.509,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[742,"機具類","機具不分類，使用費","未載明",2023,"式",72.795,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[743,"機具類","施工機具，瀝青混凝土舖裝機","搖籃到大門",2023,"時",13.3796,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[744,"機具類","瀝青混凝土刨除機","搖籃到大門",2022,"時",435,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[745,"機具類","鐵輪壓路機","搖籃到大門",2023,"時",38.18,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[746,"機具類","施工機具，劃線機","搖籃到大門",2023,"時",6.02667,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[747,"機具類","施工機具，【不分類】","搖籃到大門",2025,"時",{"v":49.068,"d":"49.07"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[748,"機具類","施工機具，搬運車，【不分類】","搖籃到大門",2025,"時",{"v":65.662,"d":"65.66"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[749,"機具類","施工機具，曳引鏟土機，【不分類】","搖籃到大門",2025,"天",{"v":881.044,"d":"881.04"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[750,"機具類","施工機具，平板車，【不分類】","搖籃到大門",2025,"時",{"v":65.662,"d":"65.66"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[751,"機具類","施工機具，平板車，【不分類】","搖籃到大門",2025,"天",{"v":525.296,"d":"525.30"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[752,"機具類","施工機具，平板車，【1 式=3天，不分類】","搖籃到大門",2025,"式",{"v":1575.888,"d":"1575.89"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[753,"機具類","施工機具，平板車，【不分類】","搖籃到大門",2025,"趟",{"v":262.648,"d":"262.65"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[754,"機具類","施工機具，吊卡車，【不分類】","搖籃到大門",2025,"天",{"v":951.296,"d":"951.30"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[755,"機具類","施工機具，推土機，【不分類】","搖籃到大門",2025,"時",{"v":87.014,"d":"87.01"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[756,"機具類","施工機具，推土機，【不分類】","搖籃到大門",2025,"天",{"v":696.112,"d":"696.11"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[757,"機具類","施工機具，推土機 60~69KW","搖籃到大門",2025,"時",{"v":42.526,"d":"42.53"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[758,"機具類","施工機具，推土機 80~89KW","搖籃到大門",2025,"時",55.61,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[759,"機具類","施工機具，推土機 120~129KW","搖籃到大門",2025,"時",81.78,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[760,"機具類","施工機具，推土機 160~169KW","搖籃到大門",2025,"時",107.95,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[761,"機具類","施工機具，推土機 250~259KW","搖籃到大門",2025,"時",{"v":147.204,"d":"147.20"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[762,"機具類","施工機具，輪型起重機，【不分類】","搖籃到大門",2025,"時",{"v":183.509,"d":"183.51"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[763,"機具類","施工機具，輪型起重機，10~19T","搖籃到大門",2025,"時",{"v":118.912,"d":"118.91"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[764,"機具類","施工機具，輪型起重機，10~19T","搖籃到大門",2025,"天",{"v":951.296,"d":"951.30"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[765,"機具類","施工機具，輪型起重機，20~29T","搖籃到大門",2025,"時",{"v":165.996,"d":"166.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[766,"機具類","施工機具，輪型起重機，20~29T","搖籃到大門",2025,"天",{"v":1327.968,"d":"1327.97"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[767,"機具類","施工機具，輪型起重機，30~39T","搖籃到大門",2025,"時",204.31,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[768,"機具類","施工機具，輪型起重機，30~39t","搖籃到大門",2025,"天",{"v":1634.476,"d":"1634.48"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[769,"機具類","施工機具，輪型起重機，40~49T","搖籃到大門",2025,"時",{"v":244.818,"d":"244.82"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[770,"機具類","施工機具，輪型起重機，40~49T","搖籃到大門",2025,"天",{"v":1958.544,"d":"1958.54"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[771,"機具類","施工機具，輪型起重機，100~109t","搖籃到大門",2025,"時",495.531,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[772,"機具類","起重機(吊車)10~19T ","未載明",2026,"天",973.162,"未載明","鐵道工程減碳參考指引","交通部鐵道局"]
[773,"機具類","起重機(吊車)20~29T","未載明",2026,"天",{"v":1358.496,"d":"1,358.50"},"未載明","鐵道工程減碳參考指引","交通部鐵道局"]
[774,"機具類","起重機(吊車)40~49T","未載明",2026,"天",{"v":2003.568,"d":"2,003.57"},"未載明","鐵道工程減碳參考指引","交通部鐵道局"]
[775,"機具類","膠輪式吊車13.6MT","未載明",2026,"時",{"v":106.8,"d":"106.80"},"未載明","鐵道工程減碳參考指引","交通部鐵道局"]
[776,"機具類","膠輪式吊車27.2MT","未載明",2026,"時",140.62,"未載明","鐵道工程減碳參考指引","交通部鐵道局"]
[777,"機具類","平土機","未載明",2026,"時",{"v":70.274,"d":"70.27"},"未載明","鐵道工程減碳參考指引","交通部鐵道局"]
[778,"機具類","平路機","未載明",2026,"時",{"v":62.656,"d":"62.66"},"未載明","鐵道工程減碳參考指引","交通部鐵道局"]
[779,"工項類","清除及掘除","未載明",2022,"m3",{"v":1.325,"d":"1.33"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02231"]
[780,"工項類","構造物開挖，機械挖","未載明",2022,"m3",{"v":1.325,"d":"1.33"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02316"]
[781,"工項類","構造物回填(不分類)","未載明",2022,"m3",{"v":10.2295,"d":"10.23"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02317"]
[782,"工項類","選擇材料回填(不分類)","未載明",2022,"m3",{"v":10.2295,"d":"10.23"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02319"]
[783,"工項類","選擇材料回填，透水材料，砂","未載明",2022,"m3",{"v":8.213,"d":"8.21"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02319"]
[784,"工項類","選擇材料回填，透水材料，礫石","未載明",2022,"m3",{"v":10.961,"d":"10.96"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02319"]
[785,"工項類","選擇材料回填，透水材料，碎石","未載明",2022,"m3",{"v":13.241,"d":"13.24"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02319"]
[786,"工項類","選擇材料回填，透水材料，塊石","未載明",2022,"m3",{"v":14.106,"d":"14.11"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02319"]
[787,"工項類","選擇材料回填，級配粒料，碎石級配","未載明",2022,"m3",{"v":7.428,"d":"7.43"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02319"]
[788,"工項類","選擇材料回填，級配粒料，天然級配","未載明",2022,"m3",{"v":7.428,"d":"7.43"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02319"]
[789,"工項類","浚挖(不分類)","未載明",2022,"m3",{"v":0.981,"d":"0.98"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[790,"工項類","土方工作(不分類)","未載明",2022,"m3",{"v":1.6715,"d":"1.67"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02300"]
[791,"工項類","土方工作，挖方","未載明",2022,"m3",{"v":0.981,"d":"0.98"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02300"]
[792,"工項類","土方工作，回填方","未載明",2022,"m3",{"v":0.736,"d":"0.74"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02300"]
[793,"工項類","土方工作，近運填方","未載明",2022,"m3",{"v":1.201,"d":"1.20"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02300"]
[794,"工項類","土方工作，遠運填方","未載明",2022,"m3",{"v":4.791,"d":"4.79"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02300"]
[795,"工項類","土方工作，挖填方","未載明",2022,"m3",{"v":0.981,"d":"0.98"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02300"]
[796,"工項類","坡面工，混凝土，厚20cm","未載明",2022,"m2",{"v":39.708,"d":"39.71"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02385"]
[797,"工項類","坡面工，混凝土，厚30cm","未載明",2022,"m2",{"v":59.122,"d":"59.12"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02385"]
[798,"工項類","砌排石工(不分類)","未載明",2022,"m2",{"v":18.7972,"d":"18.80"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02386"]
[799,"工項類","砌排石工，鋪塊石，(厚25cm，未含勾縫)","未載明",2022,"m2",{"v":0.975,"d":"0.98"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02386"]
[800,"工項類","砌排石工，乾砌塊石，(厚25cm，未含勾縫)","未載明",2022,"m2",{"v":1.221,"d":"1.22"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02386"]
[801,"工項類","砌排石工，混凝土砌塊石，(厚25cm，未含勾縫)","未載明",2022,"m2",{"v":16.427,"d":"16.43"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02386"]
[802,"工項類","砌排石工，混凝土排塊石，(厚25cm，未含勾縫)","未載明",2022,"m2",{"v":22.994,"d":"22.99"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02386"]
[803,"工項類","砌排石工，混凝土襯排塊石，(厚25cm，未含勾縫)","未載明",2022,"m2",{"v":52.369,"d":"52.37"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02386"]
[804,"工項類","級配粒料底層，碎石級配，鋪設及滾壓","未載明",2022,"m3",5.74,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02722"]
[805,"工項類","臨時擋土樁設施，打拔(不分類)","未載明",2022,"m",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02255"]
[806,"工項類","排水管涵，鋼筋混凝土管(不分類)","未載明",2022,"m",205.49,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[807,"工項類","瀝青混凝土鋪面，厚10cm","未載明",2022,"m2",{"v":21.133,"d":"21.13"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[808,"工項類","瀝青混凝土面層刨除(不分類，厚5cm)","未載明",2022,"m2",{"v":2.094,"d":"2.09"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[809,"工項類","銲接鋼線網，線徑10mm，方孔20x20cm","未載明",2022,"m2",{"v":5.152,"d":"5.15"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[810,"工項類","鋼筋(不分類)","未載明",2022,"t",893.09,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03210"]
[811,"工項類","鋼筋(不分類)","未載明",2022,"kg",{"v":0.89309,"d":"0.89"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03210"]
[812,"工項類","鋼筋，SD280，連工帶料","未載明",2022,"t",893.62,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03210"]
[813,"工項類","鋼筋，SD280，連工帶料","未載明",2022,"kg",{"v":0.89362,"d":"0.89"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03210"]
[814,"工項類","鋼筋，SD280W，連工帶料","未載明",2022,"t",893.62,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03210"]
[815,"工項類","鋼筋，SD280W，連工帶料","未載明",2022,"kg",{"v":0.89362,"d":"0.89"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03210"]
[816,"工項類","鋼筋，SD420，連工帶料","未載明",2022,"t",892.56,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03210"]
[817,"工項類","鋼筋，SD420，連工帶料","未載明",2022,"kg",{"v":0.89256,"d":"0.89"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03210"]
[818,"工項類","鋼筋，SD420W，連工帶料","未載明",2022,"t",892.56,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03210"]
[819,"工項類","鋼筋，SD420W，連工帶料","未載明",2022,"kg",{"v":0.89256,"d":"0.89"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03210"]
[820,"工項類","竹節鋼筋，SD280W","未載明",2019,"kg",{"v":0.81,"d":"0.810"},"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03210"]
[821,"工項類","竹節鋼筋，SD420W","未載明",2019,"kg",{"v":0.81,"d":"0.810"},"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03210"]
[822,"工項類","竹節鋼筋，SD280W","未載明",2019,"t",0.874,"經BSI第三方查驗證","2016年國內海光鋼鐵實際盤查","交通部公路局","03210"]
[823,"工項類","竹節鋼筋，SD420W","未載明",2019,"t",{"v":0.91,"d":"0.910"},"經BSI第三方查驗證","2017年國內海光鋼鐵實際盤","交通部公路局","03210"]
[824,"工項類","竹節鋼筋(SD280W、 SD420W)","未載明",2019,"kg",0.81,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03210"]
[825,"工項類","宜聯鋼筋","搖籃到大門",2019,"kg",{"v":0.96,"d":"0.960"},"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查-宜聯鋼鐵廠","交通部高速公路局","03210"]
[826,"工項類","竹節鋼筋(不分類)","搖籃到大門",2021,"kg",{"v":0.89,"d":"0.890"},"經BSI第三方查驗證","東和桃園廠查證聲明書","交通部高速公路局","03210"]
[827,"工項類","竹節鋼筋(不分類)(豐興 2017) ","搖籃到大門",2017,"kg",{"v":0.9074,"d":"0.907"},"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-豐興鋼鐵廠","交通部高速公路局","03210"]
[828,"工項類","竹節鋼筋(不分類)(豐興 2018) ","搖籃到大門",2018,"kg",{"v":0.9788,"d":"0.979"},"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-豐興鋼鐵廠","交通部高速公路局","03210"]
[829,"工項類","竹節鋼筋(豐興 2019) ","搖籃到大門",2019,"kg",{"v":0.8459,"d":"0.846"},"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-豐興鋼鐵廠","交通部高速公路局","03210"]
[830,"工項類","竹節鋼筋(豐興，C714\n標運輸量加權平均)","搖籃到大門",2023,"kg",{"v":0.8955,"d":"0.896"},"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-豐興鋼鐵廠","交通部高速公路局","03210"]
[831,"工項類","竹節鋼筋，SD280W","搖籃到大門",2019,"kg",0.667,"經BSI第三方查驗證","東和桃園廠查證聲明書","交通部高速公路局","03210"]
[832,"工項類","竹節鋼筋，SD420W","搖籃到大門",2019,"kg",0.667,"經BSI第三方查驗證","東和桃園廠查證聲明書","交通部高速公路局","03210"]
[833,"工項類","鋼筋混凝土用鋼筋 (SD280W)","未載明",2020,"kg",0.835,"未載明","公路總局西部濱海公路南區臨時工程處","交通部鐵道局中部工程分局","03210"]
[834,"工項類","鋼筋混凝土用鋼筋 (SD420W)","未載明",2020,"kg",0.834,"未載明","公路總局西部濱海公路南區臨時工程處","交通部鐵道局中部工程分局","03210"]
[835,"工項類","熱軋竹節鋼筋(SD420W)","搖籃到大門",2017,"kg",0.901,"未載明","產品碳足跡資訊網"," 交通部鐵道局中部工程分局","03210"]
[836,"工項類","熱軋竹節鋼筋(SD280W)","搖籃到大門",2017,"kg",0.874,"未載明","產品碳足跡資訊網"," 交通部鐵道局中部工程分局","03210"]
[837,"工項類","鋼筋，SD280W，連工帶料","未載明",2022,"t",893.62,"經BSI第三方查驗證","水利工程減碳作業參考指引","國防部","03210"]
[838,"工項類","鋼筋，SD420W，連工帶料","未載明",2022,"t",892.56,"經BSI第三方查驗證","水利工程減碳作業參考指引","國防部","03210"]
[839,"工項類","鋼筋，SD280","未載明",2022,"KG",0.894,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","03210"]
[840,"工項類","鋼筋，【不分類】","搖籃到大門",2025,"T",893.09,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[841,"工項類","鋼筋，(不含鋼筋供應，含工資及零星工料)","搖籃到大門",2025,"T",5.12,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[842,"工項類","鋼筋，(不含鋼筋供應，含工資、零星工料及機具)","搖籃到大門",2025,"T",12.971,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[843,"工項類","鋼筋，(不含鋼筋供應，含工資、零星工料及機具)","搖籃到大門",2025,"KG",0.013,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[844,"工項類","鋼筋，連工帶料","搖籃到大門",2025,"T",840.12,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[845,"工項類","鋼筋，連工帶料","搖籃到大門",2025,"KG",0.84,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[846,"工項類","鋼筋，鑽孔(含空氣槍清孔)及化學藥劑","搖籃到大門",2025,"孔",0.65,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[847,"工項類","鋼筋，植筋","搖籃到大門",2025,"孔",3.655,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[848,"工項類","鋼筋，竹節鋼筋","搖籃到大門",2025,"T",834.5,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[849,"工項類","鋼筋，竹節鋼筋","搖籃到大門",2025,"KG",0.835,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[850,"工項類","鋼筋，SD280","搖籃到大門",2025,"T",835,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[851,"工項類","鋼筋，SD280","搖籃到大門",2025,"KG",0.835,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[852,"工項類","鋼筋，SD280，連工帶料","搖籃到大門",2025,"T",893.62,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[853,"工項類","鋼筋，SD280，連工帶料","搖籃到大門",2025,"KG",0.894,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[854,"工項類","鋼筋，SD280，植筋藥劑","搖籃到大門",2025,"T",835.003,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[855,"工項類","鋼筋，SD280，鑽孔(含空氣槍清孔)及化學藥劑","搖籃到大門",2025,"T",835.003,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[856,"工項類","鋼筋，含彎紮組立(加工及組立)","搖籃到大門",2025,"KG",0.899,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[857,"工項類","鋼筋，SD280，含化學藥劑","搖籃到大門",2025,"T",835.003,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[858,"工項類","鋼筋，SD280，含彎紮組立及損耗","搖籃到大門",2025,"T",5.12,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[859,"工項類","鋼筋，含彎紮組立及損耗","搖籃到大門",2025,"KG",0.943,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[860,"工項類","鋼筋，SD280，熱軋","搖籃到大門",2025,"T",835,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[861,"工項類","鋼筋，SD280，植筋","搖籃到大門",2025,"T",835.003,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[862,"工項類","鋼筋，SD280W，連工帶料","搖籃到大門",2025,"T",893.62,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[863,"工項類","鋼筋，SD280W，連工帶料","搖籃到大門",2025,"KG",0.894,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[864,"工項類","鋼筋，SD420，連工帶料","搖籃到大門",2025,"T",892.56,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[865,"工項類","鋼筋，SD420，連工帶料","搖籃到大門",2025,"KG",0.893,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[866,"工項類","鋼筋，SD420W，連工帶料","搖籃到大門",2025,"T",892.56,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[867,"工項類","鋼筋，SD420W，連工帶料","搖籃到大門",2025,"KG",0.893,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03210"]
[868,"工項類","結構用混凝土，預拌，140kgf/cm2","未載明",2022,"m3",{"v":304.785,"d":"304.79"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[869,"工項類","結構用混凝土，預拌，175kgf/cm2","未載明",2022,"m3",{"v":344.288,"d":"344.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[870,"工項類","結構用混凝土，預拌，210kgf/cm2","未載明",2022,"m3",{"v":384.285,"d":"384.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[871,"工項類","結構用混凝土，預拌，245kgf/cm2","未載明",2022,"m3",{"v":419.785,"d":"419.79"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[872,"工項類","結構用混凝土，預拌，280kgf/cm2","未載明",2022,"m3",{"v":433.785,"d":"433.79"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[873,"工項類","結構用混凝土，預拌，350kgf/cm2","未載明",2022,"m3",511.29,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[874,"工項類","結構用混凝土，預拌，420kgf/cm2","未載明",2022,"m3",{"v":578.091,"d":"578.09"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[875,"工項類","控制性低強度回填材料(CLSm)","未載明",2022,"m3",{"v":94.495,"d":"94.50"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03377"]
[876,"工項類","結構用混凝土，預拌，140kgf/cm2(2000psi)","搖籃到工地",2017,"m3",{"v":243.78,"d":"243.780"},"未載明","低碳建築聯盟","內政部建築研究所","03310"]
[877,"工項類","結構用混凝土，預拌，210kgf/cm2(3000psi)","搖籃到工地",2017,"m3",{"v":327.75,"d":"327.750"},"未載明","低碳建築聯盟","內政部建築研究所","03310"]
[878,"工項類","預拌高爐混凝土，210kgf/cm2(3000psi)","搖籃到工地",2017,"m3",{"v":206.37,"d":"206.370"},"未載明","低碳建築聯盟","內政部建築研究所","03310"]
[879,"工項類","結構用混凝土，預拌，280kgf/cm2(4000psi)","搖籃到工地",2017,"m3",{"v":369.88,"d":"369.880"},"未載明","低碳建築聯盟","內政部建築研究所","03310"]
[880,"工項類","預拌高爐混凝土，280kgf/cm2(4000psi)","搖籃到工地",2017,"m3",{"v":231,"d":"231.000"},"未載明","低碳建築聯盟","內政部建築研究所","03310"]
[881,"工項類","結構用混凝土，預拌，350kgf/cm2(5000psi)","搖籃到工地",2017,"m3",{"v":433.45,"d":"433.450"},"未載明","低碳建築聯盟","內政部建築研究所","03310"]
[882,"工項類","預拌高爐混凝土，350kgf/cm2(5000psi)","搖籃到工地",2017,"m3",{"v":268.98,"d":"268.980"},"未載明","低碳建築聯盟","內政部建築研究所","03310"]
[883,"工項類","結構用混凝土，預拌，420kgf/cm2(6000psi)","搖籃到工地",2017,"m3",{"v":497.15,"d":"497.150"},"未載明","低碳建築聯盟","內政部建築研究所","03310"]
[884,"工項類","預拌高爐混凝土，420kgf/cm2(6000psi)","搖籃到工地",2017,"m3",{"v":306.23,"d":"306.230"},"未載明","低碳建築聯盟","內政部建築研究所","03310"]
[885,"工項類","水中混凝土(210kgf/cm2) ","搖籃到工地",2017,"m3",{"v":252.12,"d":"252.120"},"未載明","產品碳足跡資訊網","內政部建築研究所","03310"]
[886,"工項類","水中混凝土(280kgf/cm2) ","搖籃到工地",2017,"m3",{"v":285.12,"d":"285.120"},"未載明","產品碳足跡資訊網","內政部建築研究所","03310"]
[887,"工項類","噴凝土(210kgf/cm2)","搖籃到工地",2017,"m3",{"v":404.12,"d":"404.120"},"未載明","低碳建築聯盟","內政部建築研究所","03310"]
[888,"工項類","鋼纖維噴凝土(255kgf/cm2)","搖籃到工地",2017,"m3",{"v":443.56,"d":"443.560"},"未載明","低碳建築聯盟","內政部建築研究所","03310"]
[889,"工項類","預拌混凝土(80kgf/cm2)","搖籃到大門",2017,"m3",{"v":207,"d":"207.000"},"經BSI第三方查驗證","產品碳足跡資訊網","交通部鐵道局南部工程分局","03310"]
[890,"工項類","混凝土(175) ","未載明",2019,"kg",{"v":215.17,"d":"215.170"},"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03310"]
[891,"工項類","混凝土(210水中)","未載明",2019,"kg",{"v":257.84,"d":"257.840"},"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03310"]
[892,"工項類","混凝土(210)","未載明",2019,"kg",{"v":230.54,"d":"230.540"},"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03310"]
[893,"工項類","混凝土，280kgf/cm2，第 II 型水泥","未載明",null,"m3",{"v":237.07,"d":"237.070"},"未載明","2017年本團隊根基預拌廠實際盤查值","交通部公路局","03310"]
[894,"工項類","混凝土(280I I型 ) ","未載明",2019,"kg",{"v":276.81,"d":"276.810"},"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03310"]
[895,"工項類","混凝土(280水中 ) ","未載明",2019,"kg",{"v":284.58,"d":"284.580"},"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03310"]
[896,"工項類","混凝土，水中280kgf/cm2，第 II 型水泥","未載明",2022,"m3",275.239,"經BSI第三方查驗證"," 南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","交通部公路局","03310"]
[897,"工項類","混凝土，420kgf/cm2，第 II 型水泥","未載明","未載明","m3",{"v":423.86,"d":"423.860"},"未載明","2017年本團隊根基預拌廠實際盤查值","交通部公路局","03310"]
[898,"工項類","混凝土(420SCC)","未載明",2019,"kg",333.99,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03310"]
[899,"工項類","混凝土(350SCCR1)","未載明",2019,"kg",310.92,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03310"]
[900,"工項類","混凝土(420早強)","未載明",2019,"kg",343.5,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03310"]
[901,"工項類","混凝土(245)","未載明",2019,"kg",247.75,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","03310"]
[902,"工項類","噴凝土(210) ","未載明",2019,"m3",{"v":394.37,"d":"394.370"},"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[903,"工項類","鋼纖維噴凝土(255)","未載明",2019,"m3",{"v":432.77,"d":"432.770"},"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[904,"工項類","預拌混凝土(140 kgf/cm2 )","未載明",2020,"m3",200,"未載明","公路總局西部濱海公路南區臨時工程處","交通部鐵道局中部工程分局","03310"]
[905,"工項類","預拌混凝土(210 kgf/cm2 )","未載明",2020,"m3",238,"未載明","公路總局西部濱海公路南區臨時工程處","交通部鐵道局中部工程分局","03310"]
[906,"工項類","預拌混凝土(280 kgf/cm2 )","未載明",2020,"m3",338,"未載明","公路總局西部濱海公路南區臨時工程處","交通部鐵道局中部工程分局","03310"]
[907,"工項類","無收縮混凝土(420kgf/cm2)","未載明",2019,"m3",493,"未載明","公路總局西部濱海公路南區臨時工程處","交通部鐵道局中部工程分局","03310"]
[908,"工項類","結構用混凝土，預拌，420kgf/cm2","未載明",2020,"m3",424,"未載明","鐵道局南部工程分局-南迴計畫碳管理暨碳足跡盤查服務報告"," 交通部鐵道局中部工程分局","03310"]
[909,"工項類","結構用混凝土，預拌，280kgf/cm2","未載明",2020,"m3",237,"未載明","鐵道局南部工程分局-南迴計畫碳管理暨碳足跡盤查服務報告"," 交通部鐵道局中部工程分局","03310"]
[910,"工項類","結構用混凝土，預拌，80kgf/cm2","未載明",2020,"m3",207,"未載明","鐵道局南部工程分局-南迴計畫碳管理暨碳足跡盤查服務報告"," 交通部鐵道局中部工程分局","03310"]
[911,"工項類","結構用混凝土，預拌，140kgf/cm2","未載明",2022,"m3",{"v":304.785,"d":"304.79"},"經BSI第三方查驗證","水利工程減碳作業參考指引","國防部","03310"]
[912,"工項類","預拌混凝土(2000psi)","搖籃到大門",2015,"m3",{"v":255,"d":"255.000"},"未載明","產品碳足跡資訊網","國防部","03310"]
[913,"工項類","結構用混凝土，預拌，280kgf/cm2","未載明",2022,"m3",{"v":433.785,"d":"433.79"},"經BSI第三方查驗證","水利工程減碳作業參考指引","國防部","03310"]
[914,"工項類","結構用混凝土，280kgf/cm2，含澆置","未載明","未載明","m3",{"v":401.33,"d":"401.330"},"未載明","永續綠色工程資訊網","臺中市政府","03310"]
[915,"工項類","控制性低強度回填材料(CLSm)","搖籃到大門",2023,"m3",76.985,"經Afnor第三方查驗證","全興資源再生股份有限公司","臺南市政府","03377"]
[916,"工項類","CLSm","搖籃到大門",2019,"m3",{"v":66.91,"d":"66.910"},"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查","交通部高速公路局","03377"]
[917,"工項類","結構用混凝土，預拌，140kgf/cm2","未載明",2022,"M3",304.785,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","03310"]
[918,"工項類","結構用混凝土，預拌，210kgf/cm2","未載明",2022,"M3",384.285,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","03310"]
[919,"工項類","結構用混凝土，（預拌，水中），210kgf/cm2","未載明",2022,"M3",346,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","03310"]
[920,"工項類","結構用混凝土，【不分類】","搖籃到大門",2025,"M3",{"v":425.187,"d":"425.19"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[921,"工項類","結構用混凝土，含澆置及搗實，【不分類】","搖籃到大門",2025,"M3",0.138,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[922,"工項類","結構用混凝土，預拌，140kgf/cm2","搖籃到大門",2025,"M3",{"v":304.785,"d":"304.79"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[923,"工項類","結構用混凝土，預拌，175kgf/cm2","搖籃到大門",2025,"M3",{"v":344.288,"d":"344.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[924,"工項類","結構用混凝土，預拌，210kgf/cm2","搖籃到大門",2025,"M3",384.285,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[925,"工項類","結構用混凝土，預拌，210kgf/cm2，含澆置","搖籃到大門",2025,"M3",384.423,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[926,"工項類","結構用混凝土，預拌，210kgf/cm2，含澆置及搗實","搖籃到大門",2025,"M3",385.243,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[927,"工項類","結構用混凝土，預拌，245kgf/cm2","搖籃到大門",2025,"M3",{"v":419.785,"d":"419.79"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[928,"工項類","結構用混凝土，預拌，280kgf/cm2","搖籃到大門",2025,"M3",{"v":433.785,"d":"433.79"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[929,"工項類","結構用混凝土，預拌，280kgf/cm2，含澆置及搗實","搖籃到大門",2025,"M3",434.743,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[930,"工項類","結構用混凝土，預拌，350kgf/cm2","搖籃到大門",2025,"M3",511.29,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[931,"工項類","結構用混凝土，預拌，420kgf/cm2","搖籃到大門",2025,"M3",{"v":578.091,"d":"578.09"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[932,"工項類","噴凝土，抗壓強度 175kgf/cm2","搖籃到大門",2025,"M3",269.343,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[933,"工項類","控制性低強度回填材料，【不分類】","搖籃到大門",2025,"M3",{"v":157,"d":"157.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03377"]
[934,"工項類","混凝土模板及附屬品，支撐施工架，鋼料，4.1≦支撐高度＜6.0m","未載明",2022,"m2",{"v":0,"d":"0.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[935,"工項類","場鑄結構混凝土用模板(不分類)","未載明",2022,"m2",{"v":1.2702,"d":"1.27"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[936,"工項類","場鑄結構混凝土用模板，普通模板，一般工程用","未載明",2022,"m2",{"v":1.202,"d":"1.20"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[937,"工項類","場鑄結構混凝土用模板，普通模板，建築","未載明",2022,"m2",{"v":1.202,"d":"1.20"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[938,"工項類","場鑄結構混凝土用模板，清水模板","未載明",2022,"m2",{"v":1.204,"d":"1.20"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[939,"工項類","場鑄結構混凝土用模板，免拆模板，木質","未載明",2022,"m2",{"v":0.852,"d":"0.85"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[940,"工項類","場鑄結構混凝土用模板，免拆模板，鋼質(t=0.3mm)","未載明",2022,"m2",{"v":6.902,"d":"6.90"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[941,"工項類","場鑄結構混凝土用模板，鋼製模板","未載明",2022,"m2",{"v":11.109,"d":"11.11"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[942,"工項類","場鑄結構混凝土用模板，造型模板","未載明",2022,"m2",{"v":1.891,"d":"1.89"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[943,"工項類","混凝土附屬品，填縫版、止水帶、伸縮縫","未載明",2022,"m2",{"v":0,"d":"0.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[944,"工項類","混凝土附屬品，填縫版、止水帶、伸縮縫","未載明",2022,"式",{"v":0,"d":"0.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[945,"工項類","混凝土附屬品，填縫版、止水帶、伸縮縫","未載明",2022,"組",{"v":0,"d":"0.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[946,"工項類","混凝土附屬品，填縫版、止水帶、伸縮縫","未載明",2022,"處",{"v":0,"d":"0.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[947,"工項類","場鑄結構混凝土用模板，普通模板，建築","未載明",2022,"m2",{"v":1.202,"d":"1.20"},"經BSI第三方查驗證","水利工程減碳作業參考指引","國防部"]
[948,"工項類","場鑄結構混凝土用模板，清水模板","未載明",2022,"m2",{"v":1.204,"d":"1.20"},"經BSI第三方查驗證","水利工程減碳作業參考指引","國防部"]
[949,"工項類","普通模板，丙種","未載明",2022,"M2",1.202,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","03110"]
[950,"工項類","清水模板，丙種","未載明",2022,"M2",1.204,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","03110"]
[951,"工項類","場鑄結構混凝土用模板，【不分類】","搖籃到大門",2025,"M2",1.27,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[952,"工項類","場鑄結構混凝土用模板，軀体","搖籃到大門",2025,"M2",0.997,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[953,"工項類","場鑄結構混凝土用模板，普通模板","搖籃到大門",2025,"M2",{"v":0.829,"d":"0.83"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[954,"工項類","場鑄結構混凝土用模板，普通模板，一般工程用","搖籃到大門",2025,"M2",{"v":1.202,"d":"1.20"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[955,"工項類","場鑄結構混凝土用模板，普通模板，(建築，建築物)","搖籃到大門",2025,"M2",{"v":1.202,"d":"1.20"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[956,"工項類","場鑄結構混凝土用模板，普通模板，軀体","搖籃到大門",2025,"M2",0.835,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[957,"工項類","場鑄結構混凝土用模板，普通模板，基礎","搖籃到大門",2025,"M2",0.394,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[958,"工項類","場鑄結構混凝土用模板，清水模板","搖籃到大門",2025,"M2",{"v":1.204,"d":"1.20"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[959,"工項類","場鑄結構混凝土用模板，清水模板，軀体","搖籃到大門",2025,"M2",0.857,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[960,"工項類","場鑄結構混凝土用模板，(免拆模板，木質)","搖籃到大門",2025,"M2",0.16,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[961,"工項類","場鑄結構混凝土用模板，(免拆模板，鋼質)","搖籃到大門",2025,"M2",{"v":6.902,"d":"6.90"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[962,"工項類","場鑄結構混凝土用模板，鋼製模板","搖籃到大門",2025,"M2",{"v":11.109,"d":"11.11"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[963,"工項類","場鑄結構混凝土用模板，造型模板","搖籃到大門",2025,"M2",{"v":1.891,"d":"1.89"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[964,"工項類","混凝土附屬品，填縫板，保麗龍","搖籃到大門",2025,"KG",2.84,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[965,"工項類","混凝土附屬品，伸縮縫，【連工帶料】","搖籃到大門",2025,"道",4.945,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[966,"工項類","混凝土附屬品，伸縮縫，路面、堤坡","搖籃到大門",2025,"組",3.24,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[967,"工項類","混凝土附屬品，施工縫","搖籃到大門",2025,"M2",0.065,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03150"]
[968,"工項類","PVC 塑膠硬質管 (2\"*3.0*4m)","未載明",2019,"kg",3.23,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[969,"工項類","鋼筋混凝土管涵(B 型)，100cmφ，Ⅲ級","未載明",2022,"m",0.157,"經BSI第三方查驗證","南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","交通部公路局","02610"]
[970,"工項類","鋼筋混凝土管涵(B 型)，60cmφ，Ⅲ級","未載明",2022,"m",0.157,"經BSI第三方查驗證","南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","交通部公路局","02610"]
[971,"工項類","瀝青混凝土(1\"粗級配)","未載明",2019,"kg",0.0883,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","02742"]
[972,"工項類","瀝青混凝土(3/4\"密級 配)","未載明",2019,"kg",0.0875,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","02742"]
[973,"工項類","瀝青混凝土(1/2\"密級 配)","未載明",2019,"kg",0.0834,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","02742"]
[974,"工項類","標線","未載明",2019,"kg",20.37,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","02898"]
[975,"工項類","玻璃珠","未載明",2019,"kg",0.12,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[976,"工項類","亞東 350 自充填混凝土 I 型","搖籃到大門",2023,"m3",296.31,"經BSI第三方查驗證","亞東混凝土廠","交通部高速公路局","03310"]
[977,"工項類","廣達 80 混凝土 I 型","搖籃到大門",2023,"m3",146.51,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-廣達混凝土廠","交通部高速公路局","03310"]
[978,"工項類","甲騰 80 混凝土 I 型","搖籃到大門",2023,"m3",144.75,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局","03310"]
[979,"工項類","亞東 80 混凝土 I 型 ","搖籃到大門",2023,"m3",149.77,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","交通部高速公路局","03310"]
[980,"工項類","立泰混凝土，175kgf/cm2","搖籃到大門",2023,"m3",237.68,"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查-立泰預拌混凝土廠","交通部高速公路局","03310"]
[981,"工項類","廣達 175 混凝土 I 型 ","搖籃到大門",2023,"m3",188.94,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-廣達混凝土廠","交通部高速公路局","03310"]
[982,"工項類","甲騰 175 混凝土 I 型","搖籃到大門",2023,"m3",187.39,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局","03310"]
[983,"工項類","甲騰 175 低鹼混凝土 I 型","搖籃到大門","2023","t",189.44,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局","03310"]
[984,"工項類","亞東 175 混凝土 I 型","搖籃到大門",2023,"m3",187.38,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","交通部高速公路局","03310"]
[985,"工項類","立泰混凝土，245kgf/cm2","未載明",2023,"m3",289.24,"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查-立泰預拌混凝土廠","交通部高速公路局","03310"]
[986,"工項類","甲騰 210 混凝土 I 型 ","搖籃到大門",2023,"m3",463.34,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局","03310"]
[987,"工項類","廣達 245 混凝土 I 型 ","搖籃到大門",2023,"m3",243.27,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-廣達混凝土廠","交通部高速公路局","03310"]
[988,"工項類","甲騰 245 混凝土 I 型 ","搖籃到大門",2023,"m3",244.15,"經BSI第三方查驗證","甲騰混凝土廠","交通部高速公路局","03310"]
[989,"工項類","亞東 245 混凝土 I 型 ","搖籃到大門",2023,"m3",241.42,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","交通部高速公路局","03310"]
[990,"工項類","立泰混凝土，280kgf/cm2","未載明",2023,"m3",310.34,"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查-立泰預拌混凝土廠","交通部高速公路局","03310"]
[991,"工項類","廣達280 混凝土 I 型 ","搖籃到大門",2023,"m3",270.43,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-廣達混凝土廠","交通部高速公路局","03310"]
[992,"工項類","甲騰280 混凝土 I 型 ","搖籃到大門",2023,"m3",270.84,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局","03310"]
[993,"工項類","亞東280 混凝土 I 型 ","搖籃到大門",2023,"m3",262.92,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","交通部高速公路局","03310"]
[994,"工項類","甲騰 280 低鹼混凝土 I 型 ","搖籃到大門","2023","m3",271.3,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局","03310"]
[995,"工項類","廣達 315 水中混凝土 I 型","搖籃到大門",2023,"m3",271.27,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-廣達混凝土廠","交通部高速公路局","03310"]
[996,"工項類","甲騰 315 水中混凝土 I 型","搖籃到大門",2023,"m3",281.06,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局","03310"]
[997,"工項類","亞東 315 水中混凝土 I 型","搖籃到大門",2023,"m3",265.14,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","交通部高速公路局","03310"]
[998,"工項類","立泰混凝土，350kgf/cm2","搖籃到大門",2023,"m3",359.64,"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查-立泰預拌混凝土廠","交通部高速公路局","03310"]
[999,"工項類","廣達 350 自充填混凝土 I 型","搖籃到大門",2023,"m3",311.96,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-廣達混凝土廠","交通部高速公路局","03310"]
[1000,"工項類","甲騰 350 自充填混凝土 I 型 ","搖籃到大門",2023,"m3",323.88,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局","03310"]
[1001,"工項類","甲騰 350 低鹼填混凝土 I 型-1 ","搖籃到大門","2023","m3",279.85,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局","03310"]
[1002,"工項類","甲騰 350 低鹼填混凝土 I 型-2 ","搖籃到大門","2023","m3",309.82,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局","03310"]
[1003,"工項類","亞東 350 混凝土 I 型 ","搖籃到大門",2023,"m3",296.53,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","交通部高速公路局","03310"]
[1004,"工項類","亞東 350 自充填混凝土 I 型","搖籃到大門",2023,"m3",296.31,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","交通部高速公路局","03310"]
[1005,"工項類","混凝土(245)","未載明",2023,"kg",247.75,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部高速公路局","03310"]
[1006,"工項類","立泰混凝土315(水中) ","搖籃到大門",2023,"m3",342.01,"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查-立泰預拌混凝土廠","交通部高速公路局","03310"]
[1007,"工項類","甲騰420 無收縮混凝土I型 ","搖籃到大門",2023,"m3",415.19,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局","03310"]
[1008,"工項類","亞東 420 混凝土 I 型 ","搖籃到大門",2023,"m3",375.89,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","交通部高速公路局","03310"]
[1009,"工項類","亞東 420 早強混凝土 I 型","搖籃到大門","2023","m3",453.54,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","交通部高速公路局","03310"]
[1010,"工項類","亞東 420 自充填混凝土 I 型","搖籃到大門","2023","m3",306.88,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","交通部高速公路局","03310"]
[1011,"工項類","亞東420 無收縮混凝土 I 型","搖籃到大門",2023,"m3",437.42,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-亞東混凝土廠","交通部高速公路局","03310"]
[1012,"工項類","甲騰 175 噴凝土 I 型 ","搖籃到大門",2023,"m3",414.99,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局"]
[1013,"工項類","甲騰 210 噴凝土 I 型 ","搖籃到大門",2023,"m3",462.98,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局"]
[1014,"工項類","甲騰 255 鋼纖噴凝土 I 型","搖籃到大門",2023,"m3",523.75,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局"]
[1015,"工項類","甲騰 420 早強噴凝土 I 型","搖籃到大門",2023,"m3",427.6,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-甲騰混凝土廠","交通部高速公路局"]
[1016,"工項類","填縫劑","未載明",2022,"包",0.94,"經BSI第三方查驗證","南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","交通部公路局"]
[1017,"工項類","UIC60 鋼軌","未載明",2014,"m",0.947,"未載明","2014年本團隊東和鋼鐵高雄廠實際盤查","交通部公路局","05651"]
[1018,"工項類","鋼橋，鋼梁，Gr.50(不含側推工法)","未載明",2022,"t",2.839,"經BSI第三方查驗證","南迴計畫潮枋段土建及一般機電工程碳管理暨碳足跡盤查服務工作–工作成果報告","交通部公路局"]
[1019,"工項類","鋼結構","未載明",2019,"kg",2.31,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[1020,"工項類","盤式支承(橡膠)","未載明",2019,"kg",3.34,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","05821"]
[1021,"工項類","盤式支承(鍛鋼)","未載明",2019,"kg",2.31,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局","05821"]
[1022,"工項類","石英磚","未載明",2019,"kg",0.2,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[1023,"工項類","磁磚","未載明",2019,"kg",0.2,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[1024,"工項類","外置預力斜索-端錨","未載明",2019,"kg",2.31,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[1025,"工項類","外置預力斜索 (披覆 HDPE護套鋼 絞線)","未載明",2019,"kg",2.16,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[1026,"工項類","HDPE 外套管","未載明",2019,"kg",1.6,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[1027,"工項類","預力地錨護管(平面、浪型)","未載明",2019,"kg",1.6,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[1028,"工項類","全螺紋岩釘(D25)","未載明",2019,"kg",0.84,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[1029,"工項類","PVC 防水膜","未載明",2019,"kg",2.13,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[1030,"工項類","拉線箱蓋版及框","未載明",2019,"kg",3.47,"經BSI第三方查驗證","蘇花改計畫施工期間工程碳管理委託服務工作成果","交通部公路局"]
[1031,"工項類","土方工作(不分類)","未載明",2019,"m3",8.65,"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查","交通部高速公路局","02300"]
[1032,"工項類","土方","搖籃到大門",2019,"m3",8.65,"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查","交通部高速公路局","02300"]
[1033,"工項類","瀝青處理底層(BtB)","搖籃到大門","2023","t",77.79,"經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","02714"]
[1034,"工項類","瀝青處理底層(BtB)","搖籃到大門",2023,"m3",185.84,"經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","02714"]
[1035,"工項類","瀝青處理底層(BtB) ","搖籃到大門",2023,"t",75.41,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C713標)","交通部高速公路局","02714"]
[1036,"工項類","瀝青處理底層(BtB) ","搖籃到大門",2023,"t",76.47,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C714標)","交通部高速公路局","02714"]
[1037,"工項類","瀝青混凝土","搖籃到大門",2019,"kg",0.07,"經BSI第三方查驗證","國道5號頭城交流道工程碳盤查","交通部高速公路局","02742"]
[1038,"工項類","開放級配瀝青混凝土(OGAC)","搖籃到大門",2023,"t",89.21,"經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","02742"]
[1039,"工項類","開放級配瀝青混凝土(OGAC)","搖籃到大門",2023,"m3",196.25,"經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","02742"]
[1040,"工項類","石膠泥瀝青混凝土(SmA)","搖籃到大門","2023","t",140.76,"經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","02742"]
[1041,"工項類","石膠泥瀝青混凝土(SmA)","搖籃到大門","2023","m3",327.14,"經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","02742"]
[1042,"工項類","石膠泥瀝青混凝土(SmA)","搖籃到大門","2023","t",143.83,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C713標)","交通部高速公路局","02742"]
[1043,"工項類","石膠泥瀝青混凝土(SmA)","搖籃到大門","2023","t",147.73,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C714標)","交通部高速公路局","02742"]
[1044,"工項類","密級配瀝青混凝土(DGAC)","搖籃到大門",2023,"t","79.59","經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","02742"]
[1045,"工項類","密級配瀝青混凝土(DGAC)","搖籃到大門",2023,"m3","188.64","經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","02742"]
[1046,"工項類","改質密級配瀝青混凝土\n(改質 DGAC)","搖籃到大門",2023,"t",89.69,"經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","M02796"]
[1047,"工項類","改質密級配瀝青混凝土\n(改質 DGAC)","搖籃到大門",2023,"m3",214.28,"經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","M02796"]
[1048,"工項類","密級配改質瀝青混凝土(改質 DGAC) ","搖籃到大門",2023,"t",56.77,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C714標)","交通部高速公路局","M02796"]
[1049,"工項類","密級配瀝青混凝土(3/4\"DGAC)","搖籃到大門",2023,"t",77.39,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C713標)","交通部高速公路局","02742"]
[1050,"工項類","密級配瀝青混凝土(3/4\"DGAC) ","搖籃到大門",2023,"t",77.65,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C714標)","交通部高速公路局","02742"]
[1051,"工項類","熱鑄膠泥瀝青混凝土\n(GUSS Asphalt)","搖籃到大門","2023","t",125.36,"經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","02742"]
[1052,"工項類","熱鑄膠泥瀝青混凝土\n(GUSS Asphalt)","搖籃到大門","2023","m3",298.1,"經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","02742"]
[1053,"工項類","熱鑄膠泥瀝青混凝土(GUSS) ","搖籃到大門","2023","t",122.41,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查 - 鴻運瀝青廠(C714標)","交通部高速公路局","02742"]
[1054,"工項類","多孔隙瀝青混凝土(PAC)","搖籃到大門","2023","t",100.76,"經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","02798"]
[1055,"工項類","多孔隙瀝青混凝土(PAC)","搖籃到大門",2023,"m3",200.2,"經BSI第三方查驗證","國道1號后里至大雅路段拓寬-專題研究-國道鋪面工程減碳之策略期末報告","交通部高速公路局","02798"]
[1056,"工項類","多孔隙瀝青混凝土(PAC)","搖籃到大門","2023","t",101.17,"經BSI第三方查驗證","禾鑫瀝青廠","交通部高速公路局","02798"]
[1057,"工項類","多孔隙瀝青混凝土(PAC)","搖籃到大門","2023","t",102.77,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查 - 禾鑫瀝青廠(C714標)","交通部高速公路局","02798"]
[1058,"工項類","型鋼(不分類)(豐興 2019)","搖籃到大門",2023,"kg",0.9282,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-豐興鋼鐵廠","交通部高速公路局","05125"]
[1059,"工項類","鋼構(不分類)(中鋼構) ","搖籃到大門",2023,"kg",3.0049,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-中鋼結構公司","交通部高速公路局","05125"]
[1060,"工項類","盤式支承(CC-GB300-225)(單向活動型，標稱載重300t，水平支承225t，無抗上揚力)","搖籃到大門",2023,"kg/組",1183.46,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1061,"工項類","盤式支承(CC-GB350-250)(單向活動型，標稱載重350t，水平支承250t，無抗上揚力)","搖籃到大門",2023,"kg/組",1277.22,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1062,"工項類","盤式支承(CC-GB400-300)(單向活動型，標稱載重400t，水平支承300t，無抗上揚力)","搖籃到大門",2023,"kg/組",1451.91,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1063,"工項類","盤式支承(CC-GB500-225)(單向活動型，標稱載重500t，水平支承225t，無抗上揚力)","搖籃到大門",2023,"kg/組",1735.82,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1064,"工項類","盤式支承(CC-GB500-400)(單向活動型，標稱載重500t，水平支承400t，無抗上揚力)","搖籃到大門",2023,"kg/組",2291.04,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1065,"工項類","盤式支承(CC-GB600-400)(單向活動型，標稱載重600t，水平支承400t，無抗上揚力)","搖籃到大門",2023,"kg/組",2614.63,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1066,"工項類","盤式支承(SC-FB450-475)(固定型，標稱載重450t，水平支承475t，無抗上揚力)","搖籃到大門",2023,"kg/組",1744.3654552,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1067,"工項類","盤式支承(SC-FB450-650)(固定型，標稱載重450t，水平支承650t，無抗上揚力)","搖籃到大門",2023,"kg/組",3923.1376555,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1068,"工項類","盤式支承(SC-FB1600-700)(固定型，標稱載重1600t，水平支承700t，無抗上揚力)","搖籃到大門",2023,"kg/組",7957.1265781,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1069,"工項類","盤式支承(SC-FB1800-850)(固定型，標稱載重1800t，水平支承850t，無抗上揚力)","搖籃到大門",2023,"kg/組",10799.794485999999,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1070,"工項類","盤式支承(SC-FB2200-800)(固定型，標稱載重2200t，水平支承800t，無抗上揚力)","搖籃到大門",2023,"kg/組",10514.045100000001,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1071,"工項類","盤式支承(SC-GB450-325 )(單向活動型，標稱載重450t，水平支承800t，無抗上揚力)","搖籃到大門",2023,"kg/組",1941.933851,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1072,"工項類","盤式支承(SC-GB1800-550)(單向活動型，標稱載重1800t，水平支承550t，無抗上揚力)","搖籃到大門",2023,"kg/組",9861.7610904,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1073,"工項類","盤式支承(SC-GB2300-550)(單向活動型，標稱載重2300t，水平支承550t，無抗上揚力)","搖籃到大門",2023,"kg/組",12639.736601999999,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1074,"工項類","盤式支承(CC-FB400-450)(固定型，標稱載重400t，水平支承450t，無抗上揚力)","搖籃到大門",2023,"kg/組",2567.1311792,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1075,"工項類","盤式支承(CC-FB700-300)(固定型，標稱載重700t，水平支承300t，無抗上揚力)","搖籃到大門",2023,"kg/組",3332.5826346,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1076,"工項類","盤式支承(CC-FU350-445-100)(固定型，標稱載重350t，水平支承445t，抗上揚力100t)","搖籃到大門",2023,"kg/組",2388.2752736,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1077,"工項類","盤式支承(CC-GB350-50 )(單向活動型，標稱載重350t，水平支承445t，無抗上揚力)","搖籃到大門",2023,"kg/組",847.8791532,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1078,"工項類","盤式支承(CC-GB350-175 )(單向活動型，標稱載重350t，水平支承175t，無抗上揚力)","搖籃到大門",2023,"kg/組",1233.7783301,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1079,"工項類","盤式支承(CC-GB450-125)(單向活動型，標稱載重450t，水平支承125t，無抗上揚力)","搖籃到大門",2023,"kg/組",1315.6110258,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1080,"工項類","盤式支承(CC-GB800-325)(單向活動型，標稱載重800t，水平支承325t，無抗上揚力)","搖籃到大門",2023,"kg/組",3665.3680036,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1081,"工項類","盤式支承(CC-GU300-200-125)(單向活動型，標稱載重300t，水平支承200t，抗上揚力125t)","搖籃到大門",2023,"kg/組",1518.5039865,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1082,"工項類","盤式支承(CC-GU350-100-24)(單向活動型，標稱載重350t，水平支承100t，抗上揚力24t)","搖籃到大門",2023,"kg/組",1075.0709835,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1083,"工項類","盤式支承(CC-GU500-75-150)(單向活動型，標稱載重500t，水平支承75t，抗上揚力150t)","搖籃到大門",2023,"kg/組",1701.2523055,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1084,"工項類","盤式支承(CC-SB1000)(雙向活動型，標稱載重1000t)","搖籃到大門",2023,"kg/組",2775.2811949,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1085,"工項類","盤式支承(CC-GB400-600)(單向活動型，標稱載重400t，水平支承600t，無抗上揚力)","搖籃到大門",2023,"kg/組",3175.3221586,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1086,"工項類","盤式支承(CC-GB600-600)(單向活動型，標稱載重600t，水平支承600t，無抗上揚力)","搖籃到大門",2023,"kg/組",3394.8792696,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-劦承公司","交通部高速公路局","05821"]
[1087,"工項類","地工格網","搖籃到大門",2023,"kg",4.3566,"經BSI第三方查驗證","國道4號臺中環線豐原潭子段工程碳盤查-盟鑫工業","交通部高速公路局"]
[1088,"工項類","密級配瀝青混凝土 (混和料比例 2.9%)","未載明",2020,"kg",0.129,"未載明","公路總局西部濱海公路南區臨時工程處","交通部鐵道局中部工程分局","02742"]
[1089,"工項類","輕質骨材混凝土 (175kgf/cm2 )","未載明",2019,"m3",317,"未載明","公路總局西部濱海公路南區臨時工程處","交通部鐵道局南部工程分局"]
[1090,"工項類","水泥砂漿粉刷(1:3)","搖籃到大門",2015,"m2",9.83,"未載明","產品碳足跡資訊網"," 交通部鐵道局中部工程分局","04061"]
[1091,"工項類","石質地磚","未載明",2015,"kg",4.5,"未載明","宏洲窯業股份有限公司","交通部鐵道局南部工程分局"]
[1092,"工項類","磨石子地磚，30cm*30cm*2cm","未載明",2016,"片",1.7,"未載明","晶泰水泥加工廠股份有限公司","交通部鐵道局南部工程分局"]
[1093,"工項類","再生高壓透水混凝土 地磚 (20cm*20cm*6cm)","未載明",2020,"片",1.18,"未載明","健源有限公司","交通部鐵道局南部工程分局"]
[1094,"工項類","纖維水泥板/矽酸鈣板","搖籃到大門",2014,"kg",1.12,"未載明","產品碳足跡資訊網","交通部鐵道局南部工程分局"]
[1095,"工項類","砂、石","搖籃到大門",2023,"kg",0.005,"未載明","高公局國道4號臺中環線豐原潭子段工程碳盤查"," 交通部鐵道局中部工程分局"]
[1096,"工項類","固定式圍籬","未載明",2020,"公尺",3.16,"未載明","鐵道局南部工程分局-南迴計畫碳管理暨碳足跡盤查服務報告"," 交通部鐵道局中部工程分局"]
[1097,"工項類","鐵絲網柵欄","未載明",2020,"公尺",0.9,"未載明","鐵道局南部工程分局-南迴計畫碳管理暨碳足跡盤查服務報告"," 交通部鐵道局中部工程分局"]
[1098,"工項類","原木(未乾燥防腐處理)-軟木","搖籃到工地",2017,"m3",35.39,"未載明","低碳建築聯盟","內政部建築研究所"]
[1099,"工項類","原木(未乾燥防腐處理)-硬木","搖籃到工地",2017,"m3",43.48,"未載明","低碳建築聯盟","內政部建築研究所"]
[1100,"工項類","原竹(未乾燥防腐處理)-竹","搖籃到工地",2017,"m3",37.41,"未載明","低碳建築聯盟","內政部建築研究所"]
[1101,"工項類","木竹類製材(人工乾燥防腐\n處理)-軟木","搖籃到工地",2017,"m3",89.94,"未載明","低碳建築聯盟","內政部建築研究所"]
[1102,"工項類","木竹類製材(人工乾燥防腐處理)-硬木","搖籃到工地",2017,"m3",274.55,"未載明","低碳建築聯盟","內政部建築研究所"]
[1103,"工項類","木竹類製材(人工乾燥防腐處理)-竹","搖籃到工地",2017,"m3",174.22,"未載明","低碳建築聯盟","內政部建築研究所"]
[1104,"工項類","竹籐編織","搖籃到工地",2017,"m3",175.38,"未載明","低碳建築聯盟","內政部建築研究所"]
[1105,"工項類","竹籐編織(2.5mm) ","搖籃到工地",2017,"m3",1.1,"未載明","低碳建築聯盟","內政部建築研究所"]
[1106,"工項類","1:1 水泥砂漿粉刷 2cm 厚","搖籃到工地",2017,"m2",19.49,"未載明","低碳建築聯盟","內政部建築研究所","09220"]
[1107,"工項類","1:2 水泥砂漿粉刷 2cm 厚","搖籃到工地",2017,"m2",12.86,"未載明","低碳建築聯盟","內政部建築研究所","09220"]
[1108,"工項類","1:3 水泥砂漿粉刷 2cm 厚","搖籃到工地",2017,"m2",9.05,"未載明","低碳建築聯盟","內政部建築研究所","09220"]
[1109,"工項類","貼磁磚外裝","搖籃到工地",2018,"m2",28.7,"未載明","低碳建築聯盟","內政部建築研究所"]
[1110,"工項類","乾式石材外裝","搖籃到工地",2018,"m2",12.79,"未載明","低碳建築聯盟","內政部建築研究所"]
[1111,"工項類","RC 外牆 15cm","搖籃到工地",2021,"m2",73.67,"未載明","低碳建築聯盟","內政部建築研究所"]
[1112,"工項類","RC 外牆 18cm","搖籃到工地",2021,"m2",83.5,"未載明","低碳建築聯盟","內政部建築研究所"]
[1113,"工項類","清水混凝土外牆 20cm","搖籃到工地",2021,"m2",102.15,"未載明","低碳建築聯盟","內政部建築研究所"]
[1114,"工項類","預鑄混凝土外牆 15cm","搖籃到工地",2021,"m2",80.47,"未載明","低碳建築聯盟","內政部建築研究所"]
[1115,"工項類","空心磚牆","搖籃到工地",2018,"m2",23.59,"未載明","低碳建築聯盟","內政部建築研究所"]
[1116,"工項類","1B 磚牆","搖籃到工地",2018,"m2",106.79,"未載明","低碳建築聯盟","內政部建築研究所"]
[1117,"工項類","洗石子/斬石子/抿石子外裝","搖籃到工地",2018,"m2",15.98,"未載明","低碳建築聯盟","內政部建築研究所"]
[1118,"工項類","水泥砂漿1:3，第 1 型水泥","未載明","未載明","m3",49.1908,"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署","04061"]
[1119,"工項類","洗石子，宜蘭石","未載明","未載明","kg",0.103,"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署"]
[1120,"工項類","水泥砂漿，1:3","搖籃到大門",2015,"M3",437,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","04061"]
[1121,"工項類","水泥砂漿，1:3，勾縫","搖籃到大門",2015,"式",10.9496366825,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","04061"]
[1122,"工項類","實木地板-軟木 ","搖籃到工地",2017,"m3",195.13,"未載明","低碳建築聯盟","內政部建築研究所"]
[1123,"工項類","實木地板-硬木","搖籃到工地",2017,"m3",394.49,"未載明","低碳建築聯盟","內政部建築研究所"]
[1124,"工項類","實木地板-竹","搖籃到工地",2017,"m3",292.28,"未載明","低碳建築聯盟","內政部建築研究所"]
[1125,"工項類","實木地板(2cm)-軟木","搖籃到工地",2017,"m2",3.9,"未載明","低碳建築聯盟","內政部建築研究所"]
[1126,"工項類","實木地板(2cm)-硬木","搖籃到工地",2017,"m2",7.89,"未載明","低碳建築聯盟","內政部建築研究所"]
[1127,"工項類","實木地板(2cm)-竹","搖籃到工地",2017,"m2",5.84,"未載明","低碳建築聯盟","內政部建築研究所"]
[1128,"工項類","實木皮木芯板(天然木化粧合板、複合木質、海島型木地板、木芯板)","搖籃到工地",2017,"m3",382.75,"未載明","低碳建築聯盟","內政部建築研究所"]
[1129,"工項類","實木皮木芯板(天然木化粧合板、複合木質、海島型木地板、木芯板)(6 分板，18mm)","搖籃到工地",2017,"m3",6.89,"未載明","低碳建築聯盟","內政部建築研究所"]
[1130,"工項類","合板 ","搖籃到工地",2017,"m3",185.43,"未載明","低碳建築聯盟","內政部建築研究所"]
[1131,"工項類","合板(18mm) ","搖籃到工地",2017,"m2",3.34,"未載明","低碳建築聯盟","內政部建築研究所"]
[1132,"工項類","單板層積材(LVL)","搖籃到工地",2017,"m3",84,"未載明","低碳建築聯盟","內政部建築研究所"]
[1133,"工項類","單板層積材(LVL)(6分板18mm)","搖籃到工地",2017,"m2",1.51,"未載明","低碳建築聯盟","內政部建築研究所"]
[1134,"工項類","集成材(集層材、膠合木)","搖籃到工地",2017,"m3",159.66,"未載明","低碳建築聯盟","內政部建築研究所"]
[1135,"工項類","集成材(集層材、膠合木)(6分板18mm)","搖籃到工地",2017,"m2",2.88,"未載明","低碳建築聯盟","內政部建築研究所"]
[1136,"工項類","高密度粒片板(塑合板，OSB定向粒片板、HDF，密度850kg/m3，18mm)","搖籃到工地",2017,"m2",17.56,"未載明","低碳建築聯盟","內政部建築研究所"]
[1137,"工項類","中密度粒片板(密集板，mDF，密度 700kg/m3，18mm)","搖籃到工地",2017,"m2",14.47,"未載明","低碳建築聯盟","內政部建築研究所"]
[1138,"工項類","石膏板","搖籃到大門",2017,"kg",0.51,"未載明","產品碳足跡資訊網","內政部建築研究所","09250"]
[1139,"工項類","石膏板(9mm) ","搖籃到工地",2017,"m2",1.93,"未載明","低碳建築聯盟","內政部建築研究所","09250"]
[1140,"工項類","石膏板(12mm) ","搖籃到工地",2017,"m2",2.58,"未載明","低碳建築聯盟","內政部建築研究所","09250"]
[1141,"工項類","石膏板(15mm) ","搖籃到工地",2017,"m2",3.08,"未載明","低碳建築聯盟","內政部建築研究所","09250"]
[1142,"工項類","玻璃帷幕牆","搖籃到工地",2018,"m2",69.62,"未載明","低碳建築聯盟","內政部建築研究所"]
[1143,"工項類","鋁金屬帷幕牆","搖籃到工地",2018,"m2",58.12,"未載明","低碳建築聯盟","內政部建築研究所"]
[1144,"工項類","花崗岩帷幕牆","搖籃到工地",2018,"m2",39.95,"未載明","低碳建築聯盟","內政部建築研究所"]
[1145,"工項類","鋁帷幕框架構造（陽極或氟碳烤漆）","搖籃到工地",2018,"m2",30.32,"未載明","低碳建築聯盟","內政部建築研究所"]
[1146,"工項類","不鏽鋼帷幕框架構造","搖籃到工地",2018,"m2",46.63,"未載明","低碳建築聯盟","內政部建築研究所"]
[1147,"工項類","塑鋼帷幕構造（含補強鐵件）","搖籃到工地",2018,"m2",24.06,"未載明","低碳建築聯盟","內政部建築研究所"]
[1148,"工項類","抓釘式帷幕框架","搖籃到工地",2018,"m2",46.63,"未載明","低碳建築聯盟","內政部建築研究所"]
[1149,"工項類","人工拆除，鋼筋混凝土","搖籃到大門",2023,"M3",12.4613236364,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02220"]
[1150,"工項類","構造物開挖，深度＜5m，機械挖","未載明",2022,"M3",1.325,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02316"]
[1151,"工項類","鑽孔及灌漿，鑽孔(取岩心)","未載明",2022,"孔",37.1112,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02344"]
[1152,"工項類","土質改良，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02361"]
[1153,"工項類","土質改良，化學灌漿","搖籃到大門",2022,"式",36282.7044117129,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02361"]
[1154,"工項類","構造物回填，原材料回填及夯實","未載明",2022,"M3",10.23,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02317"]
[1155,"工項類","機械切割，路面挖除，瀝青混凝土","搖籃到大門",2023,"M",0.2845712212,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02220"]
[1156,"工項類","切割瀝青混凝土或無筋混凝土，5cm≦切割 深度＜10cm","搖籃到大門",2023,"M",0.284571221,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02220"]
[1157,"工項類","構造物開挖，深度＜5m，(機械挖配合人工 挖，未含抽水)，未含運費","未載明",2022,"B.M3",1.325,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02316"]
[1158,"工項類","選擇材料回填，級配粒料，碎石級配底層","未載明",2022,"C.M3",6.398,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02319"]
[1159,"工項類","污水管線施工，背填灌漿","未載明",2022,"M3",94.495,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1160,"工項類","污水管線施工，接頭處理費","未載明",2021,"kg",0.024255,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1161,"工項類","污水管線施工，安全措施費及排水費","搖籃到大門",2023,"式",39.5697272727,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1162,"工項類","污水管線施工，原有人孔RC打除及防水設施","搖籃到大門",2023,"式",12.4613236364,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1163,"工項類","圓形鋼管工作井，排水費","搖籃到大門",2023,"處",39.5697272727,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1164,"工項類","圓形鋼管工作井，工作井內通風及安全設施","搖籃到大門",2023,"式",29.0178,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1165,"工項類","圓形鋼管工作井，標稱直徑1590mm，鋼管材料費(含折舊)","搖籃到大門",2013,"M",731.1307478791,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1166,"工項類","圓形鋼管工作井，標稱直徑1890mm，鋼管材料費(含折舊)","搖籃到大門",2013,"M",870.1289889207,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1167,"工項類","圓形鋼管工作井，標稱直徑2090mm，鋼管材料費(含折舊)","搖籃到大門",2013,"M",1281.2548974239,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1168,"工項類","圓形鋼管工作井，標稱直徑2590mm，鋼管材料費(含折舊)","搖籃到大門",2013,"M",2181.3457294136,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1169,"工項類","圓形鋼管工作井，標稱直徑3090mm，鋼管材料費(含折舊)","搖籃到大門",2013,"M",3310.3203316519,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1170,"工項類","圓形鋼管工作井，標稱直徑3290mm，鋼管材料費(含折舊)","搖籃到大門",2013,"M",3526.5398177167,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1171,"工項類","圓形鋼管工作井，標稱直徑3590mm，鋼管材料費(含折舊)","搖籃到大門",2013,"M",3714.3804962355,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1172,"工項類","圓形鋼管工作井，標稱管徑≦300mm，鏡面 工處理","搖籃到大門",2013,"處",52.5533029175,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1173,"工項類","圓形鋼管工作井，標稱管徑≦300mm，到達 口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1174,"工項類","圓形鋼管工作井，標稱管徑≦300mm，推進 口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1175,"工項類","圓形鋼管工作井，300mm<標稱管徑≦600mm，鏡面工處理","搖籃到大門",2013,"處",97.5989911325,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1176,"工項類","圓形鋼管工作井，300mm<標稱管徑≦600mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1177,"工項類","圓形鋼管工作井，300mm<標稱管徑≦600mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1178,"工項類","圓形鋼管工作井，600mm<標稱管徑≦900mm，鏡面工處理","搖籃到大門",2013,"處",600.6091762,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1179,"工項類","圓形鋼管工作井，600mm<標稱管徑≦900mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1180,"工項類","圓形鋼管工作井，600mm<標稱管徑≦900mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1181,"工項類","圓形鋼管工作井，900mm<標稱管徑≦1200mm，鏡面工處理","搖籃到大門",2013,"處",1824.3503727075,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1182,"工項類","圓形鋼管工作井，900mm<標稱管徑≦1200mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1183,"工項類","圓形鋼管工作井，900mm<標稱管徑≦1200mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1184,"工項類","圓形鋼管工作井，1200mm<標稱管徑≦1500mm，鏡面工處理","搖籃到大門",2013,"處",4084.14239816,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1185,"工項類","圓形鋼管工作井，1200mm<標稱管徑≦1500mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1186,"工項類","圓形鋼管工作井，1200mm<標稱管徑≦1500mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1187,"工項類","圓形鋼管工作井，1500mm<標稱管徑≦1800mm，鏡面工處理","搖籃到大門",2013,"處",7695.3050700625,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1188,"工項類","圓形鋼管工作井，1500mm<標稱管徑≦1800mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1189,"工項類","圓形鋼管工作井，1500mm<標稱管徑≦1800mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1190,"工項類","圓形鋼管工作井，1800mm<標稱管徑≦2100mm，鏡面工處理","搖籃到大門",2013,"處",12973.158205920001,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1191,"工項類","圓形鋼管工作井，1800mm<標稱管徑≦2100mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1192,"工項類","圓形鋼管工作井，1800mm<標稱管徑≦2100mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1193,"工項類","圓形鋼管工作井，2100mm<標稱管徑≦2400mm，鏡面工處理","搖籃到大門",2013,"處",14594.80298166,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1194,"工項類","圓形鋼管工作井，2100mm<標稱管徑≦2400mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1195,"工項類","圓形鋼襯板工作井，背填灌漿","未載明",2022,"M3",94.495,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1196,"工項類","圓形鋼襯板工作井，工作井內通風及安全設施","搖籃到大門",2023,"式",29.0178,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1197,"工項類","圓形鋼襯板工作井，標稱管徑≦300mm，到 達口，鏡面工處理","搖籃到大門",2013,"處",52.5533029175,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1198,"工項類","圓形鋼襯板工作井，標稱管徑≦300mm，到 達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1199,"工項類","圓形鋼襯板工作井，標稱管徑≦300mm，推 進口，鏡面工處理","搖籃到大門",2013,"處",52.5533029175,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1200,"工項類","圓形鋼襯板工作井，標稱管徑≦300mm，推 進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1201,"工項類","圓形鋼襯板工作井，300mm<標稱管徑≦600mm，鏡面工處理","搖籃到大門",2013,"處",97.5989911325,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1202,"工項類","圓形鋼襯板工作井，300mm<標稱管徑≦600mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1203,"工項類","圓形鋼襯板工作井，300mm<標稱管徑≦600mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1204,"工項類","圓形鋼襯板工作井，600mm<標稱管徑≦900mm，鏡面工處理","搖籃到大門",2013,"處",600.6091762,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1205,"工項類","圓形鋼襯板工作井，600mm<標稱管徑≦900mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1206,"工項類","圓形鋼襯板工作井，600mm<標稱管徑≦900mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1207,"工項類","圓形鋼襯板工作井，900mm<標稱管徑≦1200mm，鏡面工處理","搖籃到大門",2013,"處",1824.3503727075,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1208,"工項類","圓形鋼襯板工作井，900mm<標稱管徑≦1200mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1209,"工項類","圓形鋼襯板工作井，900mm<標稱管徑≦1200mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1210,"工項類","圓形鋼襯板工作井，1200mm<標稱管徑≦1500mm，鏡面工處理","搖籃到大門",2013,"處",4084.14239816,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1211,"工項類","圓形鋼襯板工作井，1200mm<標稱管徑≦1500mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1212,"工項類","圓形鋼襯板工作井，1200mm<標稱管徑≦1500mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1213,"工項類","圓形鋼襯板工作井，1500mm<標稱管徑≦1800mm，鏡面工處理","搖籃到大門",2013,"處",7695.3050700625,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1214,"工項類","圓形鋼襯板工作井，1500mm<標稱管徑≦1800mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1215,"工項類","圓形鋼襯板工作井，1500mm<標稱管徑≦1800mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1216,"工項類","圓形鋼襯板工作井，1800mm<標稱管徑≦2100mm，鏡面工處理","搖籃到大門",2013,"處",12973.158205920001,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1217,"工項類","圓形鋼襯板工作井，1800mm<標稱管徑≦2100mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1218,"工項類","圓形鋼襯板工作井，1800mm<標稱管徑≦2100mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1219,"工項類","圓形鋼襯板工作井，2100mm<標稱管徑≦2400mm，鏡面工處理","搖籃到大門",2013,"處",14594.80298166,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1220,"工項類","圓形鋼襯板工作井，2100mm<標稱管徑≦2400mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1221,"工項類","圓形鋼襯板工作井，2100mm<標稱管徑≦2400mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1222,"工項類","橢圓形鋼襯板工作井，排水費","搖籃到大門",2023,"式",39.5697272727,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1223,"工項類","橢圓形鋼襯板工作井，背填灌漿","未載明",2022,"M3",94.495,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1224,"工項類","橢圓形鋼襯板工作井，工作井內通風及安全設施","搖籃到大門",2023,"式",29.0178,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1225,"工項類","橢圓形鋼襯板工作井，標稱管徑≦300mm， 鏡面工處理","搖籃到大門",2013,"處",52.5533029175,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1226,"工項類","橢圓形鋼襯板工作井，標稱管徑≦300mm， 到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1227,"工項類","橢圓形鋼襯板工作井，300mm<標稱管徑≦600mm，鏡面工處理","搖籃到大門",2013,"處",97.5989911325,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1228,"工項類","橢圓形鋼襯板工作井，300mm<標稱管徑≦600mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1229,"工項類","橢圓形鋼襯板工作井，300mm<標稱管徑≦600mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1230,"工項類","橢圓形鋼襯板工作井，600mm<標稱管徑≦900mm，鏡面工處理","搖籃到大門",2013,"處",600.6091762,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1231,"工項類","橢圓形鋼襯板工作井，600mm<標稱管徑≦900mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1232,"工項類","橢圓形鋼襯板工作井，600mm<標稱管徑≦900mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1233,"工項類","橢圓形鋼襯板工作井，900mm<標稱管徑≦1200mm，鏡面工處理","搖籃到大門",2013,"處",1824.3503727075,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1234,"工項類","橢圓形鋼襯板工作井，900mm<標稱管徑≦1200mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1235,"工項類","橢圓形鋼襯板工作井，900mm<標稱管徑≦1200mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1236,"工項類","橢圓形鋼襯板工作井，1200mm<標稱管徑≦1500mm，鏡面工處理","搖籃到大門",2013,"處",4084.14239816,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1237,"工項類","橢圓形鋼襯板工作井，1200mm<標稱管徑≦1500mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1238,"工項類","橢圓形鋼襯板工作井，1200mm<標稱管徑≦1500mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1239,"工項類","橢圓形鋼襯板工作井，1500mm<標稱管徑≦1800mm，鏡面工處理","搖籃到大門",2013,"處",7695.3050700625,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1240,"工項類","橢圓形鋼襯板工作井，1500mm<標稱管徑≦1800mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1241,"工項類","橢圓形鋼襯板工作井，1500mm<標稱管徑≦1800mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1242,"工項類","橢圓形鋼襯板工作井，1800mm<標稱管徑≦2100mm，鏡面工處理","搖籃到大門",2013,"處",12973.158205920001,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1243,"工項類","橢圓形鋼襯板工作井，1800mm<標稱管徑≦2100mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1244,"工項類","橢圓形鋼襯板工作井，1800mm<標稱管徑≦2100mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1245,"工項類","橢圓形鋼襯板工作井，2100mm<標稱管徑≦2400mm，鏡面工處理","搖籃到大門",2013,"處",14594.80298166,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1246,"工項類","橢圓形鋼襯板工作井，2100mm<標稱管徑≦2400mm，到達口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1247,"工項類","橢圓形鋼襯板工作井，2100mm<標稱管徑≦2400mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1248,"工項類","橢圓形鋼襯板工作井，2100mm<標稱管徑≦2400mm，推進口，藥劑處理","搖籃到大門",2017,"M3",394,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1249,"工項類","圓形鋼管工作井，標稱直徑2090mm，3M <埋設深度≦4M","未載明","未載明","M3",{"v":10383.6589,"d":"10,383.66"},"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1250,"工項類","圓形鋼管工作井，標稱直徑2090mm，4M <埋設深度≦5M","未載明","未載明","M3",{"v":12390.9981,"d":"12,391.00"},"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1251,"工項類","圓形鋼管工作井，標稱直徑2090mm，5M <埋設深度≦6M","未載明","未載明","M3",{"v":14398.3373,"d":"14,398.34"},"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1252,"工項類","圓形鋼管工作井，標稱直徑2090mm，6M <埋設深度≦7M","未載明","未載明","M3",{"v":16405.6765,"d":"16,405.68"},"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1253,"工項類","鋼套管推進，背填灌漿","未載明",2022,"M3",94.495,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1254,"工項類","產品，污水管線附屬工作，圓形預鑄污水人孔（P900型），頂部平板","搖籃到大門",2017,"個",68.5209240491,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[1255,"工項類","污水下水道用戶接管工程埋設施工，接頭處理費","未載明",2021,"式",0.024255,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02534"]
[1256,"工項類","污水管線附屬工作，A型圓形預鑄污水人孔， 標稱直徑1200mm，底座，含安裝","搖籃到大門",2017,"個",554,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[1257,"工項類","污水管線附屬工作，圓形預鑄污水人孔(P1200型)，1200mm底座直管，含安裝","搖籃到大門",2017,"個",367.6883654213,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","M02532"]
[1258,"工項類","污水下水道用戶接管工程埋設施工，活套式接頭處理","未載明",2021,"式",0.024255,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02534"]
[1259,"工項類","污水下水道用戶接管工程埋設施工，膠合式 接頭處理","未載明",2021,"式",0.024255,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02534"]
[1260,"工項類","順T型接頭，聚氯乙烯塑膠硬質管，標稱管徑150x100mm，含連接及安裝","搖籃到大門",2021,"只",2.99,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02534"]
[1261,"工項類","污水管線施工，接頭處理費","未載明",2021,"式",0.024255,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02531"]
[1262,"工項類","廢方處理","未載明",2022,"M3",4.791,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02323"]
[1263,"工項類","餘方自行處理(含水土保持)，總重15t傾卸貨 車","未載明",2022,"B.M3",46.069,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02323"]
[1264,"工項類","臨時擋土樁設施，鋼軌樁 37kg/m，L=5m，打拔","未載明",2022,"支",2.415,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02255"]
[1265,"工項類","臨時擋土樁設施，鋼軌樁 37kg/m，L=6m，打拔","未載明",2022,"支",2.898,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02255"]
[1266,"工項類","臨時擋土樁設施，鋼軌樁 37kg/m，L=7m，打拔","未載明",2022,"支",3.381,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02255"]
[1267,"工項類","臨時擋土樁設施，鋼軌樁 37kg/m，L=8m，打拔","未載明",2022,"支",3.864,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02255"]
[1268,"工項類","臨時擋土樁設施，鋼軌樁 37kg/m，L=9m，打拔","未載明",2022,"支",4.347,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02255"]
[1269,"工項類","臨時擋土樁設施，鋼軌樁 37kg/m，L=13m， 打拔","未載明",2022,"支",6.279,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02255"]
[1270,"工項類","臨時擋土樁設施，門型擋土","未載明",2022,"M2",11.109,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02255"]
[1271,"工項類","臨時擋土支撐工法，木橫擋及支撐","未載明",2022,"M2",1.202,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02256"]
[1272,"工項類","臨時擋土支撐工法，H型鋼橫擋及支撐","未載明",2022,"組",39.637,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02256"]
[1273,"工項類","開挖支撐及保護，水平支撐","未載明",2022,"組",39.637,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02260"]
[1274,"工項類","級配粒料底層，碎石級配","未載明","未載明","m3",6.428,"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署","02726"]
[1275,"工項類","級配粒料底層，碎石級配","未載明",2022,"M3",5.74,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02726"]
[1276,"工項類","預鑄鋼筋混凝土基座(埋管用)，D=600mm管用","搖籃到大門",2023,"座",15.6506952,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02610"]
[1277,"工項類","預鑄鋼筋混凝土基座(埋管用)，D=800mm管用","搖籃到大門",2023,"座",20.1205644,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02610"]
[1278,"工項類","預鑄鋼筋混凝土基座(埋管用)，D=1000mm 管用","搖籃到大門",2023,"座",25.2111426,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02610"]
[1279,"工項類","預鑄鋼筋混凝土基座(埋管用)，D=1200mm 管用","搖籃到大門",2023,"座",26.3908509,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02610"]
[1280,"工項類","瀝青混凝土鋪面，(第 1 類型，密級配)，黏度 AC-10，拌和廠交貨","未載明","未載明","t",93.6889,"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署","02742"]
[1281,"工項類","瀝青混凝土鋪面，(第 1 類型， 密級配)，黏度 AC-20，工地交貨","未載明","未載明","t",68.7076,"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署","02742"]
[1282,"工項類","瀝青混凝土鋪面，(第 1 類型，密級配)，粗粒料 19.0mm，拌和廠交貨","未載明","未載明","t",78.6783,"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署","02742"]
[1283,"工項類","瀝青混凝土鋪面，(第 1 類型，密級配)，粗粒料 19.0mm，針入度 60~70","未載明","未載明","m3",171.1707,"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署","02742"]
[1284,"工項類","透水性鋪面，多孔性瀝青混凝土","未載明","未載明","t",67.3417,"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署","02798"]
[1285,"工項類","瀝青混凝土舖面，再生粒料","未載明",2022,"M3",5.74,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02966"]
[1286,"工項類","瀝青混凝土面層刨除，廢方處理","未載明",2022,"M3",1.042,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02961"]
[1287,"工項類","透心骨材","未載明",2021,"M2",3.328665,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02778"]
[1288,"工項類","道路施工及復舊，緣石及側溝","未載明",2022,"M",8.182,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02952"]
[1289,"工項類","結構用混凝土，人工拌合，(樹脂水泥基座)","未載明",2022,"M3",425.187,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","03310"]
[1290,"工項類","透水性鋪面，塊狀及鏤空狀，植草磚，5≦面層厚＜10cm","未載明","未載明","m2",27.048,"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署","02778"]
[1291,"工項類","人行道面層鋪面磚(高壓)","未載明","未載明","m2",49.5368,"未載明","成功大學永續運輸基礎設施管理實驗室(營建工程碳足跡資料庫)","內政部國土管理署","02778"]
[1292,"工項類","環境保護，空氣污染防制，覆蓋物","搖籃到大門",2023,"組",295.24,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[1293,"工項類","袪水，臨時排水","搖籃到大門",2023,"式",39.5697272727,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02240"]
[1294,"工項類","產品，基本產品需求，滑材費","搖籃到大門",2020,"式",15.94025,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[1295,"工項類","產品，合成橡膠防震墊，厚3mm","未載明",2021,"M2",9.3381255,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","03150"]
[1296,"工項類","原有化糞池處理，容量<10戶，抽乾費","未載明","未載明","座",0.4710681818,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02534"]
[1297,"工項類","原有化糞池處理，10戶≦容量<20戶，抽乾費","未載明","未載明","座",7.6548579545,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02534"]
[1298,"工項類","環境保護，空氣污染防制，覆蓋物","搖籃到大門",2023,"組",295.24,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署"]
[1299,"工項類","擠壓式彈性填縫帶，(寬55mm，厚20mm)，600～1000mm鋼筋混凝土管排水用","未載明",2021,"M",3.7148,"經ARES第三方查驗證","下水道工程減碳作業參考指引","內政部國土管理署","02610"]
[1300,"工項類","機械拆除，無筋混凝土，未含運費","未載明",2022,"m3",{"v":13.641,"d":"13.64"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1301,"工項類","土方工作，填方","未載明",2022,"m3",{"v":1.339,"d":"1.34"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1302,"工項類","土方工作，遠運利用","未載明",2022,"m3",{"v":3.908,"d":"3.91"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1303,"工項類","棄土，餘方近運利用","未載明",2022,"m3",{"v":1.042,"d":"1.04"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1304,"工項類","臨時擋土樁設施，打拔(不分類)","未載明",2022,"m",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02255"]
[1305,"工項類","臨時擋土樁設施，鋼軌樁，打拔","未載明",2022,"m",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02255"]
[1306,"工項類","臨時擋土樁設施，鋼板樁，L=13m，打拔","未載明",2022,"m",{"v":14.5,"d":"14.50"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02255"]
[1307,"工項類","臨時擋土樁設施，鋼板樁，L=13m，打拔","未載明",2022,"片",{"v":5.8,"d":"5.80"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02255"]
[1308,"工項類","臨時擋土支撐工法，H型鋼橫擋及支撐，裝拆","未載明",2022,"m2",{"v":39.637,"d":"39.64"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02256"]
[1309,"工項類","自來水用塑膠管，聚氯乙烯塑膠管(不分類)","未載明",2022,"m",{"v":11.3104,"d":"11.31"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02511"]
[1310,"工項類","自來水用塑膠管，聚氯乙烯塑膠管，D=50mm(t=4.1mm)","未載明",2022,"m",{"v":2.693,"d":"2.69"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02511"]
[1311,"工項類","自來水用塑膠管，聚氯乙烯塑膠管，D=75mm(t=5.5mm)","未載明",2022,"m",{"v":5.285,"d":"5.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02511"]
[1312,"工項類","自來水用塑膠管，聚氯乙烯塑膠管，D=100mm(t=6.6mm)","未載明",2022,"m",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02511"]
[1313,"工項類","自來水用塑膠管，聚氯乙烯塑膠管，D=150mm(t=8.9mm)","未載明",2022,"m",{"v":16.082,"d":"16.08"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02511"]
[1314,"工項類","自來水用塑膠管，聚氯乙烯塑膠管，D=200mm(t=10.3mm)","未載明",2022,"m",24.31,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02511"]
[1315,"工項類","自來水用塑膠管，高密度聚乙烯管，D=200mm(t=11.9mm)","未載明",2022,"m",17.28,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02511"]
[1316,"工項類","污水管管材，聚氯乙烯塑膠硬質管，D=200mm(t=10.3mm) ","未載明",2022,"m",24.31,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02511"]
[1317,"工項類","排水管溝，塑膠管(不分類) ","未載明",2022,"m",11.31,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02601"]
[1318,"工項類","排水管溝，塑膠管，D=100mm(t=6.6mm) ","未載明",2022,"m",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02601"]
[1319,"工項類","排水管溝，塑膠管，D=150mm(t=8.9mm) ","未載明",2022,"m",{"v":16.082,"d":"16.08"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02601"]
[1320,"工項類","排水管溝，塑膠管，D=200mm(t=10.3mm) ","未載明",2022,"m",24.31,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02601"]
[1321,"工項類","排水管涵，聚氯乙烯排水管，D=50mm(t=4.1mm)","未載明",2022,"m",{"v":2.693,"d":"2.69"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1322,"工項類","排水管涵，聚氯乙烯排水管，D=75mm(t=5.5mm)","未載明",2022,"m",{"v":5.285,"d":"5.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1323,"工項類","排水管涵，聚氯乙烯排水管，D=100mm(t=6.6mm)","未載明",2022,"m",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1324,"工項類","排水管涵，聚氯乙烯排水管，D=150mm(t=8.9mm)","未載明",2022,"m",{"v":16.082,"d":"16.08"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1325,"工項類","排水管涵，聚氯乙烯排水管，D=200mm(t=10.3mm)","未載明",2022,"m",24.31,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1326,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)(不分類)","未載明",2022,"m",{"v":11.3104,"d":"11.31"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署",15105]
[1327,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=50mm(t=4.1mm)","未載明",2022,"m",{"v":2.693,"d":"2.69"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署",15105]
[1328,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=75mm(t=5.5mm)","未載明",2022,"m",{"v":5.285,"d":"5.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署",15105]
[1329,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=100mm(t=6.6mm)","未載明",2022,"m",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署",15105]
[1330,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=150mm(t=8.9mm)","未載明",2022,"m",{"v":16.082,"d":"16.08"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署",15105]
[1331,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B管厚管)，D=200mm(t=10.3mm)","未載明",2022,"m",24.31,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署",15105]
[1332,"工項類","邊坡穩定水平排水管，塑膠管(不分類)","未載明",2022,"m",{"v":11.3104,"d":"11.31"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02377"]
[1333,"工項類","邊坡穩定水平排水管，塑膠管，D=50mm(t=4.1mm)","未載明",2022,"m",{"v":2.693,"d":"2.69"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02377"]
[1334,"工項類","邊坡穩定水平排水管，塑膠管，D=75mm(t=5.5mm)","未載明",2022,"m",{"v":5.285,"d":"5.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02377"]
[1335,"工項類","邊坡穩定水平排水管，塑膠管，D=100mm(t=6.6mm)","未載明",2022,"m",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02377"]
[1336,"工項類","邊坡穩定水平排水管，塑膠管，D=150mm(t=8.9mm)","未載明",2022,"m",{"v":16.082,"d":"16.08"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02377"]
[1337,"工項類","邊坡穩定水平排水管，塑膠管，D=200mm(t=10.3mm)","未載明",2022,"m",24.31,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02377"]
[1338,"工項類","拋石","未載明",2022,"m3",{"v":5.352,"d":"5.35"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02381"]
[1339,"工項類","坡面工(不分類)","未載明",2022,"m2",{"v":49.415,"d":"49.42"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02385"]
[1340,"工項類","級配粒料基層，碎石級配，鋪設及滾壓","未載明",2022,"m3",5.74,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02722"]
[1341,"工項類","污水管管材，鋼筋混凝土管 (不分類)","未載明",2022,"m",205.49,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02533"]
[1342,"工項類","污水管管材，鋼筋混凝土管(不分類，L=2.4m) ","未載明",2022,"支",{"v":493.176,"d":"493.18"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02533"]
[1343,"工項類","污水管管材，鋼筋混凝土 管，D=600mm","未載明",2022,"m",{"v":151.338,"d":"151.34"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02533"]
[1344,"工項類","污水管管材，鋼筋混凝土 管，D=600mm(L=2.4m)","未載明",2022,"支",{"v":363.212,"d":"363.21"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02533"]
[1345,"工項類","污水管管材，鋼筋混凝土 管，D=800mm","未載明",2022,"m",{"v":205.708,"d":"205.71"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02533"]
[1346,"工項類","污水管管材，鋼筋混凝土 管，D=800mm(L=2.4m)","未載明",2022,"支",{"v":493.7,"d":"493.70"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02533"]
[1347,"工項類","污水管管材，鋼筋混凝土 管，D=1000mm","未載明",2022,"m",{"v":259.424,"d":"259.42"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02533"]
[1348,"工項類","污水管管材，鋼筋混凝土 管，D=1000mm(L=2.4m)","未載明",2022,"支",{"v":622.617,"d":"622.62"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02533"]
[1349,"工項類","管涵，鋼筋混凝土管 B 型(不分類)","未載明",2022,"m",205.49,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1350,"工項類","管涵，鋼筋混凝土管 B 型(不分類，L=2.4m) ","未載明",2022,"個",{"v":493.176,"d":"493.18"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1351,"工項類","管涵，鋼筋混凝土管 B 型，D=600mm ","未載明",2022,"m",{"v":151.338,"d":"151.34"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1352,"工項類","管涵，鋼筋混凝土管 B 型，D=600mm(L=2.4m) ","未載明",2022,"個",{"v":363.212,"d":"363.21"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1353,"工項類","管涵，鋼筋混凝土管 B 型，D=800mm","未載明",2022,"m",{"v":205.708,"d":"205.71"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1354,"工項類","管涵，鋼筋混凝土管 B 型，D=800mm(L=2.4m)","未載明",2022,"個",{"v":493.7,"d":"493.70"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1355,"工項類","管涵，鋼筋混凝土管 B 型，D=1000mm","未載明",2022,"m",{"v":259.424,"d":"259.42"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1356,"工項類","管涵，鋼筋混凝土管B型，D=1000mm(L=2.4m)","未載明",2022,"個",{"v":622.617,"d":"622.62"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1357,"工項類","排水管涵，鋼筋混凝土管(不分類)","未載明",2022,"m",205.49,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1358,"工項類","排水管涵，鋼筋混凝土管(不分類，L=2.4m)","未載明",2022,"支",{"v":493.176333333333,"d":"493.18"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1359,"工項類","排水管涵，鋼筋混凝土管(B型)，D=600mm","未載明",2022,"m",{"v":151.338,"d":"151.34"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1360,"工項類","排水管涵，鋼筋混凝土管(B型)，D=600mm(L=2.4m)","未載明",2022,"支",{"v":363.212,"d":"363.21"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1361,"工項類","排水管涵，鋼筋混凝土管(B型)，D=800mm","未載明",2022,"m",{"v":205.708,"d":"205.71"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1362,"工項類","排水管涵，鋼筋混凝土管(B型)，D=800mm(L=2.4m)","未載明",2022,"支",{"v":493.7,"d":"493.70"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1363,"工項類","排水管涵，鋼筋混凝土管(B型)，D=1000mm","未載明",2022,"m",{"v":259.424,"d":"259.42"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1364,"工項類","排水管涵，鋼筋混凝土管(B型)，D=1000mm(L=2.4m)","未載明",2022,"支",{"v":622.617,"d":"622.62"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02610"]
[1365,"工項類","預力混凝土基樁(不分類，B種)","未載明",2022,"m",{"v":79.5805,"d":"79.58"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02457"]
[1366,"工項類","預力混凝土基樁，D=300mm，B種","未載明",2022,"m",{"v":35.604,"d":"35.60"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02457"]
[1367,"工項類","預力混凝土基樁，D=500mm，B種","未載明",2022,"m",{"v":66.232,"d":"66.23"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02457"]
[1368,"工項類","預力混凝土基樁，D=600mm，B種","未載明",2022,"m",{"v":85.168,"d":"85.17"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02457"]
[1369,"工項類","預力混凝土基樁，D=800mm，B種","未載明",2022,"m",{"v":131.318,"d":"131.32"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02457"]
[1370,"工項類","預力混凝土基樁，D=800mm，B種，L=12m","未載明",2022,"支",{"v":1626.521,"d":"1626.52"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02457"]
[1371,"工項類","鑽掘樁(不分類)","未載明",2022,"m",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1372,"工項類","微型樁(不分類，D=30cm)","未載明",2022,"組",{"v":883.429333333333,"d":"883.43"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1373,"工項類","微型樁，D=30cm，L=4.5m","未載明",2022,"組",{"v":680.958,"d":"680.96"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1374,"工項類","微型樁，D=30cm，L=6m","未載明",2022,"組",{"v":863.182,"d":"863.18"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1375,"工項類","微型樁，D=30cm，L=8m","未載明",2022,"組",{"v":1106.148,"d":"1106.15"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1376,"工項類","蛇籠，橢圓60cm*100cm，甲種","未載明",2022,"m",{"v":26.176,"d":"26.18"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02373"]
[1377,"工項類","石籠(不分類)","未載明",2022,"m",45.92,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1378,"工項類","土石籠(不分類)","未載明",2022,"m",{"v":64.7675,"d":"64.77"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1379,"工項類","土石籠(不分類)","未載明",2022,"m3",{"v":64.7675,"d":"64.77"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1380,"工項類","石籠(不分類)","未載明",2022,"m3",45.92,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1381,"工項類","土石籠(不分類)","未載明",2022,"組",{"v":64.7675,"d":"64.77"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1382,"工項類","石籠(不分類)","未載明",2022,"組",45.92,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1383,"工項類","石籠，1m × 1m × 1m","未載明",2022,"m3",{"v":19.355,"d":"19.36"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1384,"工項類","土石籠，1m × 1m × 1m","未載明",2022,"m3",{"v":26.894,"d":"26.89"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1385,"工項類","石籠，1m × 1m × 1m","未載明",2022,"組",{"v":19.355,"d":"19.36"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1386,"工項類","土石籠，1m × 1m × 1m","未載明",2022,"組",{"v":26.894,"d":"26.89"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1387,"工項類","石籠，1m × 1m × 2m","未載明",2022,"m",{"v":37.065,"d":"37.07"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1388,"工項類","石籠，1m × 1m × 2m","未載明",2022,"組",{"v":37.065,"d":"37.07"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1389,"工項類","土石籠，1m × 1m × 2m","未載明",2022,"組",{"v":52.143,"d":"52.14"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1390,"工項類","土石籠，1m × 1m × 2m","未載明",2022,"m",{"v":52.143,"d":"52.14"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1391,"工項類","石籠，1m × 1m × 3m","未載明",2022,"m",{"v":54.775,"d":"54.78"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1392,"工項類","石籠，1m × 1m × 3m","未載明",2022,"組",{"v":54.775,"d":"54.78"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1393,"工項類","土石籠，1m × 1m × 3m","未載明",2022,"組",{"v":77.392,"d":"77.39"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1394,"工項類","土石籠，1m × 1m × 3m","未載明",2022,"m",{"v":77.392,"d":"77.39"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1395,"工項類","石籠，1m × 1m × 4m","未載明",2022,"m",{"v":72.485,"d":"72.49"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1396,"工項類","石籠，1m × 1m × 4m","未載明",2022,"組",{"v":72.485,"d":"72.49"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1397,"工項類","土石籠，1m × 1m × 4m","未載明",2022,"組",{"v":102.641,"d":"102.64"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1398,"工項類","土石籠，1m × 1m × 4m","未載明",2022,"m",{"v":102.641,"d":"102.64"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1399,"工項類","瀝青混凝土鋪面(不分類)","未載明",2022,"m2",{"v":13.465,"d":"13.47"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02742"]
[1400,"工項類","瀝青混凝土鋪面，厚5cm","未載明",2022,"m2",8.13,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02742"]
[1401,"工項類","瀝青混凝土鋪面，厚8cm","未載明",2022,"m2",{"v":16.704,"d":"16.70"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02742"]
[1402,"工項類","瀝青混凝土鋪面，厚10cm","未載明",2022,"m2",{"v":21.133,"d":"21.13"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02742"]
[1403,"工項類","多孔隙瀝青混凝土鋪面，厚5cm","未載明",2022,"m2",{"v":7.893,"d":"7.89"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02798"]
[1404,"工項類","瀝青透層(不分類)","未載明",2022,"m2",{"v":2E-3,"d":"0.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02745"]
[1405,"工項類","瀝青黏層(不分類)","未載明",2022,"m2",{"v":2E-3,"d":"0.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02747"]
[1406,"工項類","瀝青混凝土面層刨除(不分類，厚5cm)","未載明",2022,"m2",{"v":2.094,"d":"2.09"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02961"]
[1407,"工項類","瀝青混凝土面層刨除，厚5cm，刨除機2.2m寬","未載明",2022,"m2",{"v":2.094,"d":"2.09"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02961"]
[1408,"工項類","瀝青混凝土面層刨除，刨除料運費","未載明",2022,"m3",{"v":17.032,"d":"17.03"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02961"]
[1409,"工項類","再生瀝青混凝土，舖築及滾壓(不分類，含料)","未載明",2022,"m3",{"v":85.209,"d":"85.21"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02966"]
[1410,"工項類","再生瀝青混凝土，舖築及滾壓(不分類，含料)","未載明",2022,"t",{"v":36.259,"d":"36.26"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02966"]
[1411,"工項類","植栽，客土","未載明",2022,"m3",{"v":0,"d":"0.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02900"]
[1412,"工項類","植樹，喬木(不分類)","未載明",2022,"株",{"v":-250.8375,"d":"-250.84"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02931"]
[1413,"工項類","植樹，喬木，相思樹","未載明",2022,"株",{"v":-381,"d":"-381.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02931"]
[1414,"工項類","植樹，喬木，樟樹","未載明",2022,"株",{"v":-219,"d":"-219.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02931"]
[1415,"工項類","植樹，喬木，光臘樹","未載明",2022,"株",{"v":-168,"d":"-168.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02931"]
[1416,"工項類","植樹，喬木，楓香","未載明",2022,"株",{"v":-222,"d":"-222.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02931"]
[1417,"工項類","植樹，灌木(不分類)","未載明",2022,"株",{"v":-9.375,"d":"-9.38"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02931"]
[1418,"工項類","灌木類植栽(不分類)","未載明",2022,"株",{"v":-9.375,"d":"-9.38"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02900"]
[1419,"工項類","喬木植栽(不分類)","未載明",2022,"株",{"v":-250.8375,"d":"-250.84"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02900"]
[1420,"工項類","喬木植栽，台灣杉","未載明",2022,"株",{"v":-381,"d":"-381.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02900"]
[1421,"工項類","喬木植栽，台灣肖楠","未載明",2022,"株",{"v":-285.9,"d":"-285.90"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02900"]
[1422,"工項類","喬木植栽，烏心石","未載明",2022,"株",{"v":-178.8,"d":"-178.80"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02900"]
[1423,"工項類","喬木植栽，相思樹","未載明",2022,"株",{"v":-381,"d":"-381.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02900"]
[1424,"工項類","喬木植栽，楓香","未載明",2022,"株",{"v":-222,"d":"-222.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02900"]
[1425,"工項類","喬木植栽，櫸木","未載明",2022,"株",{"v":-171,"d":"-171.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02900"]
[1426,"工項類","結構用混凝土(純水泥)(不分類)","未載明",2022,"m3",{"v":425.187,"d":"425.19"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1427,"工項類","結構用混凝土(10%礦物摻料)(不分類)","未載明",2022,"m3",{"v":387.628571428571,"d":"387.63"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1428,"工項類","結構用混凝土(20%礦物摻料)(不分類)","未載明",2022,"m3",{"v":361.089285714286,"d":"361.09"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1429,"工項類","結構用混凝土(30%礦物摻料)(不分類)","未載明",2022,"m3",{"v":300.681142857143,"d":"300.68"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1430,"工項類","結構用混凝土(40%礦物摻料)(不分類)","未載明",2022,"m3",{"v":276.189571428571,"d":"276.19"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1431,"工項類","結構用混凝土(50%礦物摻料)(不分類)","未載明",2022,"m3",{"v":238.985571428571,"d":"238.99"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1432,"工項類","結構用混凝土，預拌，140kgf/cm2(10%礦物摻料)","未載明",2022,"m3",{"v":282.838,"d":"282.84"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1433,"工項類","結構用混凝土，預拌，140kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":267.285,"d":"267.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1434,"工項類","結構用混凝土，預拌，140kgf/cm2(30%礦物摻料)","未載明",2022,"m3",{"v":228.285,"d":"228.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1435,"工項類","結構用混凝土，預拌，140kgf/cm2(40%礦物摻料)","未載明",2022,"m3",{"v":216.997,"d":"217.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1436,"工項類","結構用混凝土，預拌，140kgf/cm2(50%礦物摻料)","未載明",2022,"m3",195.05,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1437,"工項類","結構用混凝土，預拌，175kgf/cm2(10%礦物摻料)","未載明",2022,"m3",{"v":316.285,"d":"316.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1438,"工項類","結構用混凝土，預拌，175kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":292.505,"d":"292.51"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1439,"工項類","結構用混凝土，預拌，175kgf/cm2(30%礦物摻料)","未載明",2022,"m3",{"v":249.873,"d":"249.87"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1440,"工項類","結構用混凝土，預拌，175kgf/cm2(40%礦物摻料)","未載明",2022,"m3",{"v":232.418,"d":"232.42"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1441,"工項類","結構用混凝土，預拌，175kgf/cm2(50%礦物摻料)","未載明",2022,"m3",204.43,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1442,"工項類","結構用混凝土，預拌，210kgf/cm2(10%礦物摻料)","未載明",2022,"m3",{"v":349.232,"d":"349.23"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1443,"工項類","結構用混凝土，預拌，210kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":321.285,"d":"321.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1444,"工項類","結構用混凝土，預拌，210kgf/cm2(30%礦物摻料)","未載明",2022,"m3",{"v":267.285,"d":"267.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1445,"工項類","結構用混凝土，預拌，210kgf/cm2(40%礦物摻料)","未載明",2022,"m3",{"v":244.073,"d":"244.07"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1446,"工項類","結構用混凝土，預拌，210kgf/cm2(50%礦物摻料)","未載明",2022,"m3",209.02,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1447,"工項類","結構用混凝土，預拌，245kgf/cm2(10%礦物摻料)","未載明",2022,"m3",{"v":382.048,"d":"382.05"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1448,"工項類","結構用混凝土，預拌，245kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":352.285,"d":"352.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1449,"工項類","結構用混凝土，預拌，245kgf/cm2(30%礦物摻料)","未載明",2022,"m3",{"v":293.285,"d":"293.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1450,"工項類","結構用混凝土，預拌，245kgf/cm2(40%礦物摻料)","未載明",2022,"m3",{"v":268.837,"d":"268.84"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1451,"工項類","結構用混凝土，預拌，245kgf/cm2(50%礦物摻料)","未載明",2022,"m3",{"v":231.1,"d":"231.10"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1452,"工項類","結構用混凝土，預拌，280kgf/cm2(10%礦物摻料)","未載明",2022,"m3",{"v":397.627,"d":"397.63"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1453,"工項類","結構用混凝土，預拌，280kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":366.285,"d":"366.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1454,"工項類","結構用混凝土，預拌，280kgf/cm2(30%礦物摻料)","未載明",2022,"m3",{"v":317.285,"d":"317.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1455,"工項類","結構用混凝土，預拌，280kgf/cm2(40%礦物摻料)","未載明",2022,"m3",{"v":289.153,"d":"289.15"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1456,"工項類","結構用混凝土，預拌，280kgf/cm2(50%礦物摻料)","未載明",2022,"m3",{"v":252.995,"d":"253.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1457,"工項類","結構用混凝土，預拌，350kgf/cm2(10%礦物摻料)","未載明",2022,"m3",{"v":463.285,"d":"463.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1458,"工項類","結構用混凝土，預拌，350kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":433.695,"d":"433.70"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1459,"工項類","結構用混凝土，預拌，350kgf/cm2(30%礦物摻料)","未載明",2022,"m3",354.47,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1460,"工項類","結構用混凝土，預拌，350kgf/cm2(40%礦物摻料)","未載明",2022,"m3",322.84,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1461,"工項類","結構用混凝土，預拌，350kgf/cm2(50%礦物摻料)","未載明",2022,"m3",{"v":275.865,"d":"275.87"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1462,"工項類","結構用混凝土，預拌，420kgf/cm2(10%礦物摻料)","未載明",2022,"m3",{"v":522.085,"d":"522.09"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1463,"工項類","結構用混凝土，預拌，420kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":494.285,"d":"494.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1464,"工項類","結構用混凝土，預拌，420kgf/cm2(30%礦物摻料)","未載明",2022,"m3",{"v":394.285,"d":"394.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1465,"工項類","結構用混凝土，預拌，420kgf/cm2(40%礦物摻料)","未載明",2022,"m3",{"v":359.009,"d":"359.01"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1466,"工項類","結構用混凝土，預拌，420kgf/cm2(50%礦物摻料)","未載明",2022,"m3",{"v":304.439,"d":"304.44"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03310"]
[1467,"工項類","水泥混凝土構造物，場鑄混凝土(20%礦物摻料)(不分類)","未載明",2022,"m3",{"v":361.089285714286,"d":"361.09"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1468,"工項類","水泥混凝土構造物，場鑄混凝土(50%礦物摻料)(不分類)","未載明",2022,"m3",{"v":238.985571428571,"d":"238.99"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1469,"工項類","水泥混凝土構造物，場鑄混凝土140kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":267.285,"d":"267.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1470,"工項類","水泥混凝土構造物，場鑄混凝土140kgf/cm2(50%礦物摻料)","未載明",2022,"m3",195.05,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1471,"工項類","水泥混凝土構造物，場鑄混凝土175kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":292.505,"d":"292.51"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1472,"工項類","水泥混凝土構造物，場鑄混凝土175kgf/cm2(50%礦物摻料)","未載明",2022,"m3",204.43,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1473,"工項類","水泥混凝土構造物，場鑄混凝土210kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":321.285,"d":"321.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1474,"工項類","水泥混凝土構造物，場鑄混凝土210kgf/cm2(50%礦物摻料)","未載明",2022,"m3",209.02,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1475,"工項類","水泥混凝土構造物，場鑄混凝土245kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":352.285,"d":"352.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1476,"工項類","水泥混凝土構造物，場鑄混凝土245kgf/cm2(50%礦物摻料)","未載明",2022,"m3",{"v":231.1,"d":"231.10"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1477,"工項類","水泥混凝土構造物，場鑄混凝土280kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":366.285,"d":"366.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1478,"工項類","水泥混凝土構造物，場鑄混凝土280kgf/cm2(50%礦物摻料)","未載明",2022,"m3",{"v":252.995,"d":"253.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1479,"工項類","水泥混凝土構造物，場鑄混凝土350kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":433.695,"d":"433.70"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1480,"工項類","水泥混凝土構造物，場鑄混凝土350kgf/cm2(50%礦物摻料)","未載明",2022,"m3",{"v":275.865,"d":"275.87"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1481,"工項類","水泥混凝土構造物，場鑄混凝土420kgf/cm2(20%礦物摻料)","未載明",2022,"m3",{"v":494.285,"d":"494.29"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1482,"工項類","水泥混凝土構造物，場鑄混凝土420kgf/cm2(50%礦物摻料)","未載明",2022,"m3",{"v":304.439,"d":"304.44"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1483,"工項類","預鑄混凝土，異形塊(不分類)","未載明",2022,"塊",{"v":926.6544,"d":"926.65"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1484,"工項類","預鑄混凝土，異形塊，5t","未載明",2022,"塊",{"v":463.452,"d":"463.45"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1485,"工項類","預鑄混凝土，異形塊，10t","未載明",2022,"塊",{"v":883.717,"d":"883.72"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1486,"工項類","預鑄混凝土，異形塊，15t","未載明",2022,"塊",{"v":1348.259,"d":"1348.26"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1487,"工項類","預鑄混凝土，異形塊，20t","未載明",2022,"塊",{"v":1735.132,"d":"1735.13"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1488,"工項類","港灣用預鑄混凝土塊(不分類)","未載明",2022,"塊",{"v":926.6544,"d":"926.65"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1489,"工項類","港灣用預鑄混凝土塊，重2t","未載明",2022,"塊",{"v":202.712,"d":"202.71"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1490,"工項類","港灣用預鑄混凝土塊，重5t","未載明",2022,"塊",{"v":463.452,"d":"463.45"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1491,"工項類","港灣用預鑄混凝土塊，重10t","未載明",2022,"塊",{"v":883.717,"d":"883.72"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1492,"工項類","港灣用預鑄混凝土塊，重15t","未載明",2022,"塊",{"v":1348.259,"d":"1348.26"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1493,"工項類","港灣用預鑄混凝土塊，重20t","未載明",2022,"塊",{"v":1735.132,"d":"1735.13"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1494,"工項類","混凝土塊(不分類)","未載明",2022,"塊",{"v":926.6544,"d":"926.65"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1495,"工項類","混凝土塊，重2t，含製作及吊放","未載明",2022,"塊",{"v":202.712,"d":"202.71"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1496,"工項類","混凝土塊，重5t，含製作及吊放","未載明",2022,"塊",{"v":463.452,"d":"463.45"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1497,"工項類","混凝土塊，重10t，含製作及吊放","未載明",2022,"塊",{"v":883.717,"d":"883.72"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1498,"工項類","混凝土塊，重15t，含製作及吊放","未載明",2022,"塊",{"v":1348.259,"d":"1348.26"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1499,"工項類","混凝土塊，重20t，製作","未載明",2022,"塊",{"v":1735.132,"d":"1735.13"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1500,"工項類","混凝土塊，重20t，吊放","未載明",2022,"塊",{"v":29.378,"d":"29.38"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1501,"工項類","水泥砂漿(不分類)","未載明",2022,"m3",671.33,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","04061"]
[1502,"工項類","水泥砂漿，1:1","未載明",2022,"m3",{"v":952,"d":"952.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","04061"]
[1503,"工項類","水泥砂漿，1:2","未載明",2022,"m3",{"v":625,"d":"625.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","04061"]
[1504,"工項類","水泥砂漿，1:3","未載明",2022,"m3",{"v":437,"d":"437.00"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","04061"]
[1505,"工項類","水泥砂漿粉刷，1：3水泥砂漿，牆面，打底","未載明",2022,"m2",8.74,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","09220"]
[1506,"工項類","洗石子","未載明",2022,"m2",{"v":8.089,"d":"8.09"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","09780"]
[1507,"工項類","抿石子","未載明",2022,"m2",{"v":8.089,"d":"8.09"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1508,"工項類","濕式壓花地坪","未載明",2022,"m2",{"v":60.582,"d":"60.58"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1509,"工項類","乾式噴花地坪","未載明",2022,"m2",{"v":6.896,"d":"6.90"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1510,"工項類","乾式壓花地坪","未載明",2022,"m2",6.87,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1511,"工項類","銲接鋼線網，線徑10mm，方孔10x10cm","未載明",2022,"m2",{"v":10.296,"d":"10.30"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03220"]
[1512,"工項類","銲接鋼線網，線徑10mm，方孔15x15cm","未載明",2022,"m2",{"v":6.864,"d":"6.86"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03220"]
[1513,"工項類","銲接鋼線網，線徑10mm，方孔20x20cm","未載明",2022,"m2",{"v":5.152,"d":"5.15"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03220"]
[1514,"工項類","銲接鋼線網(不分類，線徑10mm)","未載明",2022,"m2","7.437","經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","03220"]
[1515,"工項類","金屬材料(不分類，鋼)","未載明",2022,"kg",2.42,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1516,"工項類","金屬製品，不銹鋼踏步(D=19mm實心)","未載明",2022,"m",{"v":3.895,"d":"3.90"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1517,"工項類","金屬製品，不銹鋼踏步(D=19mm實心)","未載明",2022,"個",3.35,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1518,"工項類","金屬製品，不銹鋼踏步(D=19mm實心)","未載明",2022,"組",3.35,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1519,"工項類","金屬製品，不銹鋼踏步(D=19mm實心)","未載明",2022,"支",3.35,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1520,"工項類","金屬製品，不銹鋼踏步","未載明",2022,"kg",1.75,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1521,"工項類","不銹鋼欄杆(D=50mm，t=3.5mm)","未載明",2022,"m",{"v":36.508,"d":"36.51"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","05523"]
[1522,"工項類","金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座(不分類)","未載明",2022,"組",{"v":255.7945,"d":"255.79"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","05530"]
[1523,"工項類","金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=60cm(52.6kg)","未載明",2022,"組",{"v":157.274,"d":"157.27"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","05530"]
[1524,"工項類","金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=70cm(70.1kg)","未載明",2022,"組",{"v":209.599,"d":"209.60"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","05530"]
[1525,"工項類","金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=80cm(99.5kg)","未載明",2022,"組",{"v":297.505,"d":"297.51"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","05530"]
[1526,"工項類","金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=90cm(120kg)","未載明",2022,"組",{"v":358.8,"d":"358.80"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","05530"]
[1527,"工項類","不銹鋼水尺","未載明",2022,"組",{"v":113.982,"d":"113.98"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署"]
[1528,"工項類","舖單元磚(不分類)","未載明",2022,"m2",{"v":33.739,"d":"33.74"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","09341"]
[1529,"工項類","材料，石膏板，石膏板","未載明",2022,"kg",0.51,"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","09250"]
[1530,"工項類","地工織物，織布，合成纖維","未載明",2022,"m2",{"v":2.479,"d":"2.48"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02342"]
[1531,"工項類","道路施工及復舊(不分類)","未載明",2022,"m2",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","水利工程減碳作業參考指引","經濟部水利署","02952"]
[1532,"工項類","工地拆除","搖籃到大門",2025,"M3",19.627,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02220"]
[1533,"工項類","工地拆除，含運棄","搖籃到大門",2025,"M3",22.254,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02220"]
[1534,"工項類","工地拆除，結構物拆除(建築物以外之結構物拆除)","搖籃到大門",2025,"M3",17.938,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02220"]
[1535,"工項類","工地拆除，結構物拆除(建築物以外之結構物拆除)，鋼筋混凝土","搖籃到大門",2025,"M3",27.179,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02220"]
[1536,"工項類","工地拆除，機械拆除，無筋混凝土，未含運費","搖籃到大門",2025,"M3",{"v":10.872,"d":"10.87"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02220"]
[1537,"工項類","工地拆除，機械拆除，鋼筋混凝土","搖籃到大門",2025,"M3",27.179,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02220"]
[1538,"工項類","工地拆除，建築物拆除，鋼筋混凝土","搖籃到大門",2025,"M3",27.179,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02220"]
[1539,"工項類","工地拆除，機械拆除，結構物拆除(建築物以外之結構物拆除)","搖籃到大門",2025,"M3",19.627,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02220"]
[1540,"工項類","工地拆除，機械切割","搖籃到大門",2025,"M",9.814,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02220"]
[1541,"工項類","工地拆除，機械切割，路面挖除","搖籃到大門",2025,"M3",10.304,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02220"]
[1542,"工項類","工地拆除，機械切割，路面挖除，瀝青混凝土","搖籃到大門",2025,"M3",10.872,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02220"]
[1543,"工項類","工地拆除，機械切割，路面挖除，鋼筋混凝土","搖籃到大門",2025,"M3",27.179,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02220"]
[1544,"工項類","清除及掘除，雜草","搖籃到大門",2025,"M2",0.178,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02231"]
[1545,"工項類","清除及掘除，雜草雜木","搖籃到大門",2025,"M2",0.393,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02231"]
[1546,"工項類","開挖臨時覆蓋板及其支撐，鋼質覆蓋板","搖籃到大門",2025,"KG",2.42,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[1547,"工項類","開挖臨時覆蓋板及其支撐，舖設鋼板臨時作為舖面用","搖籃到大門",2025,"M2",21.744,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[1548,"工項類","開挖臨時覆蓋板及其支撐，舖設鋼板臨時作為舖面用，含載運、吊放及租金","搖籃到大門",2025,"M2",21.744,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03110"]
[1549,"工項類","開挖臨時覆蓋板及其支撐，舖設鋼板臨時作為舖面用，厚 8mm","搖籃到大門",2025,"M2",21.744,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02260"]
[1550,"工項類","開挖臨時覆蓋板及其支撐，舖設鋼板臨時作為舖面用，厚 9mm","搖籃到大門",2025,"M2",21.744,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02260"]
[1551,"工項類","開挖臨時覆蓋板及其支撐，舖設鋼板臨時作為舖面用，厚 12mm","搖籃到大門",2025,"M2",21.744,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02260"]
[1552,"工項類","開挖臨時覆蓋板及其支撐，舖設鋼板臨時作為舖面用，厚 20mm","搖籃到大門",2025,"M2",21.744,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02260"]
[1553,"工項類","構造物開挖，機械挖","搖籃到大門",2025,"M3",1.963,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02316"]
[1554,"工項類","構造物開挖，(機械挖，基礎，深度 0～4m)","搖籃到大門",2025,"M3",2.174,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02316"]
[1555,"工項類","構造物開挖，軟弱地質，機械挖","搖籃到大門",2025,"M3",2.751,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02316"]
[1556,"工項類","構造物開挖，砂土礫石，機械挖","搖籃到大門",2025,"M3",2.51,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02316"]
[1557,"工項類","構造物開挖，軟岩，機械挖","搖籃到大門",2025,"M3",2.781,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02316"]
[1558,"工項類","構造物開挖，硬岩，機械挖","搖籃到大門",2025,"M3",5.88,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02316"]
[1559,"工項類","構造物開挖，卵石(挖普通土含 30%以上砂礫)，機械挖","搖籃到大門",2025,"M3",2.51,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02316"]
[1560,"工項類","構造物回填，原材料回填","搖籃到大門",2025,"M3",0.393,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02317"]
[1561,"工項類","構造物回填，原材料回填，機具夯實","搖籃到大門",2025,"M3",8.58,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02317"]
[1562,"工項類","構造物回填，原材料回填，運距＜5km，含運費","搖籃到大門",2025,"M3",4.693,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02317"]
[1563,"工項類","構造物回填，回填及夯實(實際)","搖籃到大門",2025,"M3",8.58,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02317"]
[1564,"工項類","構造物回填，餘方近運","搖籃到大門",2025,"M3",1.178,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02317"]
[1565,"工項類","構造物回填，餘方近運，運距＜5km","搖籃到大門",2025,"M3",2.132,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02317"]
[1566,"工項類","選擇性回填材料，級配粒料","搖籃到大門",2025,"M3",{"v":7.428,"d":"7.43"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02319"]
[1567,"工項類","選擇性回填材料，級配粒料，碎石級配及夯實","搖籃到大門",2025,"M3",8.398,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02319"]
[1568,"工項類","基地及路幅開挖，含餘方近運利用","搖籃到大門",2025,"M3",0.87,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02319"]
[1569,"工項類","浚挖，小搬運費","搖籃到大門",2025,"M3",15.759,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1570,"工項類","浚挖，疏浚挖方(河道清疏)","搖籃到大門",2025,"時",114.73,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1571,"工項類","基地及路堤填築，原材料回填","搖籃到大門",2025,"M3",0.87,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02331"]
[1572,"工項類","路基整理","搖籃到大門",2025,"M2",0.491,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02336"]
[1573,"工項類","岩盤灌漿","搖籃到大門",2025,"M3",8.688,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02341"]
[1574,"工項類","土方工作，遠運利用","搖籃到大門",2025,"M3",{"v":3.908,"d":"3.91"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02300"]
[1575,"工項類","土方工作，含挖方、回填、餘方處理","搖籃到大門",2025,"M3",11.257,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02300"]
[1576,"工項類","土方工作，工區內土方調整","搖籃到大門",2025,"M3",1.626,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02300"]
[1577,"工項類","土方工作，挖岩方(挖硬岩)","搖籃到大門",2025,"M3",8.832,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02300"]
[1578,"工項類","土方工作，挖岩方(挖軟岩)","搖籃到大門",2025,"M3",5.299,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02300"]
[1579,"工項類","土方工作，挖方","搖籃到大門",2025,"M3",1.806,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02300"]
[1580,"工項類","土方工作，填方","搖籃到大門",2025,"M3",0.785,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02300"]
[1581,"工項類","土方工作，回填方","搖籃到大門",2025,"M3",1.087,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02300"]
[1582,"工項類","借土，1≦運距＜5km，包挖運","搖籃到大門",2025,"M3",1.178,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1583,"工項類","借土，5≦運距＜10km，包挖運","搖籃到大門",2025,"M3",2.355,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1584,"工項類","借土，10≦運距＜20km","搖籃到大門",2025,"M3",3.533,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1585,"工項類","借土，20≦運距＜30km","搖籃到大門",2025,"M3",4.711,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1586,"工項類","棄土，餘方近運利用","搖籃到大門",2025,"M3",{"v":1.989,"d":"1.99"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02323"]
[1587,"工項類","棄土，餘方自行處理(含水土保持)","搖籃到大門",2025,"M3",0.788,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02323"]
[1588,"工項類","棄土，棄土區費用(含水土保持)，0≦運距＜5km","搖籃到大門",2025,"M3",1.445,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02323"]
[1589,"工項類","棄土，廢方處理，含運費","搖籃到大門",2025,"M3",10.135,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02323"]
[1590,"工項類","臨時擋土樁設施，打拔，【單位 M 為打拔深度，不分類】","搖籃到大門",2025,"M",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1591,"工項類","臨時擋土樁設施，鋼軌樁 37kg/m，打拔","搖籃到大門",2025,"M",1.449,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1592,"工項類","臨時擋土樁設施，鋼軌樁 37kg/m，L=3m，買斷","搖籃到大門",2025,"支",266.7,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1593,"工項類","臨時擋土樁設施，鋼軌樁37kg/m，L=5m、間距=60cm，(單邊水平長度，含擋土支撐系統)","搖籃到大門",2025,"M",10.749,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1594,"工項類","臨時擋土樁設施，鋼軌樁 37kg/m，L=6m，含引孔、打拔","搖籃到大門",2025,"支",6.021,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1595,"工項類","臨時擋土樁設施，鋼軌樁 37kg/m，L=6m，買斷","搖籃到大門",2025,"支",533.448,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1596,"工項類","臨時擋土樁設施，鋼軌樁 50kg/m，L=3m，打拔，【單位 M 為打拔深度】","搖籃到大門",2025,"M",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1597,"工項類","臨時擋土樁設施，鋼軌樁 50kg/m，\n(L=3m，間距=50cm)，打拔，【單位 M\n為打拔深度】","搖籃到大門",2025,"M",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1598,"工項類","臨時擋土樁設施，鋼軌樁 50kg/m，\nL=3m，間距=100cm)，打拔，【單位 M\n為打拔深度】","搖籃到大門",2025,"M",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1599,"工項類","臨時擋土樁設施，鋼軌樁 50kg/m，L=4m，含引孔、打拔","搖籃到大門",2025,"支",5.538,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1600,"工項類","臨時擋土樁設施，鋼軌樁 50kg/m，L=5m，打拔，【單位 M 為打拔深度】","搖籃到大門",2025,"M",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1601,"工項類","臨時擋土樁設施，鋼軌樁 50kg/m，L=6m，打拔，【單位 M 為打拔深度】","搖籃到大門",2025,"M",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1602,"工項類","臨時擋土樁設施，鋼軌樁 50kg/m，\n(L=6m，間距=100cm)，打拔，【單位 M\n為打拔深度】","搖籃到大門",2025,"M",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1603,"工項類","臨時擋土樁設施，鋼軌樁 50kg/m，L=7m，打拔，【單位 M 為打拔深度】","搖籃到大門",2025,"M",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1604,"工項類","臨時擋土樁設施，鋼板樁，含施作","搖籃到大門",2025,"M",11.377,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1605,"工項類","臨時擋土樁設施，鋼板樁，L=6m，【材料】","搖籃到大門",2025,"片",871.2,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1606,"工項類","臨時擋土樁設施，鋼板樁，L=9m，【材料】","搖籃到大門",2025,"片",1306.8,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1607,"工項類","臨時擋土樁設施，鋼板樁，L=13m，打拔，【單位 M 為打拔深度】","搖籃到大門",2025,"M",{"v":14.5,"d":"14.50"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1608,"工項類","臨時擋土樁設施，鋼板樁，L=13m，打拔","搖籃到大門",2025,"片",{"v":5.8,"d":"5.80"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1609,"工項類","臨時擋土樁設施，鋼板樁，L=13m，打拔","搖籃到大門",2025,"支",{"v":5.8,"d":"5.80"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1610,"工項類","臨時擋土樁設施，鋼軌樁 42kg/m，【材料】","搖籃到大門",2025,"M",100.367,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1611,"工項類","臨時擋土樁設施，鋼軌樁 42kg/m，含施作","搖籃到大門",2025,"支",5.857,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1612,"工項類","臨時擋土樁設施，鋼軌樁 42kg/m，L=3m，買斷","搖籃到大門",2025,"支",301.14,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1613,"工項類","臨時擋土樁設施，鋼軌樁 42kg/m，L=4m，買斷","搖籃到大門",2025,"支",401.52,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1614,"工項類","臨時擋土樁設施，鋼軌樁 42kg/m，L=5m，買斷","搖籃到大門",2025,"支",501.9,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1615,"工項類","臨時擋土樁設施，鋼軌樁 42kg/m，\nL=6m，打拔","搖籃到大門",2025,"M",0.483,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1616,"工項類","臨時擋土樁設施，鋼軌樁 42kg/m，L=6m，買斷","搖籃到大門",2025,"支",602.28,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02255"]
[1617,"工項類","臨時擋土支撐工法，H 型鋼橫擋及支撐，裝拆","搖籃到大門",2025,"M2",{"v":39.637,"d":"39.64"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02256"]
[1618,"工項類","開挖支撐及保護，鋼軌樁，【不含材料】","搖籃到大門",2025,"支",49.068,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02260"]
[1619,"工項類","坡面工，【不分類】","搖籃到大門",2025,"M2",{"v":49.415,"d":"49.42"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02385"]
[1620,"工項類","砌排石工，鋪塊石，(厚 20cm，含勾縫)","搖籃到大門",2025,"M2",292.182,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02386"]
[1621,"工項類","砌排石工，乾砌塊石，(厚 20cm，含勾縫)","搖籃到大門",2025,"M2",8.852,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02386"]
[1622,"工項類","砌排石工，混凝土砌塊石，石塊現採，(長徑 40~80cm 佔 70%以上)","搖籃到大門",2025,"M2",10.815,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02386"]
[1623,"工項類","砌排石工，乾砌塊石 15≦∮≦40cm，(厚25cm，未含勾縫)","搖籃到大門",2025,"M2",5.309,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02386"]
[1624,"工項類","砌排石工，乾砌塊石 41≦∮≦80cm","搖籃到大門",2025,"M2",8.358,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02386"]
[1625,"工項類","砌排石工，乾砌塊石 80cm≦∮≦120cm","搖籃到大門",2025,"M3",7.181,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02386"]
[1626,"工項類","級配粒料基層，總厚 5cm","搖籃到大門",2025,"M2",{"v":0.287,"d":"0.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02722"]
[1627,"工項類","級配粒料基層，總厚 10cm","搖籃到大門",2025,"M2",{"v":0.574,"d":"0.57"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02722"]
[1628,"工項類","級配粒料基層，總厚 15cm","搖籃到大門",2025,"M2",0.861,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02722"]
[1629,"工項類","級配粒料基層，總厚 20cm","搖籃到大門",2025,"M2",{"v":1.148,"d":"1.15"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02722"]
[1630,"工項類","級配粒料底層，總厚 10cm，鋪設及滾壓","搖籃到大門",2025,"M2",1.306,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02726"]
[1631,"工項類","級配粒料底層，總厚 20cm，鋪設及滾壓","搖籃到大門",2025,"M2",4.575,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02726"]
[1632,"工項類","級配粒料底層，總厚 5cm，鋪設及滾壓","搖籃到大門",2025,"M2",0.948,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02726"]
[1633,"工項類","級配粒料底層，碎石級配，鋪設及滾壓","搖籃到大門",2025,"M3",5.74,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02726"]
[1634,"工項類","邊坡穩定水平排水管，【不分類】","搖籃到大門",2025,"M",11.31,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02377"]
[1635,"工項類","邊坡穩定水平排水管，【不分類】","搖籃到大門",2025,"KG",2.4,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02377"]
[1636,"工項類","邊坡穩定水平排水管，管徑=50mm，【t=4.1mm】","搖籃到大門",2025,"M",{"v":2.693,"d":"2.69"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02377"]
[1637,"工項類","邊坡穩定水平排水管，管徑=80mm，【t=5.1mm】","搖籃到大門",2025,"M",{"v":5.285,"d":"5.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02377"]
[1638,"工項類","邊坡穩定水平排水管，管徑=100mm，【t=6.6mm】","搖籃到大門",2025,"M",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02377"]
[1639,"工項類","邊坡穩定水平排水管，管徑=150mm，【t=9.0mm】","搖籃到大門",2025,"M",{"v":16.082,"d":"16.08"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02377"]
[1640,"工項類","邊坡穩定水平排水管，管徑=200mm，【t=10.5mm】","搖籃到大門",2025,"M",24.31,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02377"]
[1641,"工項類","邊坡穩定水平排水管，高密度聚乙烯(HDPE)管(有孔)","搖籃到大門",2025,"M",50.76,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02377"]
[1642,"工項類","邊坡穩定水平排水管，洩水管，【不分類】","搖籃到大門",2025,"M",4.968,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02377"]
[1643,"工項類","邊坡穩定水平排水管，洩水管，PVC 管(有孔)，管徑=80mm，【管厚≧5.1mm】","搖籃到大門",2025,"M",5.285,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02377"]
[1644,"工項類","邊坡穩定水平排水管，濾料袋","搖籃到大門",2025,"袋",0.126,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02377"]
[1645,"工項類","自來水用塑膠管，聚氯乙烯塑膠管，【不分類】","搖籃到大門",2025,"M",11.31,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02511"]
[1646,"工項類","自來水用塑膠管，聚氯乙烯塑膠管，標稱管徑 50mm，【t=4.1mm】","搖籃到大門",2025,"M",{"v":2.693,"d":"2.69"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02511"]
[1647,"工項類","自來水用塑膠管，聚氯乙烯塑膠管，標稱管徑 75mm，【t=5.5mm】","搖籃到大門",2025,"M",{"v":5.285,"d":"5.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02511"]
[1648,"工項類","自來水用塑膠管，聚氯乙烯塑膠管，標稱管徑 100mm，【t=6.6mm】","搖籃到大門",2025,"M",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02511"]
[1649,"工項類","自來水用塑膠管，聚氯乙烯塑膠管，標稱管徑 150mm，【t=8.9mm】","搖籃到大門",2025,"M",{"v":16.082,"d":"16.08"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02511"]
[1650,"工項類","自來水用塑膠管，聚氯乙烯塑膠管，標稱管徑 200mm，【t=10.3mm】","搖籃到大門",2025,"M",24.31,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02511"]
[1651,"工項類","自來水用塑膠管，高密度聚乙烯管，標稱管徑 200mm，【t=11.9mm】","搖籃到大門",2025,"M",17.28,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02511"]
[1652,"工項類","排水管溝，【不分類】","搖籃到大門",2025,"M",11.31,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02601"]
[1653,"工項類","排水管溝，塑膠管 B 管，D=100mm，【t=6.6mm】","搖籃到大門",2025,"M",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02601"]
[1654,"工項類","排水管溝，塑膠管 B 管，D=150mm，【t=8.9mm】","搖籃到大門",2025,"M",{"v":16.082,"d":"16.08"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02601"]
[1655,"工項類","排水管溝，塑膠管 B 管，D=200mm，【t=10.3mm】","搖籃到大門",2025,"M",24.31,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02601"]
[1656,"工項類","排水管溝，高密度聚乙烯管","搖籃到大門",2025,"M",17.28,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02601"]
[1657,"工項類","聚氯乙烯塑膠管及配件，【塑膠管】","搖籃到大門",2025,"M",9.789,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1658,"工項類","聚氯乙烯塑膠管及配件，標稱 80mm，【厚 3mm 以上】","搖籃到大門",2025,"M",4.968,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1659,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(A 管薄管)，標稱 80mm，【厚 3mm 以上】","搖籃到大門",2025,"M",2.784,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1660,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，【不分類】","搖籃到大門",2025,"M",11.31,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1661,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，標稱 50mm，厚 4.1mm","搖籃到大門",2025,"M",2.712,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1662,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，標稱 50mm，厚 4.1mm，(1 支 4M)","搖籃到大門",2025,"支",10.848,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1663,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，標稱 80mm，厚 5.1mm","搖籃到大門",2025,"M",4.968,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1664,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，標稱 80mm，厚 5.1mm，(1 支 4M)","搖籃到大門",2025,"支",19.872,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1665,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，標稱 100mm，厚 6.6mm","搖籃到大門",2025,"M",8.208,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1666,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，標稱 100mm，厚 6.6mm，(1 支 5M)","搖籃到大門",2025,"支",41.04,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1667,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，標稱 125mm，厚 7.0mm","搖籃到大門",2025,"M",10.776,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1668,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，標稱 125mm，厚 7.0mm，(1 支 5M)","搖籃到大門",2025,"支",53.88,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1669,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，標稱 150mm，厚 9.0mm","搖籃到大門",2025,"M",16.085,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1670,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，標稱 150mm，厚 9.0mm，(1 支 6M)","搖籃到大門",2025,"支",96.509,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1671,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，標稱 200mm，厚 10.5mm","搖籃到大門",2025,"M",24.816,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1672,"工項類","聚氯乙烯塑膠管及配件，硬質聚氯乙烯塑膠管(B 管厚管)，標稱 200mm，厚 10.5mm，(1 支 6M)","搖籃到大門",2025,"支",148.896,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1673,"工項類","污水管路系統，聚氯乙烯管(B 管厚管)，橘色管，【不分類】","搖籃到大門",2025,"M",11.31,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署",15151]
[1674,"工項類","污水管路系統，聚氯乙烯管(B 管厚管)，橘色管，標稱管徑 50mm，厚 4.1mm","搖籃到大門",2025,"M",{"v":2.693,"d":"2.69"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署",15151]
[1675,"工項類","污水管路系統，聚氯乙烯管(B 管厚管)，橘色管，標稱管徑 80mm，厚 5.1mm","搖籃到大門",2025,"M",{"v":5.285,"d":"5.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署",15151]
[1676,"工項類","污水管路系統，聚氯乙烯管(B 管厚管)，橘色管，標稱管徑 100mm，厚 6.6mm","搖籃到大門",2025,"M",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署",15151]
[1677,"工項類","污水管路系統，聚氯乙烯管(B 管厚管)，橘色管，標稱管徑 150mm，厚 9mm","搖籃到大門",2025,"M",{"v":16.082,"d":"16.08"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署",15151]
[1678,"工項類","拋石","搖籃到大門",2025,"M3",{"v":5.352,"d":"5.35"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02381"]
[1679,"工項類","拋石，塊石，石塊現採，【不分類】","搖籃到大門",2025,"M3",4.345,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02381"]
[1680,"工項類","拋石，塊石，40cm≦長徑，石塊現採","搖籃到大門",2025,"M3",6.903,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02381"]
[1681,"工項類","拋石，塊石，80cm≦長徑","搖籃到大門",2025,"M3",27.478,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02381"]
[1682,"工項類","拋石，卵石","搖籃到大門",2025,"M3",5.103,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02381"]
[1683,"工項類","污水管管材，鋼筋混凝土管，【不分類】","搖籃到大門",2025,"M",205.49,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02533"]
[1684,"工項類","污水管管材，鋼筋混凝土管，【L=2.4mm，不分類】","搖籃到大門",2025,"支",{"v":493.176,"d":"493.18"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02533"]
[1685,"工項類","污水管管材，鋼筋混凝土管，標稱管徑600mm","搖籃到大門",2025,"M",{"v":151.338,"d":"151.34"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02533"]
[1686,"工項類","污水管管材，鋼筋混凝土管，標稱管徑600mm，【L=2.4mm】","搖籃到大門",2025,"支",{"v":363.212,"d":"363.21"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02533"]
[1687,"工項類","污水管管材，鋼筋混凝土管，標稱管徑800mm","搖籃到大門",2025,"M",{"v":205.708,"d":"205.71"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02533"]
[1688,"工項類","污水管管材，鋼筋混凝土管，標稱管徑800mm，【L=2.4mm】","搖籃到大門",2025,"支",{"v":493.7,"d":"493.70"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02533"]
[1689,"工項類","污水管管材，鋼筋混凝土管，標稱管徑1000mm","搖籃到大門",2025,"M",{"v":259.424,"d":"259.42"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02533"]
[1690,"工項類","污水管管材，鋼筋混凝土管，標稱管徑1000mm，【L=2.4mm】","搖籃到大門",2025,"支",{"v":622.617,"d":"622.62"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02533"]
[1691,"工項類","污水管管材，聚氯乙烯塑膠硬質管，標稱管徑 200mm，【t=10.3mm】","搖籃到大門",2025,"M",24.31,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02533"]
[1692,"工項類","管涵，連工帶料，【不分類】","搖籃到大門",2025,"M",453.557,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1693,"工項類","管涵，鋼筋混凝土管 B 型，【不分類】","搖籃到大門",2025,"M",205.49,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1694,"工項類","管涵，鋼筋混凝土管 B 型，標稱管徑600mm","搖籃到大門",2025,"M",{"v":151.338,"d":"151.34"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1695,"工項類","管涵，鋼筋混凝土管 B 型，標稱管徑1000mm","搖籃到大門",2025,"M",{"v":259.424,"d":"259.42"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1696,"工項類","排水管涵，鋼筋混凝土管(B 型)，D=400mm，二級管，埋設費","搖籃到大門",2025,"支",510.84,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1697,"工項類","排水管涵，鋼筋混凝土管(B 型)，D=600mm，【L=2.4m】","搖籃到大門",2025,"支",{"v":363.212,"d":"363.21"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1698,"工項類","排水管涵，鋼筋混凝土管(B 型)，D=800mm，【L=2.4m】","搖籃到大門",2025,"支",{"v":493.7,"d":"493.70"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1699,"工項類","排水管涵，鋼筋混凝土管 B 型，D=1000mm","搖籃到大門",2025,"M",{"v":259.424,"d":"259.42"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1700,"工項類","排水管涵，鋼筋混凝土管(B 型)，D=1000mm，【L=2.4m】","搖籃到大門",2025,"支",{"v":622.617,"d":"622.62"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1701,"工項類","排水管涵，聚氯乙烯排水管","搖籃到大門",2025,"M",4.968,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1702,"工項類","排水管涵，聚氯乙烯排水管，【2m/支】","搖籃到大門",2025,"支",9.936,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1703,"工項類","排水管涵，聚氯乙烯排水管，D=50mm，【t=4.1mm】","搖籃到大門",2025,"M",{"v":2.693,"d":"2.69"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1704,"工項類","排水管涵，聚氯乙烯排水管，D=75mm，【t=5.5mm】","搖籃到大門",2025,"M",{"v":5.285,"d":"5.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1705,"工項類","排水管涵，聚氯乙烯排水管，D=100mm，【t=6.6mm】","搖籃到大門",2025,"M",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1706,"工項類","排水管涵，聚氯乙烯排水管，D=150mm，【t=8.9mm】","搖籃到大門",2025,"M",{"v":16.082,"d":"16.08"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1707,"工項類","排水管涵，聚氯乙烯排水管，D=200mm，【t=10.3mm】","搖籃到大門",2025,"M",24.31,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1708,"工項類","排水管涵，鋼筋混凝土管涵，【不分類】","搖籃到大門",2025,"M",205.49,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1709,"工項類","排水管涵，鋼筋混凝土管涵，【不分類】","搖籃到大門",2025,"支",885.72,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02610"]
[1710,"工項類","預力混凝土基樁，B 種，【不分類】","搖籃到大門",2025,"M",{"v":79.581,"d":"79.58"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02457"]
[1711,"工項類","預力混凝土基樁，D=300mm，B 種","搖籃到大門",2025,"M",{"v":35.604,"d":"35.60"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02457"]
[1712,"工項類","預力混凝土基樁，D=500mm，B 種","搖籃到大門",2025,"M",{"v":66.232,"d":"66.23"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02457"]
[1713,"工項類","預力混凝土基樁，D=600mm，B 種","搖籃到大門",2025,"M",{"v":85.168,"d":"85.17"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02457"]
[1714,"工項類","預力混凝土基樁，D=800mm，B 種","搖籃到大門",2025,"M",{"v":131.318,"d":"131.32"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02457"]
[1715,"工項類","預力混凝土基樁，D=800mm，B 種，L=12m","搖籃到大門",2025,"支",{"v":1626.521,"d":"1626.52"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02457"]
[1716,"工項類","預壘樁，注漿材料及拌和，175kgf/cm2","搖籃到大門",2025,"M3",380.71,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1717,"工項類","微型樁，15≦D＜20cm","搖籃到大門",2025,"M",12.084,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1718,"工項類","微型樁，D=30cm，【不分類】","搖籃到大門",2025,"組",{"v":883.429,"d":"883.43"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1719,"工項類","微型樁，D=30cm， 4≦L＜6m，【L=4.5m】","搖籃到大門",2025,"組",{"v":680.958,"d":"680.96"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1720,"工項類","微型樁，D=30cm， 6≦L＜8m，【L=6m】","搖籃到大門",2025,"組",{"v":863.182,"d":"863.18"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1721,"工項類","微型樁，D=30cm， 8≦L＜10m，【L=8m】","搖籃到大門",2025,"組",{"v":1106.148,"d":"1106.15"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1722,"工項類","預力地錨，水泥及灌漿","搖籃到大門",2025,"包",50.827,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02492"]
[1723,"工項類","生態護坡，打樁編柵","搖籃到大門",2025,"M",11.039,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1724,"工項類","生態護坡，稻草蓆敷蓋","搖籃到大門",2025,"M2",0.32,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1725,"工項類","生態護坡，客土袋","搖籃到大門",2025,"個",0.981,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1726,"工項類","護坡，坡面整理(山邊溝)","搖籃到大門",2025,"M2",0.344,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1727,"工項類","護坡，噴凝土護坡，鋪網噴漿溝W50xH30cm","搖籃到大門",2025,"M",189.906,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1728,"工項類","護坡，噴凝土護坡，鋪網噴漿溝W40xH30cm","搖籃到大門",2025,"M",175.524,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1729,"工項類","護坡，噴凝土護坡，鋪網噴漿溝W80xH50cm","搖籃到大門",2025,"M",281.734,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1730,"工項類","護坡，噴凝土護坡，鋪網噴漿溝W120xH50cm","搖籃到大門",2025,"M",326.093,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1731,"工項類","護坡，噴凝土格子框","搖籃到大門",2025,"M2",54.595,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1732,"工項類","蛇籠，橢圓 60cm*100cm，甲種(機編蛇籠網材另計)","搖籃到大門",2025,"M",{"v":26.176,"d":"26.18"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02373"]
[1733,"工項類","箱型石籠，【不分類】","搖籃到大門",2025,"M3",45.92,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02374"]
[1734,"工項類","箱型石籠，【不分類】","搖籃到大門",2025,"組",45.92,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02374"]
[1735,"工項類","箱型石籠，石塊現採","搖籃到大門",2025,"M3",11.776,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02374"]
[1736,"工項類","箱型石籠，石塊外購，【不含運費】","搖籃到大門",2025,"M3",49.068,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02374"]
[1737,"工項類","箱型石籠，1.0m × 1.0m ×1.0m，石塊外購，【含運費】","搖籃到大門",2025,"M3",63.882,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02374"]
[1738,"工項類","箱型石籠，箱型石籠內填卵(塊)石，石塊現採","搖籃到大門",2025,"M3",16.47,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02374"]
[1739,"工項類","箱型石籠，箱型石籠內填卵(塊)石，石塊外購","搖籃到大門",2025,"M3",49.836,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02374"]
[1740,"工項類","箱型石籠，1.0m × 1.0m ×2.0m","搖籃到大門",2025,"M",{"v":37.065,"d":"37.07"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02374"]
[1741,"工項類","箱型石籠，1.0m × 1.0m ×3.0m","搖籃到大門",2025,"M",{"v":54.775,"d":"54.78"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02374"]
[1742,"工項類","箱型石籠，1.0m × 1.0m ×4.0m","搖籃到大門",2025,"M",{"v":72.485,"d":"72.49"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02374"]
[1743,"工項類","箱型石籠，鍍鋅鋼線箱形石籠網材，小搬運","搖籃到大門",2025,"M2",2.469,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02374"]
[1744,"工項類","生態護岸，木排樁護岸(直線段)","搖籃到大門",2025,"M",4.907,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1745,"工項類","生態護岸，木排樁護岸(轉彎段)","搖籃到大門",2025,"M",18.646,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1746,"工項類","柔性舖面，粗粒料","搖籃到大門",2025,"KG",0.01,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1747,"工項類","柔性舖面，細粒料","搖籃到大門",2025,"KG",0.015,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1748,"工項類","瀝青混凝土鋪面，【不分類】","搖籃到大門",2025,"M2",{"v":13.465,"d":"13.47"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02742"]
[1749,"工項類","瀝青混凝土舖面，厚 5cm","搖籃到大門",2025,"M2",8.13,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02742"]
[1750,"工項類","瀝青混凝土鋪面，厚 8cm","搖籃到大門",2025,"M2",{"v":16.704,"d":"16.70"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02742"]
[1751,"工項類","瀝青混凝土鋪面，厚 10cm","搖籃到大門",2025,"M2",{"v":21.133,"d":"21.13"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02742"]
[1752,"工項類","瀝青混凝土舖面，密級配，粗粒料25.0mm","搖籃到大門",2025,"KG",0.084,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02742"]
[1753,"工項類","瀝青混凝土舖面，密級配，粗粒料19.0mm","搖籃到大門",2025,"KG",0.081,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02742"]
[1754,"工項類","瀝青混凝土舖面，密級配，粗粒料12.5mm","搖籃到大門",2025,"KG",0.083,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02742"]
[1755,"工項類","瀝青透層，【不分類】","搖籃到大門",2025,"M2",{"v":2E-3,"d":"0.002"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02745"]
[1756,"工項類","瀝青黏層，【不分類】","搖籃到大門",2025,"M2",{"v":2E-3,"d":"0.002"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02747"]
[1757,"工項類","多孔隙瀝青混凝土鋪面，【厚 5cm】","搖籃到大門",2025,"M2",{"v":7.893,"d":"7.89"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02798"]
[1758,"工項類","標線","搖籃到大門",2025,"KG",20.37,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02898"]
[1759,"工項類","標線，厚 2mm","搖籃到大門",2025,"M2",20.81,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02898"]
[1760,"工項類","標線，熱處理聚酯，反光，【W=15cm】","搖籃到大門",2025,"M",3.944,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02898"]
[1761,"工項類","標線，熱處理聚酯，反光，磨除(刨除)","搖籃到大門",2025,"M2",11.776,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02898"]
[1762,"工項類","標線，熱處理聚酯，反光，厚 2mm","搖籃到大門",2025,"M2",21.491,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02898"]
[1763,"工項類","標線，熱處理聚酯第Ⅱ型，厚 2mm","搖籃到大門",2025,"M2",8.915,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02898"]
[1764,"工項類","標線，路線漆，【W=15cm】","搖籃到大門",2025,"M",3.298,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02898"]
[1765,"工項類","道路施工及復舊，【不分類】","搖籃到大門",2025,"M2",{"v":8.182,"d":"8.18"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1766,"工項類","道路施工及復舊，施工便道","搖籃到大門",2025,"M",3.925,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02952"]
[1767,"工項類","瀝青混凝土面層刨除","搖籃到大門",2025,"M2",0.736,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02961"]
[1768,"工項類","瀝青混凝土面層刨除，路面切割費，【含施作】","搖籃到大門",2025,"M2",24.534,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02961"]
[1769,"工項類","瀝青混凝土面層刨除，厚 5cm","搖籃到大門",2025,"M2",{"v":2.029,"d":"2.03"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02961"]
[1770,"工項類","瀝青混凝土面層刨除，厚 5cm，刨除機2.2m寬","搖籃到大門",2025,"M2",{"v":2.094,"d":"2.09"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02961"]
[1771,"工項類","瀝青混凝土面層刨除，厚 5cm，刨除料運費","搖籃到大門",2025,"M2",{"v":17.032,"d":"17.03"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02961"]
[1772,"工項類","再生瀝青混凝土鋪面，舖築及滾壓，【含材料】","搖籃到大門",2025,"M3",{"v":85.209,"d":"85.21"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03051"]
[1773,"工項類","再生瀝青混凝土鋪面，舖築及滾壓，【含材料】","搖籃到大門",2025,"T",{"v":36.259,"d":"36.26"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03051"]
[1774,"工項類","植栽，客土，含運輸","搖籃到大門",2025,"M3",{"v":9.044,"d":"9.04"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02900"]
[1775,"工項類","移植","搖籃到大門",2025,"株",0.054,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02905"]
[1776,"工項類","移植，(喬木類，一次移植)","搖籃到大門",2025,"株",0.145,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02905"]
[1777,"工項類","植草，鋪植草皮","搖籃到大門",2025,"M2",0.187,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02920"]
[1778,"工項類","植草，草皮","搖籃到大門",2025,"M2",1.897,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02920"]
[1779,"工項類","植草，草種噴植","搖籃到大門",2025,"M2",4.529,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02920"]
[1780,"工項類","植草，掛立體網噴植","搖籃到大門",2025,"M2",10.174,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02920"]
[1781,"工項類","植草，客土袋育苗植法","搖籃到大門",2025,"M3",0.981,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02920"]
[1782,"工項類","植草，撒播，(覆蓋稻草蓆、撒砂土或其他方式處理)","搖籃到大門",2025,"M2",0.017,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02920"]
[1783,"工項類","噴植草，坡面噴植","搖籃到大門",2025,"M2",8.455,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02920"]
[1784,"工項類","地被類植栽， 一般地被類","搖籃到大門",2025,"M2",0.18,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02900"]
[1785,"工項類","植樹，喬木，【不分類】","搖籃到大門",2025,"株",{"v":-250.838,"d":"-250.84"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02931"]
[1786,"工項類","植樹，喬木，相思樹","搖籃到大門",2025,"株",{"v":-381,"d":"-381.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02931"]
[1787,"工項類","植樹，喬木，樟樹","搖籃到大門",2025,"株",{"v":-219,"d":"-219.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02931"]
[1788,"工項類","植樹，喬木，光臘樹","搖籃到大門",2025,"株",{"v":-168,"d":"-168.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02931"]
[1789,"工項類","植樹，喬木，楓香","搖籃到大門",2025,"株",{"v":-222,"d":"-222.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02931"]
[1790,"工項類","植樹，灌木，【不分類】","搖籃到大門",2025,"株",{"v":-9.375,"d":"-9.38"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02931"]
[1791,"工項類","灌木類植栽，【不分類】","搖籃到大門",2025,"株",{"v":-9.375,"d":"-9.38"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02900"]
[1792,"工項類","蔓藤類植栽，爬牆虎","搖籃到大門",2025,"株",0.01,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02900"]
[1793,"工項類","植栽維護，草花類","搖籃到大門",2025,"M2",0.028,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02936"]
[1794,"工項類","植栽維護，草花類","搖籃到大門",2025,"株",0.135,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02936"]
[1795,"工項類","植物保護，養護工作，灌木類","搖籃到大門",2025,"株",0.18,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02936"]
[1796,"工項類","植物保護，養護工作，地被類","搖籃到大門",2025,"M2",0.018,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02936"]
[1797,"工項類","喬木植栽，【不分類】","搖籃到大門",2025,"株",{"v":-250.838,"d":"-250.84"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02900"]
[1798,"工項類","喬木植栽，台灣杉","搖籃到大門",2025,"株",{"v":-381,"d":"-381.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02900"]
[1799,"工項類","喬木植栽，台灣肖楠","搖籃到大門",2025,"株",{"v":-285,"d":"-285.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02900"]
[1800,"工項類","喬木植栽，烏心石","搖籃到大門",2025,"株",{"v":-178,"d":"-178.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02900"]
[1801,"工項類","喬木植栽，相思樹","搖籃到大門",2025,"株",{"v":-381,"d":"-381.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02900"]
[1802,"工項類","喬木植栽，楓香","搖籃到大門",2025,"株",{"v":-222,"d":"-222.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02900"]
[1803,"工項類","喬木植栽，櫸木","搖籃到大門",2025,"株",{"v":-171,"d":"-171.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02900"]
[1804,"工項類","水泥混凝土構造物，場鑄混凝土，20%礦物摻料，【不分類】","搖籃到大門",2025,"M3",{"v":361.089,"d":"361.09"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1805,"工項類","水泥混凝土構造物，場鑄混凝土，50%礦物摻料，【不分類】","搖籃到大門",2025,"M3",{"v":238.986,"d":"238.99"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1806,"工項類","水泥混凝土構造物，場鑄混凝土140kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":267.285,"d":"267.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1807,"工項類","水泥混凝土構造物，場鑄混凝土140kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",195.05,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1808,"工項類","水泥混凝土構造物，場鑄混凝土175kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":292.505,"d":"292.51"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1809,"工項類","水泥混凝土構造物，場鑄混凝土175kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",204.43,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1810,"工項類","水泥混凝土構造物，場鑄混凝土210kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":321.285,"d":"321.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1811,"工項類","水泥混凝土構造物，場鑄混凝土210kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",209.02,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1812,"工項類","水泥混凝土構造物，場鑄混凝土245kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":352.285,"d":"352.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1813,"工項類","水泥混凝土構造物，場鑄混凝土245kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",{"v":231.1,"d":"231.10"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1814,"工項類","水泥混凝土構造物，場鑄混凝土280kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":366.285,"d":"366.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1815,"工項類","水泥混凝土構造物，場鑄混凝土280kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",{"v":252.995,"d":"253.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1816,"工項類","水泥混凝土構造物，場鑄混凝土350kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":433.695,"d":"433.70"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1817,"工項類","水泥混凝土構造物，場鑄混凝土350kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",{"v":275.865,"d":"275.87"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1818,"工項類","水泥混凝土構造物，場鑄混凝土420kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":494.285,"d":"494.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1819,"工項類","水泥混凝土構造物，場鑄混凝土420kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",{"v":304.439,"d":"304.44"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1820,"工項類","結構用混凝土，10%礦物摻料，【不分類】","搖籃到大門",2025,"M3",{"v":387.629,"d":"387.63"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1821,"工項類","結構用混凝土，20%礦物摻料，【不分類】","搖籃到大門",2025,"M3",{"v":361.089,"d":"361.09"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1822,"工項類","結構用混凝土，30%礦物摻料，【不分類】","搖籃到大門",2025,"M3",{"v":300.681,"d":"300.68"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1823,"工項類","結構用混凝土，40%礦物摻料，【不分類】","搖籃到大門",2025,"M3",276.19,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1824,"工項類","結構用混凝土，50%礦物摻料，【不分類】","搖籃到大門",2025,"M3",{"v":238.986,"d":"238.99"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1825,"工項類","結構用混凝土，預拌，140kgf/cm2，10%礦物摻料","搖籃到大門",2025,"M3",{"v":282.838,"d":"282.84"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1826,"工項類","結構用混凝土，預拌，140kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":267.285,"d":"267.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1827,"工項類","結構用混凝土，預拌，140kgf/cm2，30%礦物摻料","搖籃到大門",2025,"M3",{"v":228.285,"d":"228.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1828,"工項類","結構用混凝土，預拌，140kgf/cm2，40%礦物摻料","搖籃到大門",2025,"M3",{"v":216.997,"d":"217.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1829,"工項類","結構用混凝土，預拌，140kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",195.05,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1830,"工項類","結構用混凝土，預拌，175kgf/cm2，10%礦物摻料","搖籃到大門",2025,"M3",{"v":316.285,"d":"316.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1831,"工項類","結構用混凝土，預拌，175kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":292.505,"d":"292.51"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1832,"工項類","結構用混凝土，預拌，175kgf/cm2，30%礦物摻料","搖籃到大門",2025,"M3",{"v":249.873,"d":"249.87"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1833,"工項類","結構用混凝土，預拌，175kgf/cm2，40%礦物摻料","搖籃到大門",2025,"M3",{"v":232.418,"d":"232.42"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1834,"工項類","結構用混凝土，預拌，175kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",204.43,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1835,"工項類","結構用混凝土，預拌，210kgf/cm2，10%礦物摻料","搖籃到大門",2025,"M3",{"v":349.232,"d":"349.23"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1836,"工項類","結構用混凝土，預拌，210kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",321.285,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1837,"工項類","結構用混凝土，預拌，210kgf/cm2，30%礦物摻料","搖籃到大門",2025,"M3",{"v":267.285,"d":"267.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1838,"工項類","結構用混凝土，預拌，210kgf/cm2，40%礦物摻料","搖籃到大門",2025,"M3",{"v":244.073,"d":"244.07"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1839,"工項類","結構用混凝土，預拌，210kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",209.02,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1840,"工項類","結構用混凝土，預拌，245kgf/cm2，10%礦物摻料","搖籃到大門",2025,"M3",{"v":382.048,"d":"382.05"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1841,"工項類","結構用混凝土，預拌，245kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":352.285,"d":"352.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1842,"工項類","結構用混凝土，預拌，245kgf/cm2，30%礦物摻料","搖籃到大門",2025,"M3",{"v":293.285,"d":"293.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1843,"工項類","結構用混凝土，預拌，245kgf/cm2，40%礦物摻料","搖籃到大門",2025,"M3",{"v":268.837,"d":"268.84"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1844,"工項類","結構用混凝土，預拌，245kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",{"v":231.1,"d":"231.10"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1845,"工項類","結構用混凝土，預拌，280kgf/cm2，10%礦物摻料","搖籃到大門",2025,"M3",{"v":397.627,"d":"397.63"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1846,"工項類","結構用混凝土，預拌，280kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":366.285,"d":"366.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1847,"工項類","結構用混凝土，預拌，280kgf/cm2，30%礦物摻料","搖籃到大門",2025,"M3",{"v":317.285,"d":"317.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1848,"工項類","結構用混凝土，預拌，280kgf/cm2，40%礦物摻料","搖籃到大門",2025,"M3",{"v":289.153,"d":"289.15"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1849,"工項類","結構用混凝土，預拌，280kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",{"v":252.995,"d":"253.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1850,"工項類","結構用混凝土，預拌，350kgf/cm2，10%礦物摻料","搖籃到大門",2025,"M3",{"v":463.285,"d":"463.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1851,"工項類","結構用混凝土，預拌，350kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":433.695,"d":"433.70"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1852,"工項類","結構用混凝土，預拌，350kgf/cm2，30%礦物摻料","搖籃到大門",2025,"M3",354.47,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1853,"工項類","結構用混凝土，預拌，350kgf/cm2，40%礦物摻料","搖籃到大門",2025,"M3",322.84,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1854,"工項類","結構用混凝土，預拌，350kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",{"v":275.865,"d":"275.87"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1855,"工項類","結構用混凝土，預拌，420kgf/cm2，10%礦物摻料","搖籃到大門",2025,"M3",{"v":522.085,"d":"522.09"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1856,"工項類","結構用混凝土，預拌，420kgf/cm2，20%礦物摻料","搖籃到大門",2025,"M3",{"v":494.285,"d":"494.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1857,"工項類","結構用混凝土，預拌，420kgf/cm2，30%礦物摻料","搖籃到大門",2025,"M3",{"v":394.285,"d":"394.29"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1858,"工項類","結構用混凝土，預拌，420kgf/cm2，40%礦物摻料","搖籃到大門",2025,"M3",{"v":359.009,"d":"359.01"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1859,"工項類","結構用混凝土，預拌，420kgf/cm2，50%礦物摻料","搖籃到大門",2025,"M3",{"v":304.439,"d":"304.44"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03310"]
[1860,"工項類","水泥混凝土舖面","搖籃到大門",2025,"M3",437,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1861,"工項類","混凝土錨塊，【不分類】","搖籃到大門",2025,"塊",{"v":926.654,"d":"926.65"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02384"]
[1862,"工項類","混凝土錨塊，重 2t，含製作及吊放","搖籃到大門",2025,"塊",{"v":202.712,"d":"202.71"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02384"]
[1863,"工項類","混凝土錨塊，重 5t，含製作及吊放","搖籃到大門",2025,"塊",{"v":463.452,"d":"463.45"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02384"]
[1864,"工項類","混凝土錨塊，重 10t，含製作及吊放","搖籃到大門",2025,"塊",{"v":883.717,"d":"883.72"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02384"]
[1865,"工項類","混凝土錨塊，重 15t，含製作及吊放","搖籃到大門",2025,"塊",{"v":1348.259,"d":"1348.26"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02384"]
[1866,"工項類","混凝土錨塊，重 20t，製作","搖籃到大門",2025,"塊",{"v":1735.132,"d":"1735.13"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02384"]
[1867,"工項類","混凝土錨塊，重 20t，吊放","搖籃到大門",2025,"塊",{"v":29.378,"d":"29.38"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02384"]
[1868,"工項類","預鑄混凝土，異形塊，【不分類】","搖籃到大門",2025,"塊",{"v":926.654,"d":"926.65"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1869,"工項類","預鑄混凝土，異形塊，5T","搖籃到大門",2025,"塊",{"v":463.452,"d":"463.45"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1870,"工項類","預鑄混凝土，異形塊，10T","搖籃到大門",2025,"塊",{"v":883.717,"d":"883.72"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1871,"工項類","預鑄混凝土，異形塊，15T","搖籃到大門",2025,"塊",{"v":1348.259,"d":"1348.26"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1872,"工項類","預鑄混凝土，異形塊，20T","搖籃到大門",2025,"塊",{"v":1735.132,"d":"1735.13"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1873,"工項類","港灣用預鑄混凝土塊，【不分類】","搖籃到大門",2025,"塊",{"v":926.654,"d":"926.65"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1874,"工項類","港灣用預鑄混凝土塊，重 2t","搖籃到大門",2025,"塊",{"v":202.712,"d":"202.71"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1875,"工項類","港灣用預鑄混凝土塊，重 5t","搖籃到大門",2025,"塊",{"v":463.452,"d":"463.45"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1876,"工項類","港灣用預鑄混凝土塊，重 10t","搖籃到大門",2025,"塊",{"v":883.717,"d":"883.72"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1877,"工項類","港灣用預鑄混凝土塊，重 15t","搖籃到大門",2025,"塊",{"v":1348.259,"d":"1348.26"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1878,"工項類","港灣用預鑄混凝土塊，重 20t","搖籃到大門",2025,"塊",{"v":1735.132,"d":"1735.13"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1879,"工項類","水泥砂漿，【不分類】","搖籃到大門",2025,"M3",{"v":671.333,"d":"671.33"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","04061"]
[1880,"工項類","水泥砂漿，【不分類】","搖籃到大門",2025,"式",{"v":671.333,"d":"671.33"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","04061"]
[1881,"工項類","水泥砂漿，1:1","搖籃到大門",2025,"M2",21.4,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","04061"]
[1882,"工項類","水泥砂漿，1:1","搖籃到大門",2025,"M3",952,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","04061"]
[1883,"工項類","水泥砂漿，1:2","搖籃到大門",2025,"M2",14.1,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","04061"]
[1884,"工項類","水泥砂漿，1:2","搖籃到大門",2025,"M3",625,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","04061"]
[1885,"工項類","水泥砂漿，1:3","搖籃到大門",2025,"M3",437,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","04061"]
[1886,"工項類","水泥砂漿，1:4","搖籃到大門",2025,"M3",390.95,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","04061"]
[1887,"工項類","水泥砂漿粉刷，1：3 水泥砂漿","搖籃到大門",2025,"M2",9.83,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09220"]
[1888,"工項類","水泥砂漿粉刷，1：3 水泥砂漿，牆面，打底","搖籃到大門",2025,"M2",8.74,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09220"]
[1889,"工項類","水泥砂漿粉刷，1：3 水泥砂漿，牆面，打底","搖籃到大門",2025,"M3",393.028,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09220"]
[1890,"工項類","洗石子","搖籃到大門",2025,"M2",{"v":8.089,"d":"8.09"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09780"]
[1891,"工項類","抿石子","搖籃到大門",2025,"M2",{"v":8.089,"d":"8.09"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1892,"工項類","抿石子，水泥砂漿打底","搖籃到大門",2025,"M2",30.692,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1893,"工項類","人行道面層，濕式壓花地坪","搖籃到大門",2025,"M2",{"v":60.582,"d":"60.58"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02778"]
[1894,"工項類","人行道面層，乾式噴花地坪","搖籃到大門",2025,"M2",{"v":6.896,"d":"6.90"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02778"]
[1895,"工項類","人行道面層，乾式壓花地坪","搖籃到大門",2025,"M2",6.87,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02778"]
[1896,"工項類","混凝土表面修飾，表面層打除","搖籃到大門",2025,"M2",24.534,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03350"]
[1897,"工項類","混凝土表面修飾，表面打毛","搖籃到大門",2025,"M2",4.907,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03350"]
[1898,"工項類","混凝土表面處理，水泥粉光處理","搖籃到大門",2025,"M2",4.907,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03360"]
[1899,"工項類","石材，塊石","搖籃到大門",2025,"M3",7.851,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1900,"工項類","皂土複合防水，皂土防水膜","搖籃到大門",2025,"M2",0.785,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1901,"工項類","填縫劑及填縫料，填縫劑","搖籃到大門",2025,"KG",3.17,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","07921"]
[1902,"工項類","銲接鋼線網，【不分類】","搖籃到大門",2025,"T",834,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1903,"工項類","銲接鋼線網，【不分類】","搖籃到大門",2025,"KG",0.834,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1904,"工項類","銲接鋼線網，D=5.00mm，10x10cm","搖籃到大門",2025,"M2",2.569,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1905,"工項類","銲接鋼線網，D=5.00mm，15x15cm","搖籃到大門",2025,"M2",1.71,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1906,"工項類","銲接鋼線網，D=5.00mm，20x20cm","搖籃到大門",2025,"M2",1.284,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1907,"工項類","銲接鋼線網，D=5.00mm，30x30cm","搖籃到大門",2025,"M2",1.009,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1908,"工項類","銲接鋼線網，D=6.00mm，10x10cm","搖籃到大門",2025,"M2",3.703,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1909,"工項類","銲接鋼線網，D=6.00mm，10x10cm","搖籃到大門",2025,"KG",1.943,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1910,"工項類","銲接鋼線網，D=6.00mm，15x15cm","搖籃到大門",2025,"M2",2.469,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1911,"工項類","銲接鋼線網，D=6.00mm，15x15cm","搖籃到大門",2025,"KG",0.834,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1912,"工項類","銲接鋼線網，D=6.00mm，20x20cm","搖籃到大門",2025,"M2",1.851,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1913,"工項類","銲接鋼線網，D=6.00mm，20x20cm","搖籃到大門",2025,"KG",0.834,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1914,"工項類","銲接鋼線網，D=6.00mm，10x15cm","搖籃到大門",2025,"M2",3.086,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1915,"工項類","銲接鋼線網，D=6.00mm，30x30cm","搖籃到大門",2025,"M2",1.234,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1916,"工項類","銲接鋼線網，D=8.00mm，10x10cm","搖籃到大門",2025,"M2",6.58,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1917,"工項類","銲接鋼線網，D=8.00mm，15x15cm","搖籃到大門",2025,"M2",4.387,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1918,"工項類","銲接鋼線網，D=8.00mm，20x20cm","搖籃到大門",2025,"M2",3.286,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1919,"工項類","銲接鋼線網，D=8.00mm，30x30cm","搖籃到大門",2025,"M2",2.193,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1920,"工項類","銲接鋼線網，D=9.00mm，10x10cm","搖籃到大門",2025,"M2",8.323,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1921,"工項類","銲接鋼線網，D=9.00mm，15x15cm","搖籃到大門",2025,"M2",5.554,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1922,"工項類","銲接鋼線網，D=10.00mm，【不分類】","搖籃到大門",2025,"M2",{"v":7.437,"d":"7.44"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1923,"工項類","銲接鋼線網，D=10.00mm，10x10cm","搖籃到大門",2025,"M2",10.283,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1924,"工項類","銲接鋼線網，D=10.00mm，15x15cm","搖籃到大門",2025,"M2",6.855,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1925,"工項類","銲接鋼線網，D=10.00mm，20x20cm","搖籃到大門",2025,"M2",5.137,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","03220"]
[1926,"工項類","金屬材料，【不分類】","搖籃到大門",2025,"KG",2.42,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1927,"工項類","金屬材料，鐵線","搖籃到大門",2025,"M2",2.469,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1928,"工項類","金屬材料，鐵線","搖籃到大門",2025,"KG",2.263,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1929,"工項類","金屬材料，鐵線，鍍鋅","搖籃到大門",2025,"KG",2.99,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1930,"工項類","金屬材料，鋼料","搖籃到大門",2025,"KG",2.27,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1931,"工項類","金屬製品，不銹鋼踏步，【不分類】","搖籃到大門",2025,"KG",1.75,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1932,"工項類","金屬製品，不銹鋼踏步，直徑=19mm，【實心】","搖籃到大門",2025,"M",{"v":3.895,"d":"3.90"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1933,"工項類","金屬製品，不銹鋼踏步，直徑=19mm，【實心】","搖籃到大門",2025,"組",3.35,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1934,"工項類","金屬製品，鋼索，直徑 20mm","搖籃到大門",2025,"M",2.409,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1935,"工項類","扶手及欄杆，一般安全欄杆","搖籃到大門",2025,"M",23.329,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05520"]
[1936,"工項類","扶手及欄杆，欄杆","搖籃到大門",2025,"M",106.48,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05520"]
[1937,"工項類","不銹鋼欄杆，管徑 2.0\"，#304 不銹鋼，t=3.5mm","搖籃到大門",2025,"M",{"v":36.508,"d":"36.51"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05523"]
[1938,"工項類","金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，【不分類】","搖籃到大門",2025,"組",{"v":255.795,"d":"255.80"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05530"]
[1939,"工項類","金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=60cm，【52.6kg】","搖籃到大門",2025,"組",{"v":157.274,"d":"157.27"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05530"]
[1940,"工項類","金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=70cm，【70.1kg】","搖籃到大門",2025,"組",{"v":209.599,"d":"209.60"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05530"]
[1941,"工項類","金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=80cm，【99.5kg】","搖籃到大門",2025,"組",{"v":297.505,"d":"297.51"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05530"]
[1942,"工項類","金屬格柵蓋板，熱浸鍍鋅格柵蓋板及框座，W=90cm，【120kg】","搖籃到大門",2025,"組",{"v":358.8,"d":"358.80"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05530"]
[1943,"工項類","鋼軌，50kg","搖籃到大門",2025,"M",{"v":121,"d":"121.00"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05651"]
[1944,"工項類","不銹鋼板，厚度 5.0mm，不銹鋼水尺","搖籃到大門",2025,"組",{"v":113.982,"d":"113.98"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05733"]
[1945,"工項類","結構鋼，槽鋼","搖籃到大門",2025,"KG",2.99,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1946,"工項類","結構鋼，槽鋼，H100xB50mm","搖籃到大門",2025,"M",27.518,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1947,"工項類","結構鋼，H 型鋼，(H150xB150mm，t1=7mm，t2=10mm)","搖籃到大門",2025,"KG",1.46,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1948,"工項類","結構用鋼材","搖籃到大門",2025,"KG",2.94,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1949,"工項類","結構用鋼材，C 型鋼，【不分類】","搖籃到大門",2025,"KG",2.99,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1950,"工項類","結構用鋼材，C 型鋼，(75*45*15mm，t=2.3mm)，【3.25kg/m】","搖籃到大門",2025,"M",9.718,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1951,"工項類","結構用鋼材，C 型鋼，(100*50*20mm，t=2.3mm)，【4.06kg/m】","搖籃到大門",2025,"M",12.139,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1952,"工項類","結構用鋼材，C 型鋼，(100*50*20mm，t=2.5mm)，【4.39kg/m】","搖籃到大門",2025,"M",13.126,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1953,"工項類","結構用鋼材，C 型鋼，(100*50*20mm，t=3mm)，【5.19kg/m】","搖籃到大門",2025,"M",15.518,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1954,"工項類","結構用鋼材，C 型鋼，(100*50*20mm，t=3.2m)，【5.5kg/m】","搖籃到大門",2025,"M",16.445,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1955,"工項類","結構用鋼材，C 型鋼，(125*50*20mm，t=2.3mm)，【4.51kg/m】","搖籃到大門",2025,"M",13.485,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1956,"工項類","結構用鋼材，C 型鋼，(125*50*20mm，t=2.5mm)，【4.88kg/m】","搖籃到大門",2025,"M",14.591,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1957,"工項類","結構用鋼材，C 型鋼，(125*50*20mm，t=3mm)，【5.89kg/m】","搖籃到大門",2025,"M",17.611,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1958,"工項類","結構用鋼材，C 型鋼，(125*50*20mm，t=3.2m)，【6.13kg/m】","搖籃到大門",2025,"M",18.329,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1959,"工項類","結構用鋼材，C 型鋼，(150*65*20mm，t=2.3mm)，【5.5kg/m】","搖籃到大門",2025,"M",16.445,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1960,"工項類","結構用鋼材，C 型鋼，(150*65*20mm，t=2.5mm)，【5.96kg/m】","搖籃到大門",2025,"M",17.82,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1961,"工項類","結構用鋼材，C 型鋼，(150*65*20mm，t=3mm)，【7.31kg/m】","搖籃到大門",2025,"M",21.857,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1962,"工項類","結構用鋼材，C 型鋼，(150*65*20mm，t=3.2mm)，【7.76kg/m】","搖籃到大門",2025,"M",23.202,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1963,"工項類","結構用鋼材，C 型鋼，(200*75*20mm，t=3.2mm)，【9.52kg/m】","搖籃到大門",2025,"M",28.465,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1964,"工項類","結構用鋼材，C 型鋼，運輸(不含材料)","搖籃到大門",2025,"T",0.873,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1965,"工項類","結構用鋼材，熱軋型鋼，H 型鋼，【不分類】","搖籃到大門",2025,"KG",1.46,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1966,"工項類","結構用鋼材，熱軋型鋼，H 型鋼，(H100xB50mm，t1=5mm，t2=7mm)，【9.3kg/m】","搖籃到大門",2025,"M",13.578,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1967,"工項類","結構用鋼材，熱軋型鋼，H 型鋼，(H100xB100mm，t1=6mm，t2=8mm)，【16.9kg/m】","搖籃到大門",2025,"M",24.674,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1968,"工項類","結構用鋼材，熱軋型鋼，H 型鋼，(H150xB150mm，t1=7mm，t2=10mm)，【31.1kg/m】","搖籃到大門",2025,"M",45.406,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1969,"工項類","結構用鋼材，熱軋型鋼，H 型鋼，(H200xB100mm，t1=5.5mm，t2=8mm)，【20.9kg/m】","搖籃到大門",2025,"M",30.514,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1970,"工項類","結構用鋼材，熱軋型鋼，H 型鋼，(H200xB200mm，t1=8mm，t2=12mm)，【49.9kg/m】","搖籃到大門",2025,"M",72.854,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1971,"工項類","結構用鋼材，熱軋型鋼，H 型鋼，(H250xB250mm，t1=9mm，t2=14mm)，【71.8kg/m】","搖籃到大門",2025,"M",104.828,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1972,"工項類","結構用鋼材，熱軋型鋼，H 型鋼，(H300xB300mm，t1=10mm，t2=15mm)，【93kg/m】","搖籃到大門",2025,"M",135.78,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1973,"工項類","結構用鋼材，熱軋型鋼，H 型鋼，(H350xB350mm，t1=12mm，t2=19mm)，【197.1kg/m】","搖籃到大門",2025,"M",197.1,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1974,"工項類","結構用鋼材，熱軋型鋼，H 型鋼，(H400xB200mm，t1=8mm，t2=13mm)，【65.4kg/m】","搖籃到大門",2025,"M",95.484,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1975,"工項類","結構用鋼材，熱軋型鋼，H 型鋼，(H400xB400mm，t1=13mm，t2=21mm)，【172kg/m】","搖籃到大門",2025,"M",251.12,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1976,"工項類","結構用鋼材，熱軋型鋼，C 型鋼","搖籃到大門",2025,"KG",2.99,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1977,"工項類","結構用鋼材，熱軋型鋼，H 型鋼，運輸(不含材料)","搖籃到大門",2025,"T",0.873,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","05125"]
[1978,"工項類","H 型鋼樁","搖籃到大門",2025,"KG",2.79,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02462"]
[1979,"工項類","H 型鋼樁，打樁，【單位 M 為打拔深度】","搖籃到大門",2025,"M",{"v":0.483,"d":"0.48"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02462"]
[1980,"工項類","鋼板樁，【不分類】","搖籃到大門",2025,"KG",2.42,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02463"]
[1981,"工項類","高壓混凝土地磚，透水混凝土，厚 60mm","搖籃到大門",2025,"M2",26.5,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02786"]
[1982,"工項類","高壓混凝土地磚，透水混凝土，長 200*寬 100mm，厚60mm","搖籃到大門",2025,"塊",0.53,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02786"]
[1983,"工項類","高壓混凝土地磚，透水混凝土，長 200*寬 200mm，厚60mm","搖籃到大門",2025,"塊",1.06,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02786"]
[1984,"工項類","高壓混凝土地磚，透水混凝土，長 300*寬 300mm，厚60mm","搖籃到大門",2025,"塊",2.38,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02786"]
[1985,"工項類","透水性混凝土地磚，厚60mm","搖籃到大門",2025,"M2",29.5,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02794"]
[1986,"工項類","透水性混凝土地磚，長 200*寬 100mm，厚60mm","搖籃到大門",2025,"塊",0.59,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02794"]
[1987,"工項類","透水性混凝土地磚，長 200*寬 200mm，厚60mm","搖籃到大門",2025,"塊",1.18,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02794"]
[1988,"工項類","透水性混凝土地磚，長 300*寬 300mm，厚60mm","搖籃到大門",2025,"塊",2.65,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02794"]
[1989,"工項類","混凝土植草磚，長 300×寬 200mm，厚100mm","搖籃到大門",2025,"M2",62.563,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1990,"工項類","混凝土植草磚，長 300×寬 200mm，厚100mm","搖籃到大門",2025,"塊",3.753,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1991,"工項類","混凝土植草磚，長 600×寬 400mm，厚100mm","搖籃到大門",2025,"M2",57.562,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1992,"工項類","混凝土植草磚，長 600×寬 400mm，厚100mm","搖籃到大門",2025,"塊",13.825,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1993,"工項類","舖地磚，【不分類】","搖籃到大門",2025,"KG",4.5,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09341"]
[1994,"工項類","石材磚舖貼，2cm","搖籃到大門",2025,"M2",19.448,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09342"]
[1995,"工項類","磨石子地磚，300X300mm，厚度 20mm","搖籃到大門",2025,"片",1.7,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1996,"工項類","磨石子地磚，400X400mm，厚度 20mm","搖籃到大門",2025,"片",3.4,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1997,"工項類","磨石子地磚，厚度 20mm","搖籃到大門",2025,"M2",19.752,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1998,"工項類","磨石子地磚，【不分類】","搖籃到大門",2025,"KG",0.395,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[1999,"工項類","磨石子地磚，450x450mm，厚度 20mm","搖籃到大門",2025,"片",4,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2000,"工項類","磨石子地磚，500x500mm，厚度 25mm","搖籃到大門",2025,"片",5,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2001,"工項類","磨石子地磚，600x600mm，厚度 25mm","搖籃到大門",2025,"片",7.5,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2002,"工項類","磨石子地磚，600x300mm，厚度 20mm","搖籃到大門",2025,"片",3.2,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2003,"工項類","再生纖維水泥板，【不分類】","搖籃到大門",2025,"KG",1.12,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2004,"工項類","再生纖維水泥板，纖維水泥板","搖籃到大門",2025,"KG",1.12,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2005,"工項類","再生纖維水泥板，矽酸鈣板","搖籃到大門",2025,"KG",1.12,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2006,"工項類","石膏板，石膏板","搖籃到大門",2025,"KG",0.51,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09250"]
[2007,"工項類","油漆","搖籃到大門",2025,"M2",0.103,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09910"]
[2008,"工項類","油漆，一底一度","搖籃到大門",2025,"M2",0.208,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09910"]
[2009,"工項類","油漆，一底二度","搖籃到大門",2025,"M2",0.559,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09910"]
[2010,"工項類","油漆，反光漆，黃黑斜紋","搖籃到大門",2025,"M2",0.798,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09910"]
[2011,"工項類","油漆，水性水泥漆","搖籃到大門",2025,"M2",0.144,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09910"]
[2012,"工項類","油漆，水性水泥漆","搖籃到大門",2025,"KG",1.33,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09910"]
[2013,"工項類","油漆，水性水泥漆，一底一度","搖籃到大門",2025,"M2",0.286,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09910"]
[2014,"工項類","油漆，水性水泥漆，一底二度","搖籃到大門",2025,"M2",0.429,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09910"]
[2015,"工項類","油漆，油性環氧樹脂漆(油性水泥漆)","搖籃到大門",2025,"M2",0.097,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09910"]
[2016,"工項類","油漆，油性環氧樹脂漆(油性水泥漆)，一底二度","搖籃到大門",2025,"M2",0.386,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09910"]
[2017,"工項類","水泥漆","搖籃到大門",2025,"KG",1.33,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09912"]
[2018,"工項類","水泥漆，一底二度","搖籃到大門",2025,"M2",0.429,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09912"]
[2019,"工項類","水泥漆(黃色)，一底二度","搖籃到大門",2025,"M2",0.429,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09912"]
[2020,"工項類","水泥漆，連工帶料","搖籃到大門",2025,"KG",1.33,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09912"]
[2021,"工項類","水泥漆，連工帶料，一底一度","搖籃到大門",2025,"M2",0.206,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09912"]
[2022,"工項類","水泥漆，室外用，連工帶料，一底二度","搖籃到大門",2025,"M2",0.342,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09912"]
[2023,"工項類","水泥漆，水性水泥漆","搖籃到大門",2025,"M2",0.144,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09912"]
[2024,"工項類","水泥漆，水性水泥漆","搖籃到大門",2025,"KG",1.33,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09912"]
[2025,"工項類","水泥漆，水性水泥漆，一底一度","搖籃到大門",2025,"M2",0.286,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09912"]
[2026,"工項類","水泥漆，水性水泥漆，一底二度","搖籃到大門",2025,"M2",0.429,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","09912"]
[2027,"工項類","計量與計價，搬運費","搖籃到大門",2025,"T",62.17,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","01271"]
[2028,"工項類","計量與計價，二次搬運費(小搬運)，【僅含運輸碳排】","搖籃到大門",2025,"T",4.363,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","01271"]
[2029,"工項類","計量與計價，二次搬運費(小搬運)，混凝土，【僅含運輸碳排】","搖籃到大門",2025,"M3",10.472,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","01271"]
[2030,"工項類","計量與計價，二次搬運費(小搬運)，混凝土，【僅含運輸碳排】","搖籃到大門",2025,"T",4.363,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","01271"]
[2031,"工項類","計量與計價，二次搬運費(小搬運)，鋼筋，【僅含運輸碳排】","搖籃到大門",2025,"T",4.363,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","01271"]
[2032,"工項類","計量與計價，二次搬運費(小搬運)，鋼筋，【僅含運輸碳排】","搖籃到大門",2025,"KG",0.004,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","01271"]
[2033,"工項類","計量與計價，二次搬運費(小搬運)，模板，【僅含運輸碳排】","搖籃到大門",2025,"M2",0.065,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","01271"]
[2034,"工項類","計量與計價，二次搬運費(小搬運)，模板，【僅含運輸碳排】","搖籃到大門",2025,"T",4.363,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","01271"]
[2035,"工項類","計量與計價，二次搬運費(小搬運)，材料，【僅含運輸碳排】","搖籃到大門",2025,"T",4.362,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","01271"]
[2036,"工項類","計量與計價，二次搬運費(小搬運)，材料，【僅含運輸碳排】","搖籃到大門",2025,"KG",0.004,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","01271"]
[2037,"工項類","計量與計價，二次搬運費(小搬運)，石塊，【僅含運輸碳排】","搖籃到大門",2025,"M3",12.215,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","01271"]
[2038,"工項類","計量與計價，二次搬運費(小搬運)，石塊，【僅含運輸碳排】","搖籃到大門",2025,"T",4.362,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","01271"]
[2039,"工項類","臨時設施，施工便道","搖籃到大門",2025,"M",3.925,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2040,"工項類","地工織物，工程用非織物(不織布)，搭接施工","搖籃到大門",2025,"M2",2.479,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02342"]
[2041,"工項類","地工織物，織布、合成纖維","搖籃到大門",2025,"M2",{"v":2.479,"d":"2.48"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02342"]
[2042,"工項類","地工織物，不織布","搖籃到大門",2025,"KG",5.5,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02342"]
[2043,"工項類","地工織物，不織布，舖設施工","搖籃到大門",2025,"M2",2.479,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署","02342"]
[2044,"工項類","配線器材，絕緣橡膠布帶","搖籃到大門",2025,"KG",2.21,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2045,"工項類","LED 照明設備，太陽能路燈，18W，5310K-7040K，【12V，1,362lm】","搖籃到大門",2025,"盞",447,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2046,"工項類","柵欄，鐵絲網柵欄，可拆式","搖籃到大門",2025,"M",0.521,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2047,"工項類","加勁擋土牆-地工合成加勁材，加勁格網","搖籃到大門",2025,"M2",0.927,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2048,"工項類","加勁擋土牆-地工合成加勁材，地工織物，聚丙烯(PE)，含鋪設工資","搖籃到大門",2025,"M2",{"v":2.479,"d":"2.48"},"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2049,"工項類","木樁，樁尖 D=10cm","搖籃到大門",2025,"M",1.702,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]
[2050,"工項類","木樁，樁尖 D=15cm，打樁","搖籃到大門",2025,"M",19.627,"經BSI第三方查驗證","農村水保工程減碳作業指引","農業部農村水保署"]